**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/01**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /4/ /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Rehabilitation / Improvement of Sewerage System near Jama Masjid, Mubrak Muhammadi,

Sector 14-B, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 8,10,204.00*/= + O/R

*BID SECURITY.* Rs. *16,205*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/01**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,10,204.00*/= + O/R

Earnest Money Rs. *16,205*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation / Improvement of Sewerage System near Jama Masjid, Mubrak Muhammadi,

Sector 14-B, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:3:6 plain (Ch-2/10/19c) | 2017 % Cft | 3327.50 % Cft | 67,106/= |
| 02 | Excavation for pipe line in trenches & pits in al kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 4450 % Cft | 4650.00 % CFT | 20,693/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 875 % Cft | 10770.00 % CFT | 9,424/- |
| 04 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 100 Rft  500 Rft | 206.00 Rft  436.00 Rft | 36,700 /-  2,18,000/- |
| 05 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 32 Nos. | 13064.00 Each | 4,18,048/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | 107 Rft  (-) | 1540.00 Rft | -1,64,828/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3355 Cft | 2760.00 % Cft | 9,260/- |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 5517 Cft | 1065.00 % CFT | 58,756/= |
| 10 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾ and down guagge i/c etc complete. 21” dia  24” dia | 150 Nos | 913.63 Each | 1,37,045/= |
| **SUB TOTAL PART-A** | | | | **8,10,204/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation / Improvement of Sewerage System near Jama Masjid, Mubrak Muhammadi,

Sector 14-B, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 12 | P/F Per Costed RCC Ring Slab 39” dia with Rcc Man Hole cover of 21” dia as per direction of engineer incharge. | 25 Nos. | Offer Rate | Offer Rate |
| 13 | S/F Imported Earth with in the a radius of 5 miles i/c digging loading unloading all lead and lift leveling and water compaction etc complete | 1000 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/2**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: P/L Rcc pipe near Noorani Masjid in U.C # 11

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 8,45,888.00*/= + O/R

*BID SECURITY.* Rs. *16,918*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/2**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,45,888.00*/= + O/R

Earnest Money Rs. *16,918*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: P/L Rcc pipe near Noorani Masjid in U.C # 11

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1608 Cft | 3327.50%  Cft | 53,506/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3900 Cft | 4650.00 %0 CFT | 18,135/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 1750.00 % Cft | 10770.00 % CFT | 18,848/- |
| 04 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) , 12” Dia, | 800 Rft | 367.00 Rft | 2,93,600/- |
| 05 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 35 Nos. | 13064 Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 61.25 Rft | 1540.00 Rft | -94,325/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3054 Cft | 2760.00 % Cft | 8,429/- |
| 08 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 4204 Cft | 1065.00 % Cft | 44,773/- |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & | 50 Nos. | 913.63 Each | 45,682/- |
| **SUB TOTAL PART-A** | | | | **8,45,888/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: P/L Rcc pipe near Noorani Masjid in U.C # 11

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 30 Nos. | Offer Rate | Offer Rate |
| 11 | S/F Imported Earth with in the a radius of 5 miles i/c digging loading unloading all lead and lift leveling and water compaction etc complete | 3000 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/3**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Rehabilitation of Sewerage System in Street # 01 and 04 in Aliabad U.C # 11

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,20,576.00*/= + O/R

*BID SECURITY.* Rs. *16,412*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/3**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,20,576.00*/= + O/R

Earnest Money Rs. *16,412*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System in Street # 01 and 04 in Aliabad U.C # 11

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1706 Cft | 3327.50%  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3938 Cft | 4650.00 %0 CFT | 18,312/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) , 12” Dia, | 750 Rft | 367.00 Rft | 2,75,240/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 35 Nos. | 13064 Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | -80,850/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3081 Cft | 2760.00 % Cft | 8,330/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2627 Cft | 1065.00 % Cft | 27,978/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & | 63 Nos. | 913.63 Each | 57,559/- |
| **SUB TOTAL PART-A** | | | | **8,20,576/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System in Street # 01 and 04 in Aliabad U.C # 11

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 9 | P/F per costed Rcc Ring slab 39” dia with Rcc Man Hole Cover of 21” dia as per direction of Engineer Incharge. | 47 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address*** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/4**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Providing & Laying Rcc pipe in Block “C” M.P.R Colony U.C 11

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,18,748.00*/= + O/R

*BID SECURITY.* Rs. *16,375*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/4**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,18,748.00*/= + O/R

Earnest Money Rs. *16,375*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Providing & Laying Rcc pipe in Block “C” M.P.R Colony U.C 11

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1706 Cft | 3327.50%  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3938 Cft | 4650.00 %0 CFT | 18,312/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) , 12” Dia, | 750 Rft | 367.00 Rft | 2,75,240/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 35 Nos. | 13064 Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | -80,850/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3018 Cft | 2760.00 % Cft | 8,330/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2627 Cft | 1065.00 % Cft | 27,978/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & | 61 Nos. | 913.63 Each | 55,731/- |
| **SUB TOTAL PART-A** | | | | **8,18,748/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Providing & Laying Rcc pipe in Block “C” M.P.R Colony U.C 11

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 9 | P/F pre cast Rcc Ring slab 39” dia with Rcc Man hole cover of 21 “ dia as per direction of engineer incharge. | 40 sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/5**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Providing & Laying Rcc pipe in Baloch Para, Bura Mohallah, Bapra Mohallah in U.C # 11

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,46,868.00*/= + O/R

*BID SECURITY.* Rs. *16,937*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,46,868.00*/= + O/R

Earnest Money Rs. *16,937*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Providing & Laying Rcc pipe in Baloch Para, Bura Mohallah, Bapra Mohallah in U.C # 11

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1706 Cft | 3327.50%  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3938 Cft | 4650.00 %0 CFT | 18,312/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) , 12” Dia, | 750 Rft | 367.00 Rft | 2,75,240/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 36 Nos. | 13064 Each | 4,70,304/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 54 Rft | 1540.00 Rft | -83,160/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3018 Cft | 2760.00 % Cft | 8,330/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2627 Cft | 1065.00 % Cft | 27,978/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & | 80 Nos. | 913.63 Each | 73,090/- |
| **SUB TOTAL PART-A** | | | | **8,46,868/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Providing & Laying Rcc pipe in Baloch Para, Bura Mohallah, Bapra Mohallah in U.C # 11

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 9 | P/F per costed Rcc Ring slab 39” dia with Rcc Man Hole Cover of 21” dia as per direction of Engineer Incharge. | 51 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/06**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /4/ /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Improvement / Construction of road & other work near Nadra Office UC-18 in Orangi Zone,

DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 7,49,509.00*/= + O/R

*BID SECURITY.* Rs. *14,990*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/06**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,10,204.00*/= + O/R

Earnest Money Rs. *14,990*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement / Construction of road & other work near Nadra Office UC-18 in Orangi Zone,

DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7500 Sft | 773.86%  Sft | 58,040/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 25988 Cft | 1437.00%0  Cft | 37,345/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 27863 Cft | 1065.00 % CFT | 2,96,741/= |
| 06 | Premixed Patch repair 1” thick i/c cleaning cutting scattered patches in proper shapes laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials T & P and carriage upto 3 chains). Using Crush Bajiri Laying premixed Carpet. | 7500 sft | 3779.09 % Sft  986.02 % Sft  4,765.11 % Sft | 3,57,383 |
| **SUB TOTAL PART-A** | | | | **7,49,509/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement / Construction of road & other work near Nadra Office UC-18 in Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1350 Cft | Offer Rate | Offer Rate |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3300 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/07**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /4/ /2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: Rehabilitation and Improvement of road near Masha Allah Milk Shop & Near Imran Milk Shop

In Sector 10 & Other Areas in U.C -20 in Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 6,56,022.00*/= + O/R

*BID SECURITY.* Rs. *13,120*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/07**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *6,56,022.00*/= + O/R

Earnest Money Rs. *13,120*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation and Improvement of road near Masha Allah Milk Shop & Near Imran Milk Shop

In Sector 10 & Other Areas in U.C -20 in Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 14601 Cft | 1437.00%0  Cft | 20,982/= |
| 02 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14601 Cft | 1065.00 % CFT | 1,55,501/= |
| 03 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8500 Sft | 526.28%  Sft | 44,734/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8500 Sft | 4107.84 % Sft  986.02 % Sft  5093.86 % Sft | 4,32,978/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia 24” Dia | 02 Nos. | 913.63  Each | 1,827/= |
| **SUB TOTAL PART-A** | | | | **6,56,022/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation and Improvement of road near Masha Allah Milk Shop & Near Imran Milk Shop

In Sector 10 & Other Areas in U.C -20 in Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3188 Cft | Offer Rate | Offer Rate |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3910 Cft | Offer Rate | Offer Rate |
| 08 | P/F R.C.C Ring Slab 39” dia with R.c.c Man Hole Cover of 21” dia as per Direction of Engineer Incharge. | 02 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***