** DISTRICT MUNICIPAL CORPORATION, KARACHI WEST**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI**

**PTCL # 36697869 / 36660102 & FAX # 36762519**

NO. EE/B&R/OZ/DMC/NIT/06/16 Karachi, 13-01-2017

**TENDER NOTICE**

**Through Website of SPPRA & Orangi Zone DMC (West)**

Tender in sealed covers are invited for the following work (s) under SPP Rules 2010 from the firms having adequate experience in the relevant field. The tentative cost of work is under Rs. 1.0 Million.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***S #*** | ***NAME OF WORK*** | ***ESTIMATED COST*** | ***Bids Security***  ***2%*** | ***TENDER COST*** |
| 01 | Repair and Construction of cc street in different area of Sector 15/A, and 15/B at U.C # 270 Orangi Zone DMC (West). | *Rs. 4,74,189.00 + O/R* | ***Rs. 9,484.00***  ***+ O/R*** | 1000.00 |
| 02 | Repair & Improvement of Rcc pipe & Main Hole Gali # 01, Islam Nagar, U.C -22. | *Rs. 9,04,764.00 + O/R* | ***Rs.18,095.00***  ***+ O/R*** | 1000.00 |
| 03 | Rehabilitation of Rcc pipe & Main Hole gali # 21 Fareed Colony U.C -25. | *Rs. 8,24,901.00 + O/R* | ***16,498.00 + O/R*** | 1000.00 |
| 04 | Rehabilitation & Improvement of Sewerage System in Mansoor Nagar and Ghaziabad U.C # 24 Sector 11 ½ Orangi Zone, DMC (West). | *Rs. 7,80,173.00 + O/R* | ***15,603.00 + O/R*** | 1000.00 |
| 05 | Improvement and Maintenance of Sewerage System in Sector 4-E, & LS-53, in Orangi Zone, U.C # 20. | *Rs. 8,30,252.00 + O/R* | ***16,605.00 + O/R*** | 1000.00 |
| 06 | Improvement & Construction of CC street Muhammad Masjid, Gali # 01 & Gali # C/4, Ghaziabad in U.C # 16. | *Rs. 9,04,523.00 + O/R* | ***18,090.00 + O/R*** | 1000.00 |
| 07 | Rehabilitation of Sewerage System by Repairing of RCC pip and man Hole Gali # 03 Zia Colony U.C # 01 Orangi Zone. | *Rs. 8,84,618.00 + O/R* | ***17,692.00 + O/R*** | 1000.00 |

***Terms & Conditions:-***

1. Tender Schedule shall be as follows.

|  |  |  |
| --- | --- | --- |
| SCHEDULE | DATE & TIME | VENUE |
| Receiving of Application & Issuance of Tenders | 16-01-2017 03-02-2017 During Office Hours | DMC (West) Sector 11-E Shahrah-e- Orangi Karachi |
| Dropping of Tenders | 06-02-2017 11.00 A.M | Executive Engineer Orangi Zone DMC (West) Office |
| Opening of Tenders | 06-02-2017 11.30 A.M | Executive Engineer Orangi Zone DMC (West) Office |

1. The tender documents will be issued to contractor on submission of written request on latter head and on payment on non-refundable cost of tender price through pay order from Sindh Bank in favour of Orangi Zone DMC (West0.
2. The Bid Security as mentioned above in shape of pay order in favour of Orangi Zone DMC (West) shall must be enclosed with tender documents without which the tender will be treated as cancelled.
3. In case the date of opening is declared as a public holiday by the Government, the next official working day shall be deemed to be the date for submission and opening of tenders at the same time as mentioned.
4. The total bid amount as well as the rates of items must be filled both in figures and words and in case any correction is made by the contractor himself then each correction must be initialed by the contractor, otherwise the tenders are liable to be summarily rejected.
5. The bidder are required to submit the above information along with their bid.
6. If any fake documents are found then the tender is liable to be rejected / cancelled without any compensation but with penalty as per rules.
7. Canvassing in connection with tenders is strictly prohibited and tenders submitted by the contractors reported to be involved in canvassing will be liable for rejection.
8. Bid Security of the unsuccessful bidder shall be released once the contractors has been signed with the successful bidder or the validity period has expired.
9. The procuring agency may reject all or any bid subject to the relevant provisions of SPPRA Rules 2010.
10. Eligibility
11. Valid PEC in C-06 & above Category & relevant filed of specialization
12. NTN Certificate
13. S.R.B Certificate
14. Bank Statement
15. Relevant Experience
16. Turn Over of at least three years
17. Turn Over of at least three years

**Executive Engineer (B&R)** **Orangi Zone DMC (West)**

**Not to be published**

**Director (CB) SPPRA**

With a request to upload on SPPRA (Authority) website and issue ID Number

**Incharge (I.T), Orangi Zone DMC (West).**

With a request to upload on Orangi Zone DMC (West) Website.

Copy to:-

1. Administrator, DMC (West).
2. Municipal Commissioner, DMC (West).
3. Superintending Engineer, DMC (West).
4. P.S to Managing Director, Sindh Public Procurement.
5. Office File.

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/1**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair and Construction of cc street in different area of Sector 15/A, and 15/B at U.C # 270

Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *4,74,189.00*/= + O/R

*BID SECURITY.* Rs. *9,484*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/1**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *4,74,189.00*/= + O/R

Earnest Money Rs. *9,484*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair and Construction of cc street in different area of Sector 15/A, and 15/B at U.C # 270

Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain (Ch-2/P-10/19-C). | 1482 Cft | 3327.50 %  Cft | 49,322/= |
| 02 | Dismantling of cement concrete flooring. 1:3:6 plain (Ch-2/P-10/19-b) | 2025 Cft | 1306.80 %  Cft | 26,463/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3507 Cft | 1065.00 % CFT | 37,352/= |
| 05 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9). | 8800 Sft | 526.28 % Sft | 46,313/= |
| 08 | Providing and Laying topping Cement Concrete (1.2.4) including surface finishing & dividing into panels. (Ch-8/P-42/16-b-c) 2” Thick C.C | 8800 sft | 3275.50 %  sft | 2,88,244/= |
| 10 | P/L 1.2.4 Rcc Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete (CH-14/P-31/1-A) 21’ dia. | 29 Nos | 913.63 Each | 26,495/= |
| **SUB TOTAL PART-A** | | | | **4,74,189/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: Repair and Construction of cc street in different area of Sector 15/A, and 15/B at U.C # 270

Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2714 Cft | Offer Rate | Offer Rate |
| 06 | Preparing Sub Base by supplying and spreading well graded pit or bed run gravel having aliquot limit not greater than 25 & plasticity index not greater than 6 in proper camber & grade including watering rolling & compacting in layer not exceeding 6” compacted upto 98-100 % density as per modified AASHO density (Rate including all cost of materials T&P and carriage upto 3 chains. (CH-HW/P-4/D). | 2552 Cft | Offer Rate | Offer Rate |
| 07 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section shown in drawing for new payment at graded granular smooth graduation curve with in the limit for grading A or B as per AASHTO-M-142-65 (1985) and compacting to 100 % of the minimum dry density according AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by Engineer Incharge. (Ch-HW/P-5 / 13-B). | 4400 cft | Offer Rate | Offer Rate |
| 09 | Extra for using (S.R Cement) Sulphate resistant cement in place of ordinary Portland cement ( A/Rate). | 254 Cwt | Offer Rate | Offer Rate |
| 11 | P/F R.C.C Ring Slab 39” dia with Rcc man Hole Cover of 21” dia as per direction of Engineer incharge. | 55 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/2**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Improvement of Rcc pipe & Main Hole Gali # 01 Islam Nagar U.C-22.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *9,04,764.00*/= + O/R

*BID SECURITY.* Rs. *18,095*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/2**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *9,04,764.00* /= + O/R

Earnest Money Rs. *18,095*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Improvement of Rcc pipe & Main Hole Gali # 01 Islam Nagar U.C-22.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2017 Cft | 3327.50 %  Cft | 67,116/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 4450 Cft | 4650.00 CFT | 20,693/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 875 Cft | 10770.00 CFT | 9,424/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 200 Rft  500 Rft | 367.00 Rft    436.00 Rft | 73,400/-  2,18,000/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 30 Nos. | 13064.00  Each | 3,91,920/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.50 Rft | 1540.00 Rft | -80,850/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3355 cft | 2760.00 P.cft | 9,260/= |
| 8 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 5517 Cft | 1065.00 % CFT | 58,756/= |
| 9 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 150 Nos. | 913.63  Each | 1,37,045/= |
| **SUB TOTAL PART-A** | | | | **9,04,764/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Improvement of Rcc pipe & Main Hole Gali # 01 Islam Nagar U.C-22.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 25 Nos. | Offer Rate | Offer Rate |
| 11 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 1000 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/3**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Rcc pipe & Main Holes gali # 21 Fareed Colony U.C # 25 Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,24,901`.00*/= + O/R

*BID SECURITY.* Rs. *16,498*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/3**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,24,901.00*/= + O/R

Earnest Money Rs. *16,498*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Rcc pipe & Main Holes gali # 21 Fareed Colony U.C # 25 Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4, | 1910 Cft | 3327.50 %  Cft | 63,555/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5625 Cft | 4650.00 CFT | 26,156/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 33 Nos. | 13064.00  Each | 4,31,112/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 57.75 Rft | 1540.00 Rft | -88,935/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4832 cft | 2760.00 P.cft | 13,336/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 5516 Cft | 1065.00 % CFT | 58,745/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **8,24,901/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: Rehabilitation of Rcc pipe & Main Holes gali # 21 Fareed Colony U.C # 25 Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos. | Offer Rate | Offer Rate |
| 10 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 3300 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/4**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /06/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation & Improvement of sewerage system in Mansoor Nagar and Ghaziabad U.C # 24

Sector 11 ½, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,80,173.00*/= + O/R

*BID SECURITY.* Rs. *15,603*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/4**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,80,173.00*/= + O/R

Earnest Money Rs. *15,603*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation & Improvement of sewerage system in Mansoor Nagar and Ghaziabad U.C # 24

Sector 11 ½, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4, | 1606 Cft | 3327.50 %  Cft | 53,440/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6) | 1500 Cft | 10770.00 CFT | 16,155/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 61.25 Rft | 1540.00 Rft | -94,325/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3707 cft | 2760.00 P.cft | 10,231/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2399 Cft | 1065.00 % CFT | 2,550/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **7,80,173/= + O/R** |

***Signature of*** ***Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation & Improvement of sewerage system in Mansoor Nagar and Ghaziabad

U.C # 24 Sector 11 ½, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2000 Cft | Offer Rate | Offer Rate |
| 11 | P/F pre cast RCC Ring slab 39” dia with Rcc Man Hole Cover of 21” dia as per direction of Engineer Incharge | 30 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/5**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement and Maintenance of sewerage System in Sector 4-E, & H # 79 & LS-53, in

Oarangi Zone, U.C # 20.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 8,30,252.00*/= + O/R

*BID SECURITY.* Rs. *16,605*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,30,252.00*/= + O/R

Earnest Money Rs. *16,605*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement and Maintenance of sewerage System in Sector 4-E, & H # 79 & LS-53, in

Oarangi Zone, U.C # 20.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.3.6, | 1928 Cft | 1306.80 % Cft | 25,195/= |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4, | 1248 Cft | 3327.50 %  Cft | 41,527/= |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6) | 3025 Cft | 4650.00 CFT | 14,066/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6) | 1988 Cft | 10770.00 CFT | 21,411/- |
| 05 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete.(Ch-2/P-18/B-2). 8“dia,12”dia, | 50 Rft  700 Rft | 206.00 Rft  367.00 Rft | 10,300/-  2,56,900/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 48.5 Rft | 1540.00 Rft | -74,690/- |
| 08 | P/L 1.3.6 CC using GSB ¾”and down gauge i/c consolidation, curing etc complete with out shuttering. | 20 cft | 12595.00 % cft | 2,519/- |
| 09 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2239 cft | 2760.00 P.cft | 6,180/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3962 Cft | 1065.00 % CFT | 42,195/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 30 Nos. | 913.63  Each | 27,409/= |
| **SUB TOTAL PART-A** | | | | **8,30,252/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement and Maintenance of sewerage System in Sector 4-E, & H # 79 & LS-53, in

Oarangi Zone, U.C # 20.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 11 | Excavation for pipe line in trenches & pits in hard rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6) | 1988 cft | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 25 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/6**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement & Construction of CC street Muhammadi Masjid, gali # 01 & Gali # C/4,

Ghaziabad in U.C # 16.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *9,04,523`.00*/= + O/R

*BID SECURITY.* Rs. *18,090*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/6**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *9,04,523.00*/= + O/R

Earnest Money Rs. *18,090*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement & Construction of CC street Muhammadi Masjid, gali # 01 & Gali # C/4,

Ghaziabad in U.C # 16.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4, | 3909 Cft | 3327.50 %  Cft | 1,30,072/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1650 Cft | 4650.00 CFT | 7,673/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 300 Rft | 367.00 Rft | 1,10,100/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 13 Nos. | 13064.00  Each | 1,69,832/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 19.50 Rft | 1540.00 Rft | -30,030/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1282 cft | 2760.00 P.cft | 3,538/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 4277 Cft | 1065.00 % CFT | 45,550/= |
| 09 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9). | 6000 cft | 526.28 % Sft | 31,577/= |
| 10 | P/L 1.4.8 CC using GSB 2” to 3” and i/c leveling compacting, curing etc complete without shuttering. | 1500 cft | 11288.75 % cft | 1,69,331/= |
| 11 | P/L C.C Topping (1.2.4) i/c surface finishing & dividing into panelsa (ch-8/42/16-b-c) 2” th CC 1.2.4 | 6000 sft | 3275.50 % sft | 1,96,530/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 77 Nos. | 913.63  Each | 70,350/= |
| **SUB TOTAL PART-A** | | | | **9,45,523/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement & Construction of CC street Muhammadi Masjid, gali # 01 & Gali # C/4,

Ghaziabad in U.C # 16.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 320 Cft | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 6/7**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 06/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System by Repairing of RCC pip and man Hole Gali # 03 Zia Colony

U.C # 01 Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,84,618`.00*/= + O/R

*BID SECURITY.* Rs. *17,692*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 6/7**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,84,618.00*/= + O/R

Earnest Money Rs. *17,692*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System by Repairing of RCC pip and man Hole Gali # 03 Zia Colony

U.C # 01 Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in tranches & pits in hard rock by harming and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 6875 Cft | 24150.00 CFT | 1,66,031/- |
| 02 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 8” Dia. | 1000 Rft | 206.00 Rft | 2,06,000/- |
| 03 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 44 Nos. | 13064.00  Each | 5,74,816/- |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 121 Rft | 1540.00 Rft | -1,86,340/- |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 9080 Cft | 1065.00 % CFT | 96,702/= |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 30 Nos. | 913.63  Each | 27,409/= |
| **SUB TOTAL PART-A** | | | | **8,84,618/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: Rehabilitation of Sewerage System by Repairing of RCC pip and man Hole Gali # 03 Zia Colony

U.C # 01 Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 7 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 5156 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***