**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/1**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Road Pot holes Tranches Patch work by carpeting from Islam Chowk to Bhoolo

Masjid in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,40,699.00*/= + O/R

*BID SECURITY.* Rs. ***14,814***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/1**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,40,699.00*/= + O/R

Earnest Money Rs. ***14,814***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Road Pot holes Tranches Patch work by carpeting from Islam Chowk to Bhoolo

Masjid in Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 5000 Sft | 773.86 %  Sft | 38,693/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 9000 Cft | 1437.00 %  Cft | 12,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11500 Cft | 1065.00 % CFT | 1,22,475/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | Premixed Patch Repair 1” including cleanng cutting scattered patches in proper shape laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials. T & P and carriage upto 3 chins.)  P-09/19 using Crushed Bajri, laying premixed Carpet. | 10000 Sft | 3779.09 % Sft  986.02 % Sft  4765.11 % Sft | 4,76,511/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 41 Nos. | 913.63  Each | 37,459/= |
| **SUB TOTAL PART-A** | | | | **7,40,699/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Rehabilitation of Road Pot holes Tranches Patch work by carpeting from Islam Chowk to Bhoolo

Masjid in Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4200 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/2**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Maintenance of damage road from Four Star lawn to Amma hospital in Shah

Wali-ullaha Nagar, in orangi zone

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,03,240.00*/= + O/R

*BID SECURITY.* Rs. ***14,065***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/2**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,03,240.00*/= + O/R

Earnest Money Rs. ***14,065***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Maintenance of damage road from Four Star lawn to Amma hospital in Shah

Wali-ullaha Nagar, in orangi zone

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 5000 Sft | 773.86 %  Sft | 38,693/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 9000 Cft | 1437.00 %  Cft | 12,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11500 Cft | 1065.00 % CFT | 1,22,475/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | Premixed Patch Repair 1” including cleanng cutting scattered patches in proper shape laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials. T & P and carriage upto 3 chins.)  P-09/19 using Crushed Bajri, laying premixed Carpet. | 10000 Sft | 3779.09 % Sft  986.02 % Sft  4765.11 % Sft | 4,76,511/= |
| **SUB TOTAL PART-A** | | | | **7,03,240/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Repair & Maintenance of damage road from Four Star lawn to Amma hospital in Shah

Wali-ullaha Nagar, in orangi zone

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4200 Cft |  |  |
| 07 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 12 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/3**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Maintenance of pot holes and tranches by carpeting near Qatar Hospital and different

places in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,39,785.00*/= + O/R

*BID SECURITY.* Rs. ***14,796***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/3**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,39,785.00*/= + O/R

Earnest Money Rs. ***14,796***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Maintenance of pot holes and tranches by carpeting near Qatar Hospital and different

places in Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 5000 Sft | 773.86 %  Sft | 38,693/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 9000 Cft | 1437.00 %  Cft | 12,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11500 Cft | 1065.00 % CFT | 1,22,475/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | Premixed Patch Repair 1” including cleanng cutting scattered patches in proper shape laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials. T & P and carriage upto 3 chins.)  P-09/19 using Crushed Bajri, laying premixed Carpet. | 10000 Sft | 3779.09 % Sft  986.02 % Sft  4765.11 % Sft | 4,76,511/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 40 Nos. | 913.63  Each | 36,545/= |
| **SUB TOTAL PART-A** | | | | **7,39,785/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Repair & Maintenance of pot holes and tranches by carpeting near Qatar Hospital and different

Places in Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4200 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/4**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Road and tranches near al-Fatah Lawn and different places in Orangi Zone,

DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,03,240.00*/= + O/R

*BID SECURITY.* Rs. ***14,065***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/4**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,03,240.00*/= + O/R

Earnest Money Rs. ***14,065***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Road and tranches near al-Fatah Lawan and different places in Orangi Zone,

DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 5000 Sft | 773.86 %  Sft | 38,693/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 9000 Cft | 1437.00 %  Cft | 12,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11500 Cft | 1065.00 % CFT | 1,22,475/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | Premixed Patch Repair 1” including cleanng cutting scattered patches in proper shape laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials. T & P and carriage upto 3 chins.)  P-09/19 using Crushed Bajri, laying premixed Carpet. | 10000 Sft | 3779.09 % Sft  986.02 % Sft  4765.11 % Sft | 4,76,511/= |
| **SUB TOTAL PART-A** | | | | **7,03,240/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Rehabilitation of Road and tranches near al-Fatah Lawan and different places in Orangi Zone,

DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4200 Cft | Offer Rate | Offer Rate |
| 07 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 13 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/5**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Tranches Pot Holes an damage portion of Roads from Ali School to Football Chowk

in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7,37,958.00*/= + O/R

*BID SECURITY.* Rs. ***14,759***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,37,958.00*/= + O/R

Earnest Money Rs. ***14,759***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Tranches Pot Holes an dmage portion of Roads from Ali School to Footbal Chowk

in Orangi Zone..

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 5000 Sft | 773.86 %  Sft | 38,693/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 9000 Cft | 1437.00 %  Cft | 12,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11500 Cft | 1065.00 % CFT | 1,22,475/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | Premixed Patch Repair 1” including cleanng cutting scattered patches in proper shape laying premixed chips, rolling etc. complete. (Rate i/c all cost of materials. T & P and carriage upto 3 chins.)  P-09/19 using Crushed Bajri, laying premixed Carpet. | 10000 Sft | 3779.09 % Sft  986.02 % Sft  4765.11 % Sft | 4,76,511/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 38 Nos. | 913.63  Each | 34,718/= |
| **SUB TOTAL PART-A** | | | | **7,37,958/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Repairing of Tranches Pot Holes an dmage portion of Roads from Ali School to Footbal Chowk

in Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4200 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/6**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: P/F Main hole covers in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *9,58,432.00*/=

*BID SECURITY.* Rs. ***19,169***/=

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/6**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *9,58,432.00*/=

Earnest Money Rs. ***19,169***/=

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: P/F Main hole covers in Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 980 Nos.  60 Nos. | 913.63 Each  1051,25 Each | 8,95,357/=  63,075/= |
| **SUB TOTAL PART-A** | | | | **9,58,432/= +** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address : \_\_\_\_\_\_***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/7**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System near Madni Masjid in Chisty Nagar Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,58,277`.00*/= + O/R

*BID SECURITY.* Rs. *17,166*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/7**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,58,277.00*/= + O/R

Earnest Money Rs. *17,166*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System near Madni Masjid in Chisty Nagar Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 1 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5400 Cft | 4650.00 CFT | 25,110/- |
| 2 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 900 Rft | 367.00 Rft | 3,30,300/- |
| 3 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 40 Nos. | 13064.00  Each | 5,22,560/- |
| 4 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 80 Rft | 1540.00 Rft | (-) 1,23,200/- |
| 5 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4400 cft | 2760.00 P.cft | 12,144/= |
| 6 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 100 Nos. | 913.63  Each | 91,363/= |
| **SUB TOTAL PART-A** | | | | **8,58,277/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System near Madni Masjid in Chisty Nagar Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 7 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 40 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/8**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of R.C.C pipe & Main Hole in street No. 02 Baloch Mohallah in Orangi Zone

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,78,245`.00*/= + O/R

*BID SECURITY.* Rs. *17,565*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/8**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,78,245.00*/= + O/R

Earnest Money Rs. *17,565*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of R.C.C pipe & Main Hole in street No. 02 Baloch Mohallah in Orangi Zone

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 1 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5400 Cft | 4650.00 CFT | 25,110/- |
| 2 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 900 Rft | 367.00 Rft | 3,30,300/- |
| 3 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 42 Nos. | 13064.00  Each | 5,48,688/- |
| 4 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 84 Rft | 1540.00 Rft | (-) 1,29,360/- |
| 5 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4400 cft | 2760.00 P.cft | 12,144/= |
| 6 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 100 Nos. | 913.63  Each | 91,363/= |
| **SUB TOTAL PART-A** | | | | **8,78,245/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of R.C.C pipe & Main Hole in street No. 02 Baloch Mohallah in Orangi Zone

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 7 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 30 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/9**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: P/F R.C.C. Ring Slab in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *OFFER RATE*

*BID SECURITY.* Rs. 2 % *OFFER RATE*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/9**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *OFFER RATE*

Earnest Money Rs. 2 % *OFFER RATE*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: P/F R.C.C. Ring Slab in Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 1 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 333 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address : \_\_\_\_\_\_***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 7/10**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 07/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Maintenance of Main Holes and Sewerage Line near Malik Chowk in Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,59,972`.00*/= + O/R

*BID SECURITY.* Rs. *17,199*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 7/10**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,59,972.00*/= + O/R

Earnest Money Rs. *17,199*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Maintenance of Main Holes and Sewerage Line near Malik Chowk in Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 1 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5400 Cft | 4650.00 CFT | 25,110/- |
| 2 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 900 Rft | 367.00 Rft | 3,30,300/- |
| 3 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 42 Nos. | 13064.00  Each | 5,48,688/- |
| 4 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 84 Rft | 1540.00 Rft | (-) 1,29,360/- |
| 5 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4400 cft | 2760.00 P.cft | 12,144/= |
| 6 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 80 Nos. | 913.63  Each | 73,090/= |
| **SUB TOTAL PART-A** | | | | **8,59,972/= + O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Maintenance of Main Holes and Sewerage Line near Malik Chowk in Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 7 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 35 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***