**SCHEDULE-B**

**REMAINING WORK OF DARGAH KHANAN SHAH TALUKA & DISTRICT KHAIRPUR.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR NO.** | **ITEM OF WORKS** | | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| **01.** | Excavation in foundation of buildings bridges and other structures including dag belling dressing refilling around structure with excavated earth watering and ramming lead upto 5ft. (b) in ordinary soil. (S.I.No.18 P.No.5). | | **234.00** | **3176/25** | **%0Cft** | **Rs.748/-** |
|  |  |  |  |  |  |  |
| **02.** | Cement concrete brick or stone ballast 1-1/2 to 2”gauge. Ratio 1:5:10. (S.I.No.4 P.No.17). | | **59.00** | **8694/95** | **%Cft** | **Rs.5130/-** |
|  |  |  |  |  |  |  |
| **03.** | Random Rubble Masonry ratio 1:6 (S.I.No.21 P.No.27). | | **205.00** | **17723/-** | **%Cft** | **Rs.36332/-** |
|  |  |  |  |  |  |  |
| **04.** | Coursed Rubble masonry i/c hummer dressing in cement sand mortar ratio 1:6 (S.I.No.2 P.No.27). | | **183.00** | **25321/-** | **%Cft** | **Rs.46337/-** |
|  | ` |  |  |  |  |  |
| **05.** | Fabrication of mild steel reinforcement for cement concrete including cutting bending, laying in position making joints and fastenings including cost of binding wire also including cost of binding wire also includes removal of rust from bars.(S.I.No.07 P.No.20). | | **2.267** | **5001/70** | **P.Cwt** | **Rs.11343/-** |
|  |  |  |  |  |  |  |
| **06.** | R.C.C works in roof slab, beams columns rafts lintels and other structural members laid in situ recast laid in position complete in all respects ratio 1:2:4 90lbs cement 2cft sand 4cft shingle 1/8 to ¼ gauges (S.I.No.06 P.No.19). | | **73.00** | **337/-** | **P.Cft** | **24601/-** |
|  |  |  |  |  |  |  |
| **07.** | Pacca Brick work other than building sand cement mortar Ratio 1:6. (S.I.No.21 P.No.58). | | **443.00** | **12674/65** | **%Cft** | **54696/-** |
|  |  |  |  |  |  |  |
| **08.** | Cement plaster 1:6 upto 20 height ½ thick. (S.I.No.13 P.No.58). | | **2688.00** | **2206/60** | **%Sft** | **Rs.59313/-** |
|  |  |  |  |  |  |  |
| **09.** | Cement plaster 1:4 upto 20 height 3/8 thick. (S.I.No.11 P.No.58). | | **7337.00** | **2197/52** | **%Sft** | **Rs.161232/-** |
|  |  |  |  |  |  |  |
| **10.** | P/F Glazed tiles (6”x6”x1/4) or imported glass on wall facing in required colour and pattern i/c jointed in white cement or solution and pigment over base of 1:2 grey cement mortar ¼: thick i/c washing and filling of jointed in desired shape with finishing cleaning and cost of wax polish etc complete i/c writing of holly Quran in various pieces. (R.A). | | **2610.00** | **30509/77** | **%Sft** | **Rs.796305/-** |
|  |  |  |  |  |  |  |
| **11.** | Cement concrete plain including placing compacting finishing and curing, complete (including screening and washing of stone aggregate without shuttering Ratio 1:3:6. (S.I.No.05 P.No.18). | | **78.00** | **14429/25** | **%Cft** | **Rs.11255/-** |
|  |  |  |  |  |  |  |
| **12.** | P/F 3/8”thick marble tiles of approved quality & colour etc completed. | | **513.00** | **201/07** | **P-Sft** | **Rs.103149/-** |
|  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR NO.** | **ITEM OF WORKS** | | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| **13.** | Single layer of tiles 9”x4”½”x2” laid over 4”earth 1”mud plaster without bhoosa grouted (S.I.No.5 P.No.33). | | **808.00** | **5310/35** | **%Sft** | **Rs.42908/-** |
|  |  |  |  |  |  |  |
| **14.** | Distempering three coats (S.I.NO.4 (c) P.No.67). | | **2212.00** | **1079/65** | **%Sft** | **Rs.23882/-** |
|  |  |  |  |  |  |  |
| **15.** | Painting doors & windows any type three coats (S.I.No.4 c( iii) P.no.67). | | **468.00** | **1489/68** | **%Sft** | **Rs.6972/-** |
|  |  |  |  |  |  |  |
| **16.** | Painting guard bars, gates iron bars gratings; railings including standard braces etc similar open work two coats (S.I.No.11 P.No.76). | | **316.00** | **674/60** | **%Sft** | **Rs.2132/-** |
|  |  |  |  |  |  |  |
|  |  |  | **TOTAL** | | | **Rs.1386330/-** |

% Above/Below (Amount to be added/deducted).Rs.

**Grand Total** Rs.

Total Amount in word:

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |

**PART-B NON-SCHEDULE ITEM**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **ITEM OF WORKS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  |  |  |  |  |  |
| **01.** | Providing & Fixing Golden tiles etc completed. | 905.00 |  | **%Sft** | **Rs.** |
|  |  |  |  |  |  |
|  |  |  | **TOTAL** | | **Rs.** |
|  |  |  |  |  |  |

% Above/Below (Amount to be added/deducted).Rs.

**Grand Total** Rs.

Total Amount in word:

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |