NAME OF WORK: - **Construction of Surface Drains & Paving Block at Village Gigra Kalhora UC Ripri.**

Name of Contractor: - \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Whom tender issued: - GOVERNMENT CONTRACTOR

Tender fee received : - \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

D.R No : - \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Dated : - \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| **EXECUTIVE ENGINEER**  PUBLIC HEALTH ENGINEERING  DIVISION-II KHAIRPUR @ RANIPUR |

MEMORANDUM

General Description As Above

Estimated Cost Rs. 480000p0/-

Earnest Money @ 2% Rs. 96000/-

Security Deposit @10% Rs. 480000/-

Percentage if any to be Rs. 384000/-

Deduction from bill 8%

Date of written order to complete **12 Months**

I/We here by tendered for execution of above work at percentage rate \_\_\_\_\_\_\_\_\_ below/above on schedule rate in the schedule B in accordance with section designed drawing etc and shall executed the agreement on the proper from in case may tender in accepted.

Earnest shape of call deposit vide no\_\_\_\_\_\_\_\_\_\_\_\_\_ dated \_\_\_\_\_\_\_\_\_\_\_ for Rs\_\_\_\_\_\_\_ of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contractor

**EXECUTIVE ENGINEER**

PUBLIC HEALTH ENGINEERING

DIVISION-II KHAIRPUR @ RANIPUR

Bid Reference No:- **Construction of Surface Drains & Paving Block at Village Gigra Kalhora UC Ripri.**

To,

The Executive Engineer,

Public Health Engg. Division-II

**Khairpur.**

**GENTLEMAN.**

1. Having examined the Bidding Documents instructions to bidders, bidding datea conditions of Contract, Contract Data, specification, Drawings, if any, Schedule of prices and agenda Nos: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ for the execution of the above named works, we the undersigned being a company doing business under the name of and address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ and being duly incorporated under the laws of Pakistan hereby offer to execute, and complete such work and remedy any defects therein in conformity with the said Documents including agenda there to for the Total Bid Price of Rs.\_\_\_\_\_\_\_\_\_\_\_ (Rupees \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_) of such other sum as my be ascertained in accordance with said Documents.
2. We understand that all the schedules attached here to form part of this Bid.
3. As security for due performance of the undertaking and obligations of this Bid, we submit herewith a bid security in the shape of call deposit No. \_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated: \_\_\_\_\_\_\_\_\_\_\_ Bank \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ in the amount of Rs. \_\_\_\_\_\_\_\_\_\_\_\_\_\_ drawn in your favour or made payable to your and valid for a period of twenty eight (242) days beyond the period of validity of Bid.
4. We undertake, if our Bid is accepted to commence the work and to deliver and complete the work comprised in the contract within the time9s) stated in contract data.
5. We agreed to abide by this Bid for the period of **12 Months** from the date fixed for receiving the same and it shall remain binding upon and may be acceptable at any time before the expiration of that period.
6. Unless and until a formal agreement is prepared and executed this bid together with your written acceptance thereof, shall constitute a binding contract between us.
7. We undertake if our Bid is accepted to execute the performance security referred to in conditions of contract for the due performance of the contract.

**Contd: P/2**

1. We understand that you are not bound to accept the lowest or any bid your may receive.
2. We do hereby declare that the Bid is made without any collusion comparison of figures or arrangement with any other person or persons making a bid for the works.

Date this \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 2017.

Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

In the capacity of \_\_\_\_\_\_\_\_\_\_\_\_\_ duly authorized to sign bid for and on behalf of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

(Name of Bidder in Block Capitals).

**(S E A L)**

Address:

WITNESS:

Signature:- \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name :-

Address :-

|  |
| --- |
| Executive Engineer  Public Health Engineering  Division II Khairpur @ Ranipur |

**BIDDING DATA**

(This section should be filled in by the Executive Engineer Public Health Engineering Division-II Khairpur @ Ranipur before issuance of the Bidding Documents).

|  |  |
| --- | --- |
| **a)** Name of Procuring Agency | **Executive Engineer Public Health Engineering Division-II Khairpur @ Ranipur** |
| **b)** Brief Description of Work | **Construction of Surface Drains & Paving Block at Village Gigra Kalhora UC Ripri.** |
| **c)** Procuring Agency’s address | **Office of the Executive Engineer Public Health Engineering Division-II Khairpur @ Ranipur** |
| **d)** Estimated Cost | **Million: 4.800** |
| **e)** Amount of Bid Security | **2%** |
| **f)** Period of Bid Validity (Days) | **90 Days** |
| **g)** Security Deposit (Including Bid Security) | **10%** |
| **h)** Percentage if any, to be deducted from bills (Income . Tax + Security Deposit) | **Income Tax Rs: 7.5%**  **Security Deposit Rs: 10%** |
| **i)** Deadline for submission of Bids along with time. |  |
| **j)** Venue, Time and Date of Bid opening | **Office of the Executive Engineer Public Health Engineering Division-II Khairpur @ Ranipur** |
| **k)** Time for completion from written order of commence. | **12 Months** |
| **l)** Liquidity Damages | **0.5%** |
| **m)** Deposit Receipt \_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Amount \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | |
| **n)** D.R No:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date and Amount \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | |
| **o)** Tender issued to \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | |

**(Authority Issuing Bidding Documents)**

|  |
| --- |
| ***EXECUTIVE ENGINEER***  PUBLIC HEALTH ENGINEERING  DIV-II KHAIRPUR @ RANIPUR |

***schedule b***

**NAME OF WORK :-construction of SURFACE DRAINS & C.C PAVING BLOCK AT VILLAGE GIGRA KALHORA U/C RIPRI TALUKA GAMBAT DISTRICT KHAIRPUR.**

**part .i Surface drains**

1. Excavation in foundation of building bridges and other structure

i/c dag belling refilling around the structure with excavated

earth watering ramming lead up to one chain and lift up to 5 ft

. (PH Sch. No.18 P.NO.4)

Qty. 5517.00 Cft. @Rs.3176/25 P%0 Cft. Rs:17523 /-

1. Cement concrete plain i/c placing compacting finishing curing

complete i/c screening and washing stone aggregate w/o

shuttering (CSI No.5(i) P.NO.16) **(a) Ratio 1:4:8**

Qty. 1191.75 Cft. @Rs.11288/75 P% Cft. Rs:134534/-

1. Pacca Brick work in foundation and plinth in cement sand Ratio

(CSI No47(e) P.NO.20)

Qty. 3150.00 Cft @Rs.11948/36 P% Cft Rs.376373/-

1. Construction of standard of open drains cunette block

of cement concrete 1:2:4 in situ to design profile i/c cost

of mould as per drawing i/c applying floating coat of

cement 1/32” thick to the exposed face finished smooth

curing etc complete as per detail drawing

(PHSI No. D P.NO.58)

T–I

Qty.1350.00 Rft. @Rs.94/- P. Rft. Rs.126900 /-

T–II

Qty.500.00 Rft. @Rs:174/- P. Rft. Rs.87000/

1. Cement plaster 1:4 20’ height ½” thick (CSI No.11 (b) P.NO.52)

Qty.4875.00 Sft @Rs.2283/93 P% Sft Rs.111342/-

1. RCC work in roof slab, beams columns rafts, lintels, and other

structure members laid in situ of pre cost laid in position

complete in all respect 1:2:4 (CSI No.6 (a) P.NO.16)

Qty. 340.16 Cft @Rs.337/- P.Cft Rs:114635/-

1. Fabrication of mild steel reinforcement for cement concrete i/c

cutting bending laying in position making K=joints and

fastering i/c cost of binding wire also i/c removal of rust from

bars (CSI No.7(ii) P.NO.19).

Qty. 12.15Cwt @Rs.5001.70 P.Cwt Rs:60764 /-

**Total Rs:1029071 /-**

**PART.II C.C Block**

1. Barrow pit excavation undressed lead up to 100 ft in

ordinary soil (CSI-3(a) P-1)

Qty. 1983.00CFT @Rs.2117/50 P%0 Cft. Rs.4199 /-

2. Lying Earth in 6” layers & leveling dressing &

Watering for Etc complete. (CSI-13(b)P-3)

Qty. 7500.00 CFT @Rs.263/- P%0 Cft Rs.1973 /-

3.Extra for every 50”ft additional lead or part there of

(C.S.I No: 8 (a) P-3)

Qty: 1983.00CFT @Rs.5039/- P%0 Cft Rs.9992/-

4. Cement concrete brick or stone ballast 1 ½” to 2” guage

Ratio 1:4:8 (CSI No.4(b)9 P. 15).

Qty. 1650.00 CFT @Rs.9416/28 P% Cft. Rs.155369/-

5. Cement concrete plain 1:2:4 i/c placing compacting

finishing and curing complete i/c screening and washing

of stone aggregate without shuttering

(CSI No.5 P.No.16)

Qty. 1250.00 CFT @Rs.14429/25 P% Cft. Rs.180366 /-

6. Errection and removal of conctten R,C C or plan CC of partal wool

(CSI No.5 P.No.16)

Qty. 250.00 CFT @Rs.3127.41 P% Cft. Rs.7819 /-

**Total Rs.359718/-**

**PART.IIi PAVERS Block**

1. Cement concrete plain 1:2:4 i/c placing compacting

finishing and curing complete i/c screening and washing

of stone aggregate without shuttering

(CSI No.5 P.No.16)

1. **Ratio.1:4:8**

Qty. 206.25 CFT @Rs.11288.75 P% Cft. Rs.23283 /-

1. **Ratio.1:2:4**

Qty. 181.50 CFT @Rs.14429.25 P% Cft. Rs.26189 /-

1. Hard Murrum or fine powdery Murrum (GSMI NO.71 P.NO.4)

Qt. 2750.00 Sft. @Rs 1800.00 P% Sft. Rs.49,500/-

1. Providing and fixing cement paving block flooring having size

197x97x60(mm) of city / quddra coble shape with natural

colours having strength b/w 5000 psi 8500 psi i/c filling the

joints with hill sand and laying in specified manner / pattern and design etc

complete. (CSI NO 71 P. NO:49 )

Qty. 11000.00 Sft @Rs.199/77 P Sft. Rs.2197470/-

1. Dry brick on edge paving sand grouted i/c preparation of bed by watering ramming and bringing the same to proper chamber ½’’ thick mud plaster.

(CSI No.5 P.No.39)

Qty. 3000.00 CFT @Rs.3823.57 P% Cft. Rs.114707/-

**Total Rs.2411149/-**

**ABSTRACT OF COST**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SNO | Name of Work | Schedule Amount | Non Schedule Amount | G Total |
| 1 | Surface Drains | Rs:1029071 /- | ----- | Rs:1029071 /- |
| 2 | CC Block | Rs.359718/- | ------ | Rs.359718/- |
| 3 | Pavers Block | Rs.2411149/- | ----- | Rs.2411149/- |
|  | Total | Rs.3799938/- | ----- | Rs.3799938/- |

***C O N D I T I O N S***

01. Any error/omission in the description of item of work rate original schedule will correct accordingly under Executive Engineer, Public Health Engineering Division-II Khairpur

02. No premium will be allowed as Non-Schedule Items

03. The work will be carried out as per P.W.D specification and approval details working estimates

|  |
| --- |
| ***EXECUTIVE ENGINEER***  PUBLIC HEALTH ENGINEERING  DIVISION-II KHAIRPUR |

***(CONTRACTOR)***