Name of work: M/R TO CHIEF MINISTER HOUSE KARACHI DAY TO DAY COMPLAINTS HARD WARE & SANITARY ITEMS)

Schedule B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S. No. | Description | Qty | Rate | Unit | Amount |
| 1 | Nyloon Wire Guaze 144 mesh per square inch fixed to chowkats with ¾”deodar strips and sc | 330.00 | 193/53 | SFT | 63865 |
| 2 | P/F GI expended metal 1/2”to ¾” mesh 16 guage fixed to chowkats without deodar patti (S.I.65B/66) | 330.00  Sft | 60/43 | Sft | 22483 |
| 3 | P/F with sunk iron screwes wooden archtrative approved design shape having with not less then 3.7lbs 2-1/2 inches as directed by Engineer Incharge (S.I.6 | 330.00 | 49/97 | Sft | 16490 |
| 4 | P/F approved quality mortice lock | 12-Nos | 1786/13 | Each | 21439 |
|  | Total |  |  |  | 124272 |
|  | Total A |  |  |  |  |
|  | Part C N.S.Items |  |  |  |  |
| 1 | P/F Hydrollic door closer as per approved quality by the Engineer Incharge etc | 16-Nos |  | “ |  |
| 2 | S/F UPVC Pipe 1”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 120-Rft |  | Rft |  |
| B | --do—3./4”dia | 100-Rft |  | Rft |  |
| 3 | S/F Basin Mixture (Master make) or equelent quality etc complete. | 8-Nos |  | “ |  |
| 4 | P/F Tee Stop Cock master make in CP coated as directed by Engineer Incharge etc complete. | 24-Nos |  | “ |  |
| 5 | P/F Water Heater Geyser 30 Gallons Singer make or equelent quality i/c necessary fitting the cost of i/c as directed by the consultant. | **2-No** |  | **Each** |  |
| 6 | S/F CI man hole cover size 24”x24” as approved quality by the Engineer Incharge etc complete. | 12-Nos |  | Each |  |
| 7 | P/F Basin Pedistal as approved quality. | 8-Nos |  |  |  |
| 8 | P/F Handle door Lock as approved quality | 12-Nos |  |  |  |
| 9 | S/F Cement Bag as per approved quality etc com | 3-Nos |  | “ |  |
| 10 | S/F double bib cock heavy pattern as per approved quality as directed by the Engineer Incharge etc complete. | 12-Nos |  | ` |  |
| 11 | P/F GI Angle 18x18 as approved quality | 3-Nos |  |  |  |
| 12 | P/F Ply Sheet 36x18 as per approved quality. | 3-Nos |  |  |  |
| 13 | P/F Long Hinges ½”x6” as per approved quality | 12-Packet |  |  |  |
| 14 | S/O Steel Nails 2”long as approved quality | 12-Packet |  |  |  |
| 15 | P/F Draws Lock as per approved quality | 12-Nos |  |  |  |
|  | Total C |  |  |  |  |
|  | G Total |  |  |  |  |
|  | Say Rs |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Buildings sub Division-IX,

Karachi