**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/1**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement of sewerage System near H.NO. 1255/F-C and other gali at Masqati Mollaha in U.C # 21 Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,53,728.00* /= + O/R

*BID SECURITY.* Rs. *17,075*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/1**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,53,728.00/=* + O/R

Earnest Money Rs. *17,075*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement of sewerage System near H.NO. 1255/F-C and other gali at Masqati Mollaha in U.C # 21 Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | -2327 Cft | 3327.50 %  Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | -3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 8 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6891 Cft | 1065.00 % CFT | 73,389/= |
| 9 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 25 Nos. | 913.63  Each | 22,841/= |
| **SUB TOTAL PART-A** | | | | **8,53,728/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement of sewerage System near H.NO. 1255/F-C and other gali at Masqati Mollaha in U.C # 21 Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | Hiring of private Labour for cleaning of Nallah (by Afghani or Bajorri for 8 hours.) O/R | 40 Nos. | Offer Rate | Offer Rate |
| 11 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 1500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/2**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation / Improvement of RCC pipe & Man Hole near Masjid Yousuf Al-gillani in U.C # 21, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,68,268.00* /= + O/R

*BID SECURITY.* Rs. *17,365*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/2**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,68,268.00* /= + O/R

Earnest Money Rs. *17,365*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation / Improvement of RCC pipe & Man Hole near Masjid Yousuf Al-gillani in U.C # 21, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2387 Cft | 3327.50 %  Cft | 79,427/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 6094 Cft | 10770.00 CFT | 65,632/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 61.25 Rft | 1540.00 Rft | (-) 94,325/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 5301 cft | 2760.00 P.cft | 14,631/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3180 Cft | 1065.00 % CFT | 33,867/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | (-) 40 Nos. | 913.63  Each | 36,545/= |
| **SUB TOTAL PART-A** | | | | **8,68,268/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation / Improvement of RCC pipe & Man Hole near Masjid Yousuf Al-gillani in U.C # 21, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | (-)28 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/3**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation and Improvement of Sewerage System by RCC pipe from Farahan High School to Al hajj Pakwan Center, U.C # 08 Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,95,718.00*/= + O/R

*BID SECURITY.* Rs. *17,914*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/3**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,95,718.00* /= + O/R

Earnest Money Rs. *17,914*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation and Improvement of Sewerage System by RCC pipe from Farahan High School to

Al hajj Pakwan Center, U.C # 08 Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.3.6, | 975 Cft | 1306.80 % Cft | 12,741/= |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2156 Cft | 3327.50 %  Cft | 71,741/= |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 2025 Cft | 4650.00 CFT | 9,416/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3375 Cft | 10770.00 CFT | 36,349/- |
| 05 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 800 Rft | 367.00 Rft | 2,93,600/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 43 Rft | 1540.00 Rft | (-) 65,450/- |
| 08 | P/L 1.3.6 CC using GSB ¾”and down gauge i/c consolidation, curing etc complete with out shuttering. | 204 cft | 12595.00 % cft | 25,730/- |
| 09 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1165 cft | 2760.00 P.cft | 3,215/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3000 Cft | 1065.00 % CFT | 31,950/= |
| 11 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 21 Nos. | 913.63  Each | 19,186/= |
| **SUB TOTAL PART-A** | | | | **8,95,718/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Improvement of Rcc pipe & Main Hole Gali # 01 Islam Nagar U.C-22.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 12 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 25 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/4**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System gali # 01 Eliahabad, in U.C # 22, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,27,326.00*/= + O/R

*BID SECURITY.* Rs. *16,547*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/4**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,27,326.00* /= + O/R

Earnest Money Rs. *16,547*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System gali # 01 Eliahabad, in U.C # 22, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2200 Cft | 3327.50 %  Cft | 73,205/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 6094 Cft | 4650.00 CFT | 28,337/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 61.25 Rft | 1540.00 Rft | -94,325/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 5301 cft | 2760.00 P.cft | 14,631/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2993 Cft | 1065.00 % CFT | 31,875/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 45 Nos. | 913.63  Each | 41,113/= |
| **SUB TOTAL PART-A** | | | | **8,27,326/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System gali # 01 Eliahabad, in U.C # 22, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1313 Cft | Offer Rate | Offer Rate |
| 10 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 27 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/5**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System & Main Holes near unique Hospital gali & other area of shah

Mollaha # III U.C # 21, in Orngi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,20,845.00*/= + O/R

*BID SECURITY.* Rs. *16,417*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,20,845.00* /= + O/R

Earnest Money Rs. *16,417*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System & Main Holes near unique Hospital gali & other area of shah

Mollaha # III U.C # 21, in Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1563 Cft | 3327.50 %  Cft | 52,009/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 6094 Cft | 10770.00 CFT | 65,632/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 34 Nos. | 13064.00  Each | 4,44,176/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 59.5 Rft | 1540.00 Rft | -91,630/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 5410 cft | 2760.00 P.cft | 14,932/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2247 Cft | 1065.00 % CFT | 23,931/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 40 Nos. | 913.63  Each | 36,545/= |
| **SUB TOTAL PART-A** | | | | **8,20,845/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System & Main Holes near unique Hospital gali & other area of shah

Mollaha # III U.C # 21, in Orngi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1641 Cft | Offer Rate | Offer Rate |
| 10 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 30 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/6**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of damages R.C.C pipe & Main Hole opposite graveyard Shah Mollaha # 02,

U.C # 21, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,58,490.00*/= + O/R

*BID SECURITY.* Rs. *17,170*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/6**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,58,490.00* /= + O/R

Earnest Money Rs. *17,170*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of damages R.C.C pipe & Main Hole opposite graveyard Shah Mollaha # 02,

U.C # 21, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2496 Cft | 3327.50 %  Cft | 83.054/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 6094 Cft | 10770.00 CFT | 65,632/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 61.25 Rft | 1540.00 Rft | -94,325/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 5410 cft | 2760.00 P.cft | 14,932/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3180 Cft | 1065.00 % CFT | 33,867/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 25 Nos. | 913.63  Each | 22,840/= |
| **SUB TOTAL PART-A** | | | | **8,58,490/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of damages R.C.C pipe & Main Hole opposite graveyard Shah Mollaha # 02,

U.C # 21, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1313 Cft | Offer Rate | Offer Rate |
| 10 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 16 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/7**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /08/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair of cc drain / Slab near Unique Hospital, Shah Mollaha, UC # 21, Orangi Zone,

D.M.C (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *4,45,614.00*/= + O/R

*BID SECURITY.* Rs. *8,912*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/7**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *4,45,614.00*/= + O/R

Earnest Money Rs. *8,912*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair of cc drain / Slab near Unique Hospital, Shah Mollaha, UC # 21, Orangi Zone,

D.M.C (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of Rcc separating reinforcement from concrete cleaning & straightening (10/20) | 299 Cft | 5445.00%  Cft | 16,281/= |
| 02 | Cement concrete plain 1.2.4 i/c placing, compacting, finishing and curing complete i/c screening & washing of stone aggregate without shuttring. (17/5-1). | 123 cft | 14429.25 % Cft | 17,748/= |
| 03 | Erection and removal of centering for RCC or plain CC work in partal wood (vertical) (18/19-b-ii). | 296 sft | 3127.41 % Sft | 9,257/= |
| 04 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 5.055 cwt | 5001.70 %  Cft | 25,284/= |
| 05 | Rcc work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 250 cft | 337.00 cft | 84,250/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 15750 Cft | 1065.00 % CFT | 1,67,738/= |
| 09 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 938 Cft | 10770.00 CFT | 10,102/- |
| 10 | P/L RCC Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting, and Jointing with rubber ring etc complete. (Ch-18/2) 15” Dia, | 150 Rft | 367.00 Rft | 55,050/- |
| 11 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 06 Nos. | 13064.00  Each | 78,384/- |
| 12 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 12.0 Rft | 1540.00 Rft | -18,480/- |
| **SUB TOTAL PART-A** | | | | **4,45,614/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Repair of cc drain / Slab near Unique Hospital, Shah Mollaha, UC # 21, Orangi Zone,

D.M.C (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 07 | P/F RCC pre cast slab 2” thick of required size and shape and racking out Joints with CM curing etc complete as per direction of Engineer in charge O/R. | 175 Sft | Offer Rate | Offer Rate |
| 06 | Hiring of private Labour for cleaning of nallah afghani or Bajorri for 8 hours.) O/R | 350 Nos | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 32 Nos. | Offer Rate | Offer Rate |
|  |  |  |  |  |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 8/8**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 08 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of R.c.c pipe & Main Hole near H # 2603, Touheeddi Mollaha in U.C # 21, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,06,294.00* /= + O/R

*BID SECURITY.* Rs. *16,126*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 8/8**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,06,294.00* /= + O/R

Earnest Money Rs. *16,126*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of R.c.c pipe & Main Hole near H # 2603, Touheeddi Mollaha in U.C # 21, Orangi

Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1863 Cft | 3327.50 %  Cft | 61,991/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 4725 Cft | 4650.00 CFT | 21,971/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 15 “ Dia. | 630 Rft | 436.00 Rft | 2,74,680/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 32 Nos. | 13064.00  Each | 4,18,048/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 56 Rft | 1540.00 Rft | (-) 86,240/- |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6588 Cft | 1065.00 % CFT | 70,162/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **8,06,294/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of R.c.c pipe & Main Hole near H # 2603, Touheeddi Mollaha in U.C # 21, Orangi

Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2000 Cft | Offer Rate | Offer Rate |
| 09 | Hiring of private Labour for cleaning of nallah afghani or Bajorri for 8 hours.) O/R | 48 Nos | Offer Rate | Offer Rate |
| 10 | P/F Per Coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***