**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/1**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Rcc pipe & Man Hole near House # 2517/ FC, Faqeer colony, in U.C # 21, Orangi Zone, DMC (W).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,54,641.00* /= + O/R

*BID SECURITY.* Rs. *17,093*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/1**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,54,641.00/=* + O/R

Earnest Money Rs. *17,093*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Rcc pipe & Man Hole near House # 2517/ FC, Faqeer colony, in U.C # 21, Orangi Zone, DMC (W).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2327 Cft | 3327.50 %  Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6891 Cft | 1065.00 % CFT | 73,389/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 26 Nos. | 913.63  Each | 23,754/= |
| **SUB TOTAL PART-A** | | | | **8,54,641/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of Rcc pipe & Man Hole near House # 2517/FC, Faqeer colony, in U.C # 21, Orangi Zone, DMC (W).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | Hiring of private Labour for cleaning of Nallah (by Afghani or Bajorri for 8 hours.) O/R | 40 Nos. | Offer Rate | Offer Rate |
| 11 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 1500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/2**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair of sewerage system and cc street near H # 146 and 286 in ittifaq colony, H # 146 and 82

in Aziz Nagar, U.C # 17 Orangi Zone.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *9,04,522.00* /= + O/R

*BID SECURITY.* Rs. *18,090*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/2**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *9,04,522.00* /= + O/R

Earnest Money Rs. *18,090*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair of sewerage system and cc street near H # 146 and 286 in ittifaq colony, H # 146 and 82

in Aziz Nagar, U.C # 17 Orangi Zone.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 3909 Cft | 3327.50 %  Cft | 1,30,072/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1650 Cft | 4650.00 CFT | 7,673/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 300 Rft | 367.00 Rft | 1,10,100/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 13 Nos. | 13064.00  Each | 1,69,832/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 19.5 Rft | 1540.00 Rft | -30,030/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1282 cft | 2760.00 P.cft | 3,538/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 4277 Cft | 1065.00 % CFT | 45,550/= |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6000 Sft | 526.28%  Sft | 3,15,768/= |
| 09 | P/L 1.4.8 CC using GSB 2” to 3” and i/c leveling compacting, curing etc complete without shuttering. | 1500 cft | 11288.75 % cft | 1,69,331/= |
| 10 | P/L C.C Topping (1.2.4) i/c surface finishing & dividing into panelsa (ch-8/42/16-b-c) 2” th CC 1.2.4 | 6000 sft | 3275.50 % sft | 1,96,530/= |
| 11 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 77 Nos. | 913.63  Each | 70,350/= |
| **SUB TOTAL PART-A** | | | | **9,04,522/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair of sewerage system and cc street near H # 146 and 286 in ittifaq colony, H # 146 and 82

in Aziz Nagar, U.C # 17 Orangi Zone.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 12 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 320 Cft | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/3**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation / Improvement of Rcc pipe & Main Hole near Shahi Masjid, near Faisal Masjid,

Mujahid Shah House, Shah Mollaha in U.C # 21, Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,21,575.00* /= + O/R

*BID SECURITY.* Rs. *18,090*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/3**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,21,575.00* /= + O/R

Earnest Money Rs. *18,090*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation / Improvement of Rcc pipe & Main Hole near Shahi Masjid, near Faisal Masjid,

Mujahid Shah House, Shah Mollaha in U.C # 21, Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1900 Cft | 3327.50 %  Cft | 63,223/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5625 Cft | 4650.00 CFT | 26,156/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 33 Nos. | 13064.00  Each | 4,31,112/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 57.75 Rft | 1540.00 Rft | -88,935/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4832 cft | 2760.00 P.cft | 13,336/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 5516 Cft | 1065.00 % CFT | 58,745/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 42,682/= |
| **SUB TOTAL PART-A** | | | | **8,21,575/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation / Improvement of Rcc pipe & Main Hole near Shahi Masjid, near Faisal Masjid,

Mujahid Shah House, Shah Mollaha in U.C # 21, Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1650 Cft | Offer Rate | Offer Rate |
| 10 | P/F per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 25 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/4**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement and Repairing of Road / street by Haring of Tractor etc, at different location in

Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 2,63,427.00* /= + O/R

*BID SECURITY.* Rs. *5,269*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/4**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *2,63,427.00* /= + O/R

Earnest Money Rs. *5,269*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement and Repairing of Road / street by Haring of Tractor etc, at different location in

Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7600 Sft | 773.86%  Sft | 58,813/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 10750 Cft | 1437.00%0  Cft | 15,448/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14550 Cft | 1065.00 % CFT | 1,54,958/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6500 Sft | 526.28%  Sft | 34,208/= |
| **SUB TOTAL PART-A** | | | | **2,63,427/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement and Repairing of Road / street by Haring of Tractor etc, at different location in

Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1050 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4000 Cft | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 08 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/5**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of broken pipe & Main Hole and other work in Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *3,36,038.00* /= + O/R

*BID SECURITY.* Rs. *6,721*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *3,36,038.00* /= + O/R

Earnest Money Rs. *6,721*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of broken pipe & Main Hole and other work in Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1011 Cft | 3327.50 %  Cft | 33,641/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 576 Cft | 4650.00 CFT | 2,678/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 96 Rft | 367.00 Rft | 35,232/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 08 Nos. | 13064.00  Each | 1,04,512/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 14 Rft | 1540.00 Rft | -21,560/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 475 cft | 2760.00 P.cft | 1,311/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 55 Nos. | 913.63  Each | 50,250/= |
| 08 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 7219 Cft | 1437.00%0  Cft | 10,374/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 11230 Cft | 1065.00 % CFT | 1,19,600/= |
| **SUB TOTAL PART-A** | | | | **3,36,038/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of broken pipe & Main Hole and other work in Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3500 Cft | Offer Rate | Offer Rate |
| 11 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 12 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 02 Nos  (04 days) | Offer Rate | Offer Rate |
| 13 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 14 Nos  (10 days) | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/6**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing / Maintenance of Pot Hole near Urdu Chowk, Sabri Chowk and different location in

Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 2,62,121.00* /= + O/R

*BID SECURITY.* Rs. *5,242*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/6**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *2,62,121.00* /= + O/R

Earnest Money Rs. *5,242*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing / Maintenance of Pot Hole near Urdu Chowk, Sabri Chowk and different location in

Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7500 Sft | 773.86%  Sft | 58,040/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 10750 Cft | 1437.00%0  Cft | 15,448/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14500 Cft | 1065.00 % CFT | 1,54,425/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6500 Sft | 526.28%  Sft | 34,208/= |
| **SUB TOTAL PART-A** | | | | **2,62,121/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing / Maintenance of Pot Hole near Urdu Chowk, Sabri Chowk and different location in

Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 900 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4050 Cft | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 08 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/7**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Main Road / Street Potholes and different area in Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 2,64,753.00* /= + O/R

*BID SECURITY.* Rs. *5,295*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/7**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *2,64,753.00* /= + O/R

Earnest Money Rs. *5,295*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Main Road / Street Potholes and different area in Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7500 Sft | 773.86%  Sft | 58,040/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 10750 Cft | 1437.00%0  Cft | 15,448/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14500 Cft | 1065.00 % CFT | 1,54,425/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 7000 Sft | 526.28%  Sft | 36,840/= |
| **SUB TOTAL PART-A** | | | | **2,64,753/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of Main Road / Street Potholes and different area in Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 900 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4050 Cft | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 02 Nos  (04 days) | Offer Rate | Offer Rate |
| 09 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/8**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing and cleaning of sewerage line by winching and Repairing of Man hole near Shahanshah Hotel in Yousuf Goth.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *5,23,818.00*/= + O/R

*BID SECURITY.* Rs. *10,476*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/8**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,23,818.00* /= + O/R

Earnest Money Rs. *10,476*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing and cleaning of sewerage line by winching and Repairing of Man hole near

Shahanshah Hotel in Yousuf Goth.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Cleaning inside sewerage lines completely restoring original silt free space /diameter of pipe lines-by labour and equipment Mechanically / electrically driven). Including accessories like pulley’s Steel rope, bucket and draggers sizing from 6” to 18” dia. Their” to an fro” pulling action ( No of passes shall be as many as required) would be taken in two phases (First phase entire length from down stream to up stream) bringing down peak hours sewerage to flow in side pipe line (as free flow) and in second phase from up stream to down stream of entire length ensuring no silt is observed in buckets (6” dia to 18” dia) except only sewerage water and finally passing a steel ball of dia 12” lesser that the diameter oif pipe but not exceeding 48” dia ball even for larger dia pipe to ensure perfect cleaning. The job includes all the hire / cost of equipment and accessories of above winching machine / devices along with / engines with winching drum set having, steel) rope pully mounted over it, steel bucket from 6” to 18” dia hooks and other protection likes Safety barriers, traffic signs, traffic cones ensuring no damages to pipe along with ensuring safety to labour and other public property / lives and removal of silts / solid during desalting and removal of silts / solid during desalting and clearance of site etc. complete as per full satisfaction of site engineer.  V). 24 “ dia | 600 Rft | 209.30 P.Rft | 1,25,580 |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 550 Cft | 4650.00 CFT | 2,558/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 8” Dia. | 100 Rft | 206.00 Rft | 20,600/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 06 Nos. | 13064.00  Each | 78,384/- |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 08.082 Rft | 1540.00 Rft | (-) 12,446/- |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 20,000 Cft | 1065.00 % CFT | 2,13,000/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 50 Nos.  48 Nos. | 913.63 Each  1051.25 Each | 42,682/=  50,460/= |
| **SUB TOTAL PART-A** | | | | **5,23,818/=**  **O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing and cleaning of sewerage line by winching and Repairing of Man hole

near Shahanshah Hotel in Yousuf Goth.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of street & road sides etc with POL . | 12 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of skilled Afghani labour for cleaning of Nallah in different points all respect. | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/9**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Cleaning of sewerage line and maintenance of main hole near Roshan Hospital in UC-38

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 7,77,145.00*/= + O/R

*BID SECURITY.* Rs. *15,543*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/9**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,77,145.00* /= + O/R

Earnest Money Rs. *15,543*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Cleaning of sewerage line and maintenance of main hole near Roshan Hospital in UC-38.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Cleaning inside sewerage lines completely restoring original silt free space /diameter of pipe lines-by labour and equipment Mechanically / electrically driven). Including accessories like pulley’s Steel rope, bucket and draggers sizing from 6” to 18” dia. Their” to an fro” pulling action ( No of passes shall be as many as required) would be taken in two phases (First phase entire length from down stream to up stream) bringing down peak hours sewerage to flow in side pipe line (as free flow) and in second phase from up stream to down stream of entire length ensuring no silt is observed in buckets (6” dia to 18” dia) except only sewerage water and finally passing a steel ball of dia 12” lesser that the diameter oif pipe but not exceeding 48” dia ball even for larger dia pipe to ensure perfect cleaning. The job includes all the hire / cost of equipment and accessories of above winching machine / devices along with / engines with winching drum set having, steel) rope pully mounted over it, steel bucket from 6” to 18” dia hooks and other protection likes Safety barriers, traffic signs, traffic cones ensuring no damages to pipe along with ensuring safety to labour and other public property / lives and removal of silts / solid during desalting and removal of silts / solid during desalting and clearance of site etc. complete as per full satisfaction of site engineer.  V). 24 “ Dia | 2000 P.Ft | 209.30 P.rft | 4,18,600 |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 550 Cft | 4650.00 CFT | 2,558/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 100 Rft | 367.00 Rft | 36,700/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 06 Nos. | 13064.00  Each | 78,384/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 09 Rft | 1540.00 Rft | (-) 13,860/- |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 20,000 Cft | 1065.00 % CFT | 2,13,000/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 25 Nos.  18 Nos. | 913.63 Each  1051.25 Each | 22,841/=  18,923/= |
| **SUB TOTAL PART-A** | | | | **7,77,145/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Cleaning of sewerage line and maintenance of main hole near Roshan Hospital in UC-38

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 09 Days | Offer Rate | Offer Rate |
| 10 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 55 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/10**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation and cleaning of sewerage line by winching and labour in Rahim Goth in

UC-38, Surjani Town.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 7,78,560.00*/= + O/R

*BID SECURITY.* Rs. *15,571*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/10**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,78,560.00* /= + O/R

Earnest Money Rs. *15,571*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation and cleaning of sewerage line by winching and labour in Rahim Goth in

UC-38, Surjani Town.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Cleaning inside sewerage lines completely restoring original silt free space /diameter of pipe lines-by labour and equipment Mechanically / electrically driven). Including accessories like pulley’s Steel rope, bucket and draggers sizing from 6” to 18” dia. Their” to an fro” pulling action ( No of passes shall be as many as required) would be taken in two phases (First phase entire length from down stream to up stream) bringing down peak hours sewerage to flow in side pipe line (as free flow) and in second phase from up stream to down stream of entire length ensuring no silt is observed in buckets (6” dia to 18” dia) except only sewerage water and finally passing a steel ball of dia 12” lesser that the diameter oif pipe but not exceeding 48” dia ball even for larger dia pipe to ensure perfect cleaning. The job includes all the hire / cost of equipment and accessories of above winching machine / devices along with / engines with winching drum set having, steel) rope pully mounted over it, steel bucket from 6” to 18” dia hooks and other protection likes Safety barriers, traffic signs, traffic cones ensuring no damages to pipe along with ensuring safety to labour and other public property / lives and removal of silts / solid during desalting and removal of silts / solid during desalting and clearance of site etc. complete as per full satisfaction of site engineer.  (v). 24” Dia | 2000 P.Rft | 209.30 Per Rft | 4,18,600 |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 550 Cft | 4650.00 CFT | 2,558/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 100 Rft | 367.00 Rft | 36,700/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 06 Nos. | 13064.00  Each | 78,384/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 09 Rft | 1540.00 Rft | (-) 13,860/- |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 20,000 Cft | 1065.00 % CFT | 2,13,000/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 30 Nos.  15 Nos. | 913.63 Each  1051.25 Each | 27,409/=  15,769/= |
| **SUB TOTAL PART-A** | | | | **7,78,560/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation and cleaning of sewerage line by winching and labour in Rahim Goth in

UC-38, Surjani Town.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | P/F Per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 10 Days | Offer Rate | Offer Rate |
| 10 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 55 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/11**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of RCC Pipe and main hole near Rehmani Masjid, Usmani Mohallah in UC # 22.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,55,575.00* /= + O/R

*BID SECURITY.* Rs. *17,112*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/11**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,55,575.00/=* + O/R

Earnest Money Rs. *17,112*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of RCC Pipe and main hole near Rehmani Masjid, Usmani Mohallah in UC # 22. **PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2400 Cft | 3327.50 %  Cft | 79,860/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 15 “ Dia. | 600 Rft | 436.00 Rft | 2,61,600/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 36 Nos. | 13064.00  Each | 4,70,304/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 60.869 Rft | 1540.00 Rft | -93,738/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6000 Cft | 1065.00 % CFT | 63,900/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 20 Nos. | 913.63  Each | 18,273/= |
| **SUB TOTAL PART-A** | | | | **8,55,575/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of RCC Pipe and main hole near Rehmani Masjid, Usmani Mohallah in UC # 22.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 36 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/12**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT/09 / /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System near Kabadi Ground and different area in U.C # 22,

Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,53,728.00*/= + O/R

*BID SECURITY.* Rs. 17,075/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/12**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 8,53,728 *.00*/= + O/R

Earnest Money Rs. 17,075/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System near Kabadi Ground and different area in U.C # 22,

Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2327 Cft | 3327.50 % Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kind of soil murum i/c trimming and dressing sides to true alignment & shape leveling of beds of tranches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) and 12” dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 35 Nos. | 13064 Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | 70 Rft  (-) | 1540.00 Rft | 1,07,800/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 2207 Cft | 2760.00 % Cft | 6,091/- |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide  & lift (Ch 1/1-1) | 6891 Cft | 1065.00 % CFT | 73,389/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 25 Nos. | 913.63 Each | 22,841/- |
| **SUB TOTAL PART-A** | | | | **8,53,728/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System near Kabadi Ground and different area in U.C # 22,

Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | Hiring of private Labour for cleaning of nallah afghani or Bajorri for 8 hours.) O/R | 40 Nos | Offer Rate | Offer Rate |
| 11 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 1500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/13**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT/09 / /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of Sewerage System near B.M School in UC-22, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,14,258.00*/= + O/R

*BID SECURITY.* Rs. 18,285/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/13**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 9,14,258 *.00*/= + O/R

Earnest Money Rs. 18,285/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of Sewerage System near B.M School in UC-22, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 3852 Cft | 3327.50 % Cft | 1,28,175/= |
| 02 | Excavation for pipe line in trenches & pits in all kind of soil murum i/c trimming and dressing sides to true alignment & shape leveling of beds of tranches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 5625 Cft | 4650.00 CFT | 26,156/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) and 12” dia. | 750 Rft | 367.00 Rft | 2,75,200/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 38 Nos. | 13064 Each | 4,96,432/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | 66.58 Rft  (-) | 1540.00 Rft | 1,02,534/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 4832 Cft | 2760.00 % Cft | 13,336/- |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide  & lift (Ch 1/1-1) | 4698 Cft | 1065.00 % CFT | 50,034/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 30 Nos. | 913.63 Each | 27,409/- |
| **SUB TOTAL PART-A** | | | | **9,14,258/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of Sewerage System near B.M School in UC-22, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 30 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/14**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT/09 / /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Maintenance of C.C Steps in gali # 5,6, and other gali in Zia Colony, Sheet # 01.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,66,930.00*/= + O/R

*BID SECURITY.* Rs. 11,339/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/14**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 5,66,930 *.00*/= + O/R

Earnest Money Rs. 11,339/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Maintenance of C.C Steps in gali # 5,6, and other gali in Zia Colony, Sheet # 01.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation of hard rock requiring blasting prohibited and disposal of excavated material up to 50 ft. Lead (including dressing and leveling to designed section etc complete. (2/7-b). | 675 cft | 25936.00  % cft | 17,507/- |
| 02 | Random Rubble masonry (Un coursed) Ratio 1:6 (Ch-6-28/3-d-iii). | 1013 cft | 18535.08 % cft | 1,87,760/- |
| 03 | Add extra Labour (First Floor)  (2nd Floor)  (3rd Floor)  (4th Floor)  Extra labour for every 5ft additional height of un covered wall. | 1013 cft | 626.18 % Cft  1439.90 % Cft  2268.75 % Cft  3654.20 % Cft  1149.50 % Cft  9138.53 % Cft | 92,573/- |
| 04 | Dressing stone (Hammer dressed) (30/9-a) | 1350 sft | 2390.00 % sft | 32,265/- |
| 05 | Grouting stone pitching of apron is 1:3 cement mortar.  ( 30/12). | 1350 Sft | 4480.44 % Sft | 60,486/- |
| 06 | Cement Plaster 1:4 up to 20 feet height ½” thick on walls. | 675 sft | 2283.93 % Sft | 15,417/- |
| 07 | Election and removal of centering for Rcc or plan CC work of partal wood. Vertical (18/19-b-ii). | 230 sft | 3127.41 % sft | 7,193/- |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9). | 5000 Sft | 526.28 % Sft | 26,314/= |
| 11 | P/L C.C Topping (1.2.4) i/c surface finishing & (CH-8/42/16-b-c) 1 ½ th C.C 1.2.4. | 5000 sft | 2548.29 % Sft | 1,27,415  /- |
| **SUB TOTAL PART-A** | | | | **5,66,930/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Maintenance of C.C Steps in gali # 5,6, and other gali in Zia Colony, Sheet # 01.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3300 Cft | Offer Rate | Offer Rate |
| 10 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 1450 Cft | Offer Rate | Offer Rate |
| 12 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 75 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/15**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT/09 / /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of steps in Hill area gali # 9, 10, and other gali in U.C # 01.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,70,680.00*/= + O/R

*BID SECURITY.* Rs. 11,414/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/15**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 5,70,680 *.00*/= + O/R

Earnest Money Rs. 11,414/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of steps in Hill area gali # 9, 10, and other gali in U.C # 01. **PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation of hard rock requiring blasting prohibited and disposal of excavated material up to 50 ft. Lead (including dressing and leveling to designed section etc complete. (2/7-b). | 675 cft | 25936.00  % cft | 17,507/- |
| 02 | Random Rubble masonry (Un coursed) Ratio 1:6 (Ch-6-28/3-d-iii). | 1013 cft | 18535.08 % cft | 1,87,760/- |
| 03 | Add extra Labour (First Floor)  (2nd Floor)  (3rd Floor)  (4th Floor)  Extra labour for every 5ft additional height of un covered wall. | 1013 cft | 626.18 % Cft  1439.90 % Cft  2268.75 % Cft  3654.20 % Cft  1149.50 % Cft  9138.53 % Cft | 92,573/- |
| 04 | Dressing stone (Hammer dressed) (30/9-a) | 1350 sft | 2390.00 % sft | 32,265/- |
| 05 | Grouting stone pitching of apron is 1:3 cement mortar.  ( 30/12). | 1350 Sft | 4480.44 % Sft | 60,486/- |
| 06 | Cement Plaster 1:4 up to 20 feet height ½” thick on walls. | 675 sft | 2283.93 % Sft | 15,417/- |
| 07 | Election and removal of centering for Rcc or plan CC work of partal wood. Vertical (18/19-b-ii). | 230 sft | 3127.41 % sft | 7,193/- |
| 12 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide  & lift (Ch 1/1-1) | 352.11 Cft | 1065.00 % CFT | 3,750/= |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9). | 5000 Sft | 526.28 % Sft | 26,314/= |
| 11 | P/L C.C Topping (1.2.4) i/c surface finishing & (CH-8/42/16-b-c) 1 ½ th C.C 1.2.4. | 5000 sft | 2548.29 % Sft | 1,27,415  /- |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **5,70,680/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of steps in Hill area gali # 9, 10, and other gali in U.C # 01.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3300 Cft | Offer Rate | Offer Rate |
| 10 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 1450 Cft | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 75 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/16**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT/09 / /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Providing and Fixing damages Main hole Covers and Ring slab near Shahjahan Chowk

& other area in U.C # 22, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 39,286.00*/= + O/R

*BID SECURITY.* Rs. 786/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/16**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 39,286 *.00*/= + O/R

Earnest Money Rs. 786/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Providing and Fixing damages Main hole Covers and Ring slab near Shahjahan Chowk

& other area in U.C # 22, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia & 24” Dia | 43 Nos. | 913.63 Each | 39,286/- |
| **SUB TOTAL PART-A** | | | | **39,286/=+O/R** |

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 11 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 320 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/17**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Replacement of R.C.C pipe and Maintenance of Sewerage System in U.C # 38 and

U.C # 39 in Surjani Town.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *3,74,391.00* /= + O/R

*BID SECURITY.* Rs. *7,488*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/17**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *3,74,391.00* /= + O/R

Earnest Money Rs. *7,488*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Replacement of R.C.C pipe and Maintenance of Sewerage System in U.C # 38 and

U.C # 39 in Surjani Town.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 354 Cft | 3327.50 %  Cft | 11,779/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 2600 Cft | 4650.00 CFT | 12,090/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 8” Dia, | 400 Rft | 206.00 Rft | 82,400/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 18 Nos. | 13064.00  Each | 2,35,152/- |
| 05 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 25 Nos. | 913.63  Each | 22,841/= |
| 06 | Billing or pumping out sub soil water during excavation concrete cast in situ or masonry work in foundation. Only three operation allowed. | 1865 cft | 543.00 % cft | 10,129/= |
| **SUB TOTAL PART-A** | | | | **3,74,391/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Replacement of R.C.C pipe and Maintenance of Sewerage System in U.C # 38 and

U.C # 39 in Surjani Town.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 07 | P/F per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 10 Nos | Offer Rate | Offer Rate |
| 08 | P/F R.C.C Pre cast slab 2” thick of required size and shape and racking out Joints with CM curing etc complete as per direction of engineer incharge. | 648 cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/18**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement & desalting of Nallah near House # 366, Shah Jahan Chowk, UC-22 Orangi

Zone, D.M.C (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 3,85,325.00* /= + O/R

*BID SECURITY.* Rs. *7,707*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/18**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *3,85,325.00* /= + O/R

Earnest Money Rs. *7,707*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement & desalting of Nallah near House # 366, Shah Jahan Chowk, UC-22 Orangi

Zone, D.M.C (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Hiring Seal Dumpers Hino for Lifting of Garbage & Silt of Nallah i/c loading & unloading in all respect with POL. ( For 8 hours Per Day). | 192 hours | 2006.90 Per Hour | 3,85,325 |
| **SUB TOTAL PART-A** | | | | **3,85,325/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Hiring of excavator for desalting and cleaning of nallah Long Boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
|  |  |  |  |  |
| 03 | Hiring of Loader for lifting of Garbage, & silt etc with POL ( For 8 hours Per Day) | 24 hours | Offer Rate | Offer Rate |
| 04 | Hiring of Private Labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 240 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/19**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement of C.C Drain and R.C.C Slab near House # 1236, Main Road UC-22, Orangi Zone,

D.M.C (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs. 7,86,681/- + O/R*

*BID SECURITY.* Rs. 15,734/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/19**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs. 7,86,681/- + O/R*

Earnest Money Rs. 15,734/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement of C.C Drain and R.C.C Slab near House # 1236, Main Road UC-22, Orangi Zone,

D.M.C (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of Rcc separating reinforcement from concrete cleaning & straightening (10/20) | 563 cft | 5445.00%  Cft | 30,655/= |
| 02 | Stone filling dry hand packed as filling behind retaining walls or in pitching and aprons. | 675 cft | 2684.00 %  Cft | 18,117/= |
| 03 | P/L 1.4.8 CC using GSB 2” to 3” and i/c leveling compacting, curing etc complete without shuttering. | 225 cft | 11288.75 % cft | 25,400/= |
| 04 | Cement concrete plain 1:2:4 i/c placing, compacting, finishing and curing completed i/c screening and washing of stone aggregate without shuttering. (17/5-f) | 1050 cft | 14429.25 % Cft | 1,51,507/= |
| 05 | Erection and removal of centering for Rcc or plan CC work of partal wood. Vertical (18/19-b-ii). | 2400 cft | 3127.41 % sft | 75,058/- |
| 06 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 250 cwt | 5001.70 %  Cft | 1,25,043/= |
| 07 | Rcc work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 450 cft | 337.00 cft | 1,51,650/= |
| 08 | Billing or pumping out sub soil water during excavation concrete cast in situ or masonry work in foundation. Only three operation allowed. | 5400 cft | 543.00 % cft | 29,322/= |
| 09 | S/F new jute bags 4 to 5 Cft capacity wh sand or earth laying in position under water, (79/3-b) | 400 Nos | 202.46 Each | 80,984/= |
| 11 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 720 Cft | 4650.00 CFT | 3,348/- |
| 12 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) and 12” dia. | 120 Rft | 367.00 Rft | 44,040/- |
| 13 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 05 Nos. | 13064 Each | 65,320/- |
| 14 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | 10 Rft (-) | 1540.00 Rft | (-) 15,400/- |
| 15 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 593 Cft | 2760.00 % Cft | 1.637/- |
| **SUB TOTAL PART-A** | | | | **7 ,86,681/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Improvement of C.C Drain and R.C.C Slab near House # 1236, Main Road UC-22, Orangi Zone,

D.M.C (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F RCC pre cast slab or i/c linter (I-beam) of required size and shape and racking out Joints with CM curing etc complete as per direction of Engineer in charge. | 900 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/20**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Sewerage Line near Farooque Masjid at Sector 8/L, and other places in U.C # 12.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,22,413.00* /= + O/R

*BID SECURITY.* Rs. ***16,448***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/20**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,22,413.00/=* + O/R

Earnest Money Rs. ***16,448***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Sewerage Line near Farooque Masjid at Sector 8/L, and other places in U.C # 12.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1050 Cft | 3327.50 %  Cft | 34,939/= |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.3.6, | 1218 Cft | 1306.80 %  Cft | 15,917/= |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3200 Cft | 4650.00 CFT | 14,880/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 1600 Cft | 10770.00 CFT | 17,232/- |
| 05 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 700 Rft | 367.00 Rft | 2,56,900/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 29.88 Rft | 1540.00 Rft | -46,011/- |
| 08 | P/L 1.3.6 CC using GSB ¾”and down gauge i/c consolidation, curing etc complete without shuttering. | 48 cft | 12595.00 % cft | 6,046/- |
| 09 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1600 cft | 2760.00 P.cft | 4,416/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 5741 Cft | 1065.00 % CFT | 60,854/= |
| **SUB TOTAL PART-A** | | | | **8,22,413/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of Sewerage Line near Farooque Masjid at Sector 8/L, and other places in U.C # 12.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 11 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 59 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/21**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation / Improvement of pipe drain Sector 7-C, 9/E, in Orangi Zone D.M.C (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,36,633.00* /= + O/R

*BID SECURITY.* Rs. ***16,733***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/21**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,36,633.00/=* + O/R

Earnest Money Rs. ***16,733***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation / Improvement of pipe drain Sector 7-C, 9/E, in Orangi Zone D.M.C (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1050 Cft | 3327.50 %  Cft | 34,939/= |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.3.6, | 1707 Cft | 1306.80 %  Cft | 22,307/= |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3200 Cft | 4650.00 CFT | 14,880/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 1600 Cft | 10770.00 CFT | 17,232/- |
| 05 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia. | 725 Rft | 367.00 Rft | 2,66,075/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 34 Nos. | 13064.00  Each | 4,44,176/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 31.00 Rft | 1540.00 Rft | -47,840/- |
| 08 | P/L 1.3.6 CC using GSB ¾”and down gauge i/c consolidation, curing etc complete without shuttering. | 96 cft | 12595.00 % cft | 12,091/- |
| 09 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1600 cft | 2760.00 P.cft | 4,416/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6418.50 Cft | 1065.00 % CFT | 68,357/= |
| **SUB TOTAL PART-A** | | | | **8,36,633/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation / Improvement of pipe drain Sector 7-C, 9/E, in Orangi Zone D.M.C (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 11 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 54 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/22**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement/Repair of sewerage system in Bismillah Town Sector 4-B Surjani town U.C-38.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,51,821/- +O/R*

*BID SECURITY.* Rs. ***17,036***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/22**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,51,821/- +O/R*

Earnest Money Rs. ***17,036***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement/Repair of sewerage system in Bismillah Town Sector 4-B Surjani town U.C-38

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2255 Cft | 3327.50 %  Cft | 75,035/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5250 Cft | 4650.00 CFT | 24,413/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 700 Rft | 367.00 Rft | 2,56,900/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 30 Nos. | 13064.00  Each | 3,92,920/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 30 Rft | 1540.00 Rft | -46,200/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4391 cft | 2760.00 P.cft | 12,119/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 8634 Cft | 1065.00 % CFT | 91,952/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **8,51,821/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement/Repair of sewerage system in Bismillah Town Sector 4-B Surjani town U.C-38

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 50 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/23**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair and maintenance of sewerage line in gali # 01 and 02 near jama-e-Masjid Aligarh in

U.C-13 Orangi Zone DMC west

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,36,633/- +O/R*

*BID SECURITY.* Rs. ***16,733***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/23**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,36,633/- +O/R*

Earnest Money Rs. ***16,733***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair and maintenance of sewerage line in gali # 01 and 02 near jama-e-Masjid Aligarh in

U.C-13 Orangi Zone DMC west

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.3.6. | 2041 Cft | 1306.80 %  Cft | 26,672/= |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1318 Cft | 3327.50 %  Cft | 43,856/= |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3025 Cft | 4650.00 CFT | 14,066/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 1988 Cft | 10770.00 CFT | 21,411/- |
| 05 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 8” Dia, 12” Dia, 15 “ Dia. | 50 Rft  700 Rft | 206.00 Rft  367.00 Rft | 10,300/-  2,56,900/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 47.5 Rft | 1540.00 Rft | -73,150/- |
| 08 | P/L 1.3.6 CC using GSB ¾”and down gauge i/c consolidation, curing etc complete without shuttering. | 20 cft | 12595.00 % cft | 2,519/- |
| 09 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2239 cft | 2760.00 P.cft | 6,180/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 4145 Cft | 1065.00 % CFT | 44,144/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 29 Nos. | 913.63  Each | 26,495/= |
| **SUB TOTAL PART-A** | | | | **8,36,634/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair and maintenance of sewerage line in gali # 01 and 02 near jama-e-Masjid Aligarh in

U.C-13 Orangi Zone DMC west

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 11 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-64/10). | 1988 Cft | Offer Rate | Offer Rate |
| 13 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 23 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/24**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of sewerage system in sector 5-B U.C-39 Surjani Town

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,51,900/- +O/R*

*BID SECURITY.* Rs. ***17,038***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/24**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,51,900/- +O/R*

Earnest Money Rs. ***17,038***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of sewerage system in sector 5-B U.C-39 Surjani Town

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2327 Cft | 3327.50 %  Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 8” Dia, 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6891 Cft | 1065.00 % CFT | 73,389/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 23 Nos. | 913.63  Each | 21,013/= |
| **SUB TOTAL PART-A** | | | | **8,51,900/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of sewerage system in sector 5-B U.C-39 Surjani Town

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | Hiring of private Labour for cleaning of Nallah (by Afghani or Bajorri for 8 hours.) O/R | 40 Nos. | Offer Rate | Offer Rate |
| 11 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 1500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/25**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of sewerage system and repair maintenance of main hole in sector L-1 U.C-39

sujani Town DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,19,672/- +O/R*

*BID SECURITY.* Rs. ***16,393***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/25**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,19,672/- +O/R*

Earnest Money Rs. ***16,393***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of sewerage system and repair maintenance of main hole in sector L-1 U.C-39

Sujani Town DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,76,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | -80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3018 cft | 2760.00 P.cft | 8,330/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2627 Cft | 1065.00 % CFT | 27,978/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 62 Nos. | 913.63  Each | 56,645/= |
| **SUB TOTAL PART-A** | | | | **8,19,672/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of sewerage system and repair maintenance of main hole in sector L-1 U.C-39

Sujani Town DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 45 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/26**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of sewerage system in yousuf Goth sector 2 surjani town U.C-38.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,74,755/- +O/R*

*BID SECURITY.* Rs. ***17,495***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/26**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,74,755/- +O/R*

Earnest Money Rs. ***17,495***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of sewerage system in yousuf Goth sector 2 surjani town U.C-38.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2250 Cft | 3327.50 %  Cft | 74,869/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 5250 Cft | 4650.00 CFT | 24,413/- |
| 03 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 700 Rft | 367.00 Rft | 2,56,900/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 30 Nos. | 13064.00  Each | 3,91,920/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 15 Rft | 1540.00 Rft | -23,100/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 4391 cft | 2760.00 P.cft | 12,119/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 8634 Cft | 1065.00 % CFT | 91,952/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **8,74,755/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of sewerage system in yousuf Goth sector 2 surjani town U.C-38.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 50 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/27**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair of RCC pipe main hole near chandni chowk and hiring of labour and tractor from nallah

desalting in Orangi Zone DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.3,13,197/- +O/R*

*BID SECURITY.* Rs. ***6,264***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/27**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.3,13,197/- +O/R*

Earnest Money Rs. ***6,264***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair of RCC pipe main hole near chandni chowk and hiring of labour and tractor from nallah desalting in Orangi Zone DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1011 Cft | 3327.50 %  Cft | 33,641/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 576 Cft | 4650.00 % 0 CFT | 2,678/- |
| 03 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 96 Rft | 367.00 Rft | 35,232/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 08 Nos. | 13064.00  Each | 1,04,512/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 14 Rft | 1540.00 Rft | -21,560/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 475 cft | 2760.00 P.cft | 1,311/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 30 Nos. | 913.63  Each | 27,409/= |
| 08 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 7219 Cft | 1437.00%0  Cft | 10,374/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 11230 Cft | 1065.00 % CFT | 1,19,600/= |
| **SUB TOTAL PART-A** | | | | **3,13,197/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair of RCC pipe main hole near chandni chowk and hiring of labour and tractor from nallah

desalting in Orangi Zone DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 900 Cft | Offer Rate | Offer Rate |
| 11 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3500 Cft | Offer Rate | Offer Rate |
| 12 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 13 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 08 Nos | Offer Rate | Offer Rate |
| 14 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 140 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/28**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: P/L sewerage line and repairing of pot holes in chilistan colony in Ghaziabad Orangi Zone DMC

west.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.3,64,400/- +O/R*

*BID SECURITY.* Rs. ***7,288***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/28**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.3,64,400/- +O/R*

Earnest Money Rs. ***7,288***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: P/L sewerage line and repairing of pot holes in chilistan colony in Ghaziabad Orangi Zone DMC

west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2000 Cft | 3327.50 %  Cft | 66,550/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1600 Cft | 4650.00 CFT | 2,299/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 400 Rft | 367.00 Rft | 1,46,800/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 10 Nos. | 13064.00  Each | 1,30,640/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 20 Rft | 1540.00 Rft | -30,800/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1170 cft | 2760.00 P.cft | 3,229/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **3,64,400/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: P/L sewerage line and repairing of pot holes in chilistan colony in Ghaziabad Orangi Zone DMC

west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 100 Nos | Offer Rate | Offer Rate |
| 08 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 5500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/29**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of pot holes in trenches and other work in Ali Nagar road sector 11 ½ Orangi Zone

DMC west

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.4,80,436/- +O/R*

*BID SECURITY.* Rs. ***9,609***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/29**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.4,80,436/- +O/R*

Earnest Money Rs. ***9,609***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of pot holes in trenches and other work in Ali Nagar road sector 11 ½ Orangi Zone

DMC west

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 2500 Sft | 3327.50%  Sft | 83,188/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 17600 Cft | 1437.00%  Cft | 25,291/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 20,100 Cft | 1065.00 % CFT | 2,14,073/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 30000 Sft | 526.28%  Sft | 1,57,884/= |
| **SUB TOTAL PART-A** | | | | **4,80,436/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of pot holes in trenches and other work in Ali Nagar road sector 11 ½ Orangi Zone

DMC west

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3000 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 5700 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/30**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of nallah RCC slab near Ghousia pan house at Touheed colony U.C-26

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.2,92,056/- +O/R*

*BID SECURITY.* Rs. ***5,841***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/30**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.2,92,056/- +O/R*

Earnest Money Rs. ***5,841***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of nallah RCC slab near Ghousia pan house at Touheed colony U.C-26

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of Rcc separating reinforcement from concrete cleaning & straightening (10/20) | 745 cft | 5445.00%  Cft | 40,565/= |
| 02 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 6.446 cwt | 5001.70 %  Cft | 32,241/= |
| 03 | Rcc work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 356 cft | 337.00 cft | 1,19,972/= |
| 04 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 6,505 Cft | 1065.00 % CFT | 69,278/= |
| 05 | Hire charges of pumping set of upto 10 H.P pumping out water from 10 ft deep trench. (P.H 76/23-1) | 20 days | 1500  per day | 30,000/= |
| **SUB TOTAL PART-A** | | | | **2,92,056/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Rehabilitation of nallah RCC slab near Ghousia pan house at Touheed colony U.C-26

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 06 | P/F RCC pre cast slab 2” thick of required size and shape and racking out joints with CM curing etc complete as per direction of engineer incharge. | 960 sft | Offer Rate | Offer Rate |
| 07 | P/F RCC pre cast slab or i/c linter of required size and shape and racking out Joints with CM curing etc complete as per direction of Engineer in charge. | 42 Sft | Offer Rate | Offer Rate |
| 08 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 250 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 40 hours | Offer Rate | Offer Rate |
| 10 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 07 days | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/31**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement of drain by RCC slab near house # 1690 in Ghousia Baloch colony U.C-19

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.2,23,840/- +O/R*

*BID SECURITY.* Rs. ***4,476***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/31**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.2,23,840/- +O/R*

Earnest Money Rs. ***4,476***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement of drain by RCC slab near house # 1690 in Ghousia Baloch colony U.C-19

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of RCC separating reinforcement from concrete cleaning & straightening (10/20) | 660 cft | 5445.00%  Cft | 35,937/= |
| 02 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 9.0 cwt | 5001.70 %  Cft | 45,015/= |
| 03 | RCC work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 424 cft | 337.00 cft | 1,42,888/= |
| **SUB TOTAL PART-A** | | | | **2,23,840/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Improvement of drain by RCC slab near house # 1690 in Ghousia Baloch colony U.C-19

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | P/F RCC pre cast slab 2” thick of required size and shape and racking out joints with CM curing etc complete as per direction of engineer incharge. | 840 sft | Offer Rate | Offer Rate |
| 05 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 32 hours | Offer Rate | Offer Rate |
| 06 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 06 days | Offer Rate | Offer Rate |
| 07 | Hiring of Tractor Trolly heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 160 Trip | Offer Rate | Offer Rate |
| 08 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 194 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/32**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair and improvement of drain and RCC slab near Qurban hotel U.C-19.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.1,83,177/- +O/R*

*BID SECURITY.* Rs. ***3,664***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/32**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.1,83,177/- +O/R*

Earnest Money Rs. ***3,664***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair and improvement of drain and RCC slab near Qurban hotel U.C-19.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of Rcc separating reinforcement from concrete cleaning & straightening (10/20) | 500 cft | 5445.00%  Cft | 27,225/= |
| 02 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 07.8 cwt | 5001.70 %  Cft | 39,013/= |
| 03 | Rcc work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 347 cft | 337.00 cft | 1,16,939/= |
| **SUB TOTAL PART-A** | | | | **1,83,177/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Repair and improvement of drain and RCC slab near Qurban hotel U.C-19.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | P/F RCC pre cast slab 2” thick of required size and shape and racking out joints with CM curing etc complete as per direction of engineer incharge. | 1000 sft | Offer Rate | Offer Rate |
| 05 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 32 hours | Offer Rate | Offer Rate |
| 06 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 06 days | Offer Rate | Offer Rate |
| 07 | Hiring of Tractor Toilly heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 160 Tripe | Offer Rate | Offer Rate |
| 08 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 210 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/33**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement construction of RCC slab on drain near Adeel lawn near old 1-D Bus stop U.C-26

Orangi Zone DMC west

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.3,59,769/- +O/R*

*BID SECURITY.* Rs. ***7,195***/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/33**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.3,59,769/- +O/R*

Earnest Money Rs. ***7,195***/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement construction of RCC slab on drain near Adeel lawn near old 1-D bus stop U.C-26

Orangi Zone DMC west

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of Rcc separating reinforcement from concrete cleaning & straightening (10/20) | 745 cft | 5445.00%  Cft | 40,565/= |
| 04 | P/L 1:4:8 CC using GSB 2” to 3” and i/c leveling compacting, curing etc complete without shuttering. | 300 cft | 11288.75.% cft | 33,866/= |
| 02 | Fabrication of mild steel reinforcement cement concrete i/c cutting binding laying in position making Joints and fastening i/c cost of bending wire also i/c removal rust from bars. (19/7-iib) | 6.446 cwt | 5001.70 %  Cft | 32,241/= |
| 03 | Rcc work i/c all labour materials except the cost of reinforcement and Its labor for bending binding which will be a paid separately. This ratio also i/c all kind froms, molds, lifting, shuttering, cutting, rendering & finishing expose surface i/c screening, & washing of shingle Ratio 1:2:4. (18/6-ai). | 356 cft | 337.00 cft | 1,19,972/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 12,500 Cft | 1065.00 % CFT | 1,33,125/= |
| **SUB TOTAL PART-A** | | | | **3,59,769/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of*** ***Contractor***

Subject: Improvement construction of RCC slab on drain near Adeel lawn near old 1-D bus stop U.C-26

Orangi Zone DMC west

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/F RCC pre cast slab 2” thick of required size and shape and racking out joints with CM curing etc complete as per direction of engineer incharge. | 960 sft | Offer Rate | Offer Rate |
| 06 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 250 Nos | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 40 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 07 days | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/34**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of sewerage system by RCC pipe 15” dia Main Line at Sher Muhammad

Mohallah In U.C-22 Orangi zone DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. Rs.8,18,727/- +O/R*

*BID SECURITY.* Rs. ***16,375.00 + O/R***

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/34**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *Rs.8,18,727/- +O/R*

Earnest Money Rs. ***16,375.00 + O/R***

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of sewerage system by RCC pipe 15” dia Main Line at Sher Muhammad Mohallah

In U.C-22 Orangi zone DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2044 Cft | 3327.50 %  Cft | 68,014/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1500 Cft | 4650.00 CFT | 6,975/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 5250 Cft | 10770.00 CFT | 56,543/- |
| 04 | P/L RCC pipe with Rubber ring pipe of class “A” and fixing in tranches i/c cutting, fitting and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 15” Dia, | 600 Rft | 436.00 Rft | 2,61,600/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 30 Nos. | 13064.00  Each | 3,91,920/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 30 Rft | 1540.00 Rft | -46,200/- |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 7500 Cft | 1065.00 % CFT | 79,875/= |
| **SUB TOTAL PART-A** | | | | **8,18,727/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of sewerage system by RCC pipe 15” dia Main Line at Sher Muhammad Mohallah

In U.C-22 Orangi zone DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 08 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3500 Cft | Offer Rate | Offer Rate |
| 09 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/35**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement / Repair of RCC pipe and Main Holes gali # 13 Amjad wali gali U.C-22

Orangi Zone DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,45,384.00* /= + O/R

*BID SECURITY.* Rs. ***16,908.00 + O/R***

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/35**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,45,384.00/=* + O/R

Earnest Money Rs. ***16,908.00 + O/R***

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement / Repair of RCC pipe and Main Holes gali # 13 Amjad wali gali U.C-22 Orangi

Zone DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2400 Cft | 3327.50 %  Cft | 79,860/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2300 cft | 2760.00 P.cft | 6,348/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 8000 Cft | 1065.00 % CFT | 85,200/= |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,45,384/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement / Repair of RCC pipe and Main Holes gali # 13 Amjad wali gali U.C-22 Orangi

Zone DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 3000 Cft | Offer Rate | Offer Rate |
| 10 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/36**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair and Maintenance of Road and filling of pot holes near Model Park in Orangi Zone

DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 2,64,753.00* /= + O/R

*BID SECURITY.* Rs. ***5,295.00 + O/R***

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/36**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *2,64,753.00* /= + O/R

Earnest Money Rs. ***5,295.00 + O/R***

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair and Maintenance of Road and filling of pot holes near Model Park in Orangi Zone

DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7500 Sft | 773.86%  Sft | 58,040/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 10750 Cft | 1437.00%0  Cft | 15,448/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14500 Cft | 1065.00 % CFT | 1,54,425/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 7000 Sft | 526.28%  Sft | 36,840/= |
| **SUB TOTAL PART-A** | | | | **2,64,753/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair and Maintenance of Road and filling of pot holes near Model Park in Orangi Zone

DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 900 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4050 Cft | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 02 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/37**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /09/ /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing and Maintenance of pot holes near ALLAH wala College in Orangi Zone DMC west.

**BILL OF QUANTITIES**

*ESTIMATED COST. RS. 2,62,121.00* /= + O/R

*BID SECURITY.* Rs. ***5,242.00 + O/R***

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/37**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *2,62,121.00* /= + O/R

Earnest Money Rs. ***5,242.00 + O/R***

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing and Maintenance of pot holes near ALLAH wala College in Orangi Zone DMC west.

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7500 Sft | 773.86%  Sft | 58,040/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 10750 Cft | 1437.00%0  Cft | 15,448/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, building rubbish i/c loading unloading stacking at site. All lide & lift (Ch 1/1-1) | 14500 Cft | 1065.00 % CFT | 1,54,425/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6500 Sft | 526.28%  Sft | 34,208/= |
| **SUB TOTAL PART-A** | | | | **2,62,121/= + O/R** |

***Signature of Contractor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing and Maintenance of pot holes near ALLAH wala College in Orangi Zone DMC west.

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 900 Cft | Offer Rate | Offer Rate |
| 06 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4050 Cft | Offer Rate | Offer Rate |
| 07 | Hiring of excavator for desalting and cleaning of nallah long boom i/c POL ( For 8 hours Per Day) | 80 hours | Offer Rate | Offer Rate |
| 08 | Hiring of Tractor blade heavy Duty for cleaning of garbage, street or road side earth etc with POL ( For 8 hours Per Day) | 08 Nos | Offer Rate | Offer Rate |
| 09 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours) | 150 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 9/38**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 09 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Reparing / Improvement cc street & Sewerage line near SNS Coaching Center Yaseen watch House, Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,30,000.00* /= + O/R

*BID SECURITY.* Rs. *16,600*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 9/38**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,30,000.00/=* + O/R

Earnest Money Rs. *16,600*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Reparing / Improvement cc street & Sewerage line near SNS Coaching Center Yaseen watch House, Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2643 Cft | 3327.50 %  Cft | 87,946/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 2800 Cft | 10770.00 CFT | 30,156/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 400 Rft | 367.00 Rft | 1,46,800/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 18 Nos. | 13064.00  Each | 2,35,152/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 35.995 Rft | 1540.00 Rft | -55,432/- |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 8693 Cft | 1065.00 % CFT | 92,580/= |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6500 Sft | 526.28%  Sft | 34,208/= |
| 08 | P/L 2” thick Topping c.c (1.2.4) i/c surface finishing & dividing into panelsa (ch-8/42/16-c). | 6500 sft | 3275.50 % sft | 2,12,908/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
| **SUB TOTAL PART-A** | | | | **8,30,000/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Reparing / Improvement cc street & Sewerage line near SNS Coaching Center Yaseen watch House, Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2000 Cft | Offer Rate | Offer Rate |
| 11 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2000 Cft | Offer Rate | Offer Rate |
| 12 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 05 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***