|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO CHIEF SECRETARY HOUSE KARACHI**  **(MAIN LBUILDING & ANNEXE BUILDING COLOURING PAINTING FRENCH POLISHING & WOOD WORK )** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  |  |  |
| 1. | Nyloon wire gauge 144 mesh per square inch fixed to chowkats. (SI.63-B/P-66) | 304.40 Sft. | 74/94 | %Sft. | 22812/- |
|  | Rupees. Seventy Four. And. Ninety four.. Paisa | | | | |
| 2. | P/F GI expanded metal 1/8-20 gauge fixed to chowkats. (66-b P-66). | 304.40 Sft. | 68/13 | PSft | 20739/- |
|  | Rupees. Sixty Eight. And. Thirteen. Paisa | | | | |
| 3. | Providing and laying 1” thick topping cement concrete ( 1:2:4 ) including Surface finishing and dividing into panels: ( c ) 2” thick.( SI.16 ( c ) / P-42 ). | 288.00 Sft. | 3275/50 | %Sft | 9443/- |
|  | Rupees. Three thousand Two hundred Seventy Five. And. Fifty.. Paisa | | | | |
|  |  | **Total Rs** | | | **52984/-** |
|  | **Above / Below Rs.** | | | |  |
|  | **Total Rs “A”** | | | |  |
|  | **NON-SCHEDULE ITEMS PART-“B”** |  |  |  |  |
| 1 | Preparing old surface & painting with quality matt (Berger / Nelson) make in/c filling of crack & joints & after this rubbing with sand paper & rubbing brick with fine finishing in/c all cost of labour, material, cartage & wastage etc as directed by the Engineer Incharge. | 20330.94 Sft |  | PSft |  |
| 2 | P/L step by step French polish of doors windows, ventilators, cupboard, cabinet, floor stair & Jeffery work etc in/c preparing surface with zero No. sand paper & then surface polishing using Indian Lakh dana, sprit, thinner, pigment, ICI laquar, hardner ICI sealer, tarpin oil as per required etc polishing as satisfaction and approval of chief Secretary House Authority etc complete. | 7081.95  Sft |  | PSft |  |
| 3 | P/F wooden Almirah with wooden frame work -1/2”x1” as required size & thickness in/c making front shutter with lamination sheet 3/4” thick & back shelve in/c side walls with 18” deep boxes P/F wooden leaping or Gola around shutter or making gola by router in approved shape & design the cost in/c necessary hinges, catchers, handles, sliding channel, draws lock, nails, screws etc in/c necessary tools plants to be used in making as directed by the Engineer Incharge. | 105.00  Sft. |  | P/Sft. |  |
| 4 | Rubbing and chemical polishing of marble floor with machine in/c fine finishing etc complete. | 1992.92  Sft |  | P/Sft |  |
| 5 | S/F 30 Gallon Geyser Singer or approved company with 10 to 12 gauge inside tank, selector switch, thermostat in all respect fitted with all UPVC / CPVC fittings in/c installed on cement concrete plate form to required size &height with 1:3:6 finishing curing etc complete. | 01 No |  | Each. |  |
|  |  | **Total Part “B” Rs.** | | |  |
|  |  | **Total Part-“A” Rs.** | | |  |
|  |  | **G: Total Part ( A+B ) Rs.** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-I,**  **KARACHI.** |