S. No: 30

BILL OF QUANTITES

(A) Description and rate of items based on composite schedule of rates.

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GBHS BAHAR LARIK TALUKA KINGRI DISTRICT KHAIRPUR SEMIS CODE: 415040381 (Lev: Block & C/Wall)**

S;NO; DESCRIPTION. QTY; RATE. UNTI. AMOUNT.

1. Excavation in foundation of building bridges and other str:with excavated earth

Lead upto 5”ft.(SI:NO:18-b P-4)

1590.0 Rs:3176/25 %0cft. 5050/-

2. Cement concerte brick or stone ballast 1 ½” to 2” guage ratio 1;5;10.(SI:NO:4-c P-14)

518.0 Rs:8694/95 %cft. 45040/-

3. Pacca brick work in foundation and plinth ratio 1;6.(SI:NO:4-a P-20)

2102.0 Rs;11948/3 %cft. 251154/-

4. R.C.C. work i/c all labour and material except the cost of steel and its labour for bending

And binding which will be paid sepratelly.This rate also i/c all kinds of moulds lifting

Shuttering curring rendering and finshing the exposed surface i/c secreening and washing

Of shingle 1;2;4.(SI:NO:6-a P-16)

477.0 Rs:337/- P/sft. 160749/-

5. Fabrication of mild steel reinforcement for c.c.i/c cutting bending and binding i/c rust removal

From bars.(SI:NO:8-d P-20)

21.294 Rs:5001/70 P/cwt. 106506/-

7. Pacca brick work in other than building ratio 1;6.(SI:NO:7-e P-22)

3275.0 Rs:12346/65 %cft. 404353/-

8. Cement plaster ½”thick upto 20” height ratio 1;6.(SI:NO:13-b P-51)

7125.0 Rs:2206/60 %Sft. 157220/-

9. Cement plaster 3/8” thick upto 20” height ratio 1;4(SI:NO:11-a P-51).

7125.0 Rs:2197/52 %sft. 156573/-

10. Cement pointing stricking o f joints on walls ratio 1;2.(SI:NO: P- )

4000.0 Rs:1287/44 %sft. 51498/-

11. M/F steel grated door 1/16” thick i/c angle iron frame with locking arrangements.(SI:NO:24 p-91)

126.0 Rs:726/72 %sft 91567/-

12. P/L “Halla” or patterns tiles glazed 8”x8” on floor walls in required of specified jointed in

White cement sand motor etc complete.(SI:NO:62 P-47)

32.0 Rs:34520/31 %sft. 32481/-

13. S/F broden glass on courtyard walls i/c 1;3;6 cement concerte coping (SI:NO:61 P-104)

500.0 RS:70/40 %sft. 35200/-

14. Colour wash two coats.(SI:NO:23 P-53)

11125.0 Rs:859/90 %sft. 95664/-

15. Painting guard bars iron gated i/c any type (SI:NO:14-d P-68)

252.0 Rs:977/40 %sft. 2463/-

\_\_\_\_\_\_\_\_\_\_\_

Total Rs: 15,63037/-