***SCHEDULE OF QUANTITIES***

***WORK No: 03***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,79,345/- Earnest Money Rs: 19,587/-/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Construction of R.C.C Work for Dus Bin in Different point Jurisdiction of UC-33***

***Baldia Zone DMC (West).***

|  |
| --- |
|  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Excavation for Foundation of Building Bridges and other structure i/c dag bolling dressing refilling ground structure with excavated earth watering and rounding lead up to 5feet.* | *1764* | *3176.25* | *%0Cft* | *5603/-* |
| *2.* | *Stone Pitching for top Laying only (1.3 to 1.5) thick in bed.* | *378* | *1996* | *%Cft* | *7545/-* |
| *3.* | *Cement concrete brick or stone ballast 1 ½ “to 2” gauge 1:4:8 ratio.* | *924* | *9416.28* | *%Cft* | *87006/-* |
| *4.* | *RCC Work in roof slob beams columns rofts, lintels and other structural members laid in situ or precast laid in position complete in all respects. Ratio (1:2:4) 90 lbs cement 2 Cft sand 2 Cft Shingle 1/8” to 1/4 “gauge.* | *1470* | *337* | *P-Cft* | *495390/-* |
| *5.* | *Fabrication at mold steel reinforcement cement concrete i/c cutting binding laying in position making joints and fastening i/c cast of bending wire also i/c removal rust from bars,* | *65.62* | *500* | *P-Cast* | *328212/-* |
| *6.* | *Providing of mild and laying 3” thick topping and concrete (1:2:4) including surface finishing and dividing into panels.* | *1260* | *4411.82* | *%Cft* | *55589/-* |
| ***Total Estimated Cost*** | | | | | ***9,79,345.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*