**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/01**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation / Repairing of RCC pipe & in ward # 01, near Madina Masjid & saddiqa Masjid, in U.C # 12, Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,23,327.00* /= + O/R

*BID SECURITY.* Rs. 16,465/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/01**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,23,327.00/=* + O/R

Earnest Money Rs. 16,465/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation / Repairing of RCC pipe & in ward # 01, near Madina Masjid & saddiqa Masjid, in

U.C # 12, Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | (-)80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3018 cft | 2760.00 P.cft | 8,330/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2627 Cft | 1065.00 % CFT | 27,978/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 66 Nos. | 913.63  Each | 60,300/= |
| **SUB TOTAL PART-A** | | | | **8,23,327/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation / Repairing of RCC pipe & in ward # 01, near Madina Masjid & saddiqa Masjid, in U.C # 12, Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 45 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/02**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair of sewerage System in sector 1-A, & 7-A, near M.N.A office, in U.C 13, Orangi Zone, DMC

(West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,24,240.00* /= + O/R

*BID SECURITY.* Rs. 16,485/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/02**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,24,240.00/=* + O/R

Earnest Money Rs. 16,485/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair of sewerage System in sector 1-A, & 7-A, near M.N.A office, in U.C 13, Orangi Zone, DMC

(West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | (-)80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3018 cft | 2760.00 P.cft | 8,330/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2627 Cft | 1065.00 % CFT | 27,978/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 67 Nos. | 913.63  Each | 61,213/= |
| **SUB TOTAL PART-A** | | | | **8,24,240/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair of sewerage System in sector 1-A, & 7-A, near M.N.A office, in U.C 13, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 45 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/03**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Construction of Sewerage Line near Liaquat Chowk in U.C # 16, Orangi Zone.

DMC (W)

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,12,904*.00* /= + O/R

*BID SECURITY.* Rs. 14,258/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/03**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,12,904*.00/=* + O/R

Earnest Money Rs. 14,258/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Construction of Sewerage Line near Liaquat Chowk in U.C # 16, Orangi Zone.

DMC (W)

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 750 Cft | 1306.80 %  Cft | 9,801/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1750 Cft | 4650.00 CFT | 8,138/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 2450 Cft | 10770.00 CFT | 26,386/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 300 Rft  400 Rft | 206.00 Rft  367.00 Rft | 61,800/-  1,46,800/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 45 Rft | 1540.00 Rft | -69,300/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3341 cft | 2760.00 P.cft | 9,221/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 1609 Cft | 1065.00 % CFT | 17,136/= |
|  |  |  |  |  |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
|  |  |  |  |  |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **7,12,904/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Construction of Sewerage Line near Liaquat Chowk in U.C # 16, Orangi Zone.

DMC (W)

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 85 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/04**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: P/L RCC PIPE & Winching of sewerage line in yousuf Goth, in U.C # 38 Surjai Town,

DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,26,003.00* /= + O/R

*BID SECURITY.* Rs. 16,520/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/04**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,26,003.00/=* + O/R

Earnest Money Rs. 16,520/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: P/L RCC PIPE & Winching of sewerage line in yousuf Goth, in U.C # 38 Surjai Town,DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 400 Cft | 1306.80 % Cft | 5,227/- |
| 02 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 600 Cft | 3327.50 % Cft | 19,965/- |
| 03 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 400 Cft | 4650.00 CFT | 1,860/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 800 Cft | 10770.00 CFT | 8,616/- |
| 05 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 200 Rft | 367.00 Rft | 73,400/- |
| 06 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 12 Nos. | 13064.00  Each | 1,56,768/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 8 Rft | 1540.00 Rft | (-)1,522/- |
| 08 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 1467 cft | 2760.00 P.cft | 40,489/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 1100 Cft | 1065.00 % CFT | 11,715/= |
| 11 | Cleaning inside sewerage lines completely restoring original silt free space /diameter of pipe lines-by labour and equipment Mechanically / electrically driven). Including accessories like pulley’s Steel rope, bucket and draggers sizing from 6” to 18” dia. Their” to an fro” pulling action ( No of passes shall be as many as required) would be taken in two phases (First phase entire length from down stream to up stream) bringing down peak hours sewerage to flow in side pipe line (as free flow) and in second phase from up stream to down stream of entire length ensuring no silt is observed in buckets (6” dia to 18” dia) except only sewerage water and finally passing a steel ball of dia 12” lesser that the diameter oif pipe but not exceeding 48” dia ball even for larger dia pipe to ensure perfect cleaning. The job includes all the hire / cost of equipment and accessories of above winching machine / devices along with / engines with winching drum set having, steel) rope pully mounted over it, steel bucket from 6” to 18” dia hooks and other protection likes Safety barriers, traffic signs, traffic cones ensuring no damages to pipe along with ensuring safety to labour and other public property / lives and removal of silts / solid during desalting and removal of silts / solid during desalting and clearance of site etc. complete as per full satisfaction of site engineer.  i). 12 “ dia  iii). 18 “ dia  v). 24 “ dia | 3000 Rft  1000 Rft  665 Rft | 80.50 P.Rft  128.80 P.Rft  209.30 P.Rft | 2,41,500/-  1,28,800/-  1,39,185/- |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,26,003/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: P/L RCC PIPE & Winching of sewerage line in yousuf Goth, in U.C # 38 Surjai Town,DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 20 Nos | Offer Rate | Offer Rate |
| 12 | Hiring of Labour for cleaning of Nallaha. (For 8 Hours ). | 08 Labour  10 Days | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/05**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Sewerage Line and Broken Main Holes in Bangla Bazar in U.C # 17, Orangi Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,33,130.00* /= + O/R

*BID SECURITY.* Rs. 16,663/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/05**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,33,130.00/=* + O/R

Earnest Money Rs. 16,663/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Sewerage Line and Broken Main Holes in Bangla Bazar in U.C # 17, Orangi Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | (-)80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3145 cft | 2760.00 P.cft | 8,680/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3000 Cft | 1065.00 % CFT | 31,950/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 72 Nos. | 913.63  Each | 65,781/= |
| **SUB TOTAL PART-A** | | | | **8,33,130/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of Sewerage Line and Broken Main Holes in Bangla Bazar in U.C # 17, Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 40 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/06**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repairing of Broking Main Hole and Cover in ward # 1,2,3, & 4, in U.C -18, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *5,14,910.00* /= + O/R

*BID SECURITY.* Rs. 10,298/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/06**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,14,910.00/=* + O/R

Earnest Money Rs. 10,298/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repairing of Broking Main Hole and Cover in ward # 1,2,3,& 4, in U.C -18, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1005 Cft | 3327.50 %  Cft | 33,441/= |
| 02 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 20 Nos. | 13064.00  Each | 2,61,280/- |
| 03 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 35 Rft | 1540.00 Rft | (-) 53,900/- |
| 04 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 300 Nos. | 913.63  Each | 2,74,089/= |
| **SUB TOTAL PART-A** | | | | **5,14,910/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repairing of Broking Main Hole and Cover in ward # 1,2,3,& 4, in U.C -18, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 155 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/07**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Repair & Construction of Sewerage Line near Baba Willayat Ward # 03, in U.C # 19, Orangi

Zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *7.40,016.00* /= + O/R

*BID SECURITY.* Rs. 14,800/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/07**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7.40,016.00/=* + O/R

Earnest Money Rs. 14,800/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Repair & Construction of Sewerage Line near Baba Willayat Ward # 03, in U.C # 19, Orangi

Zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1020 Cft | 1306.80 %  Cft | 13,329/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 1750 Cft | 4650.00 CFT | 8,138/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 2450 Cft | 10770.00 CFT | 26,386/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 400 Rft  400 Rft | 206.00 Rft  367.00 Rft | 82,400/-  1,46,800/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 45 Rft | 1540.00 Rft | -69,300/- |
| 07 | P/L 1.3.6 CC using GSB ¾” and down gauge i/c consolidation, curing etc complete without shutring. | 72 Rft | 12595.00 Rft | 90,684/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3341 cft | 2760.00 P.cft | 9,221/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 1889 Cft | 1065.00 % CFT | 20,119/= |
|  |  |  |  |  |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1)21” Dia | 50 Nos. | 913.63  Each | 45,682/= |
|  |  |  |  |  |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **7,40,016/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Repair & Construction of Sewerage Line near Baba Willayat Ward # 03, in U.C # 19, Orangi Zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 75 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/08**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11/2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,33,130.00* /= + O/R

*BID SECURITY.* Rs. 16,663/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/08**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,30,909.00/=* + O/R

Earnest Money Rs. 16,663/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | (-)80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3145 cft | 2760.00 P.cft | 8,680/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 3000 Cft | 1065.00 % CFT | 31,950/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 72 Nos. | 913.63  Each | 65,781/= |
| **SUB TOTAL PART-A** | | | | **8,33,130/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 40 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/08**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,30,909.00* /= + O/R

*BID SECURITY.* Rs. 16,618/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/08**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,30,909.00/=* + O/R

Earnest Money Rs. 16,618/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 36 Nos. | 13064.00  Each | 4,70,304/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | - 80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3018 cft | 2760.00 P.cft | 8,330/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2627 Cft | 1065.00 % CFT | 27,978/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 60 Nos. | 913.63  Each | 54,818/= |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,30,909/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of R.C.C pipe & main Hole near Ibrahim Ali Bhai School in U.C # 20, Orangi zone DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 45 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/09**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE NIT #/ 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation & repairing of cc street in Lal Shabaz Nagar and other places, in U.C # 26, Orangi

Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *5,28,559.00*/= + O/R

*BID SECURITY.* Rs. 10,571/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/09**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,28,559.00*/= + O/R

Earnest Money Rs. 10,571/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation & repairing of cc street in Lal Shabaz Nagar and other places, in U.C # 26, Orangi

Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1752 Cft | 3327.50 % Cft | 58,289/= |
| 02 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 2475 Cft | 1306.80 % Cft | 32,343/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 4227 Cft | 1065.00 % CFT | 45,015/= |
| 05 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 3570 Cft | 1437.00 % Cft | 5,130/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 1020 Sft | 526.28%  Sft | 53,681/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10200 Sft | 3275.50 % Sft | 3,34,101/= |
| **SUB TOTAL PART-A** | | | | **5,28,559/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Rehabilitation & repairing of cc street in Lal Shabaz Nagar and other places, in U.C # 26, Orangi

Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | Supplying and Fixing Imported Earth with in the radious of 5 miles including digging, loading, unloading, all lead and lift leveling, water compaction etc complete (A/Rate). | 4556 P.cft | Offer Rate | Offer Rate |
| 07 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2958 Cft | Offer Rate | Offer Rate |
| 08 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3825 P. Cft | Offer Rate | Offer Rate |
| 10 | Extra for using (S.R Cement ) Sulphate resistant cement in place of ordinary Portland cement (A/Rate). | 295 P.Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/10**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Construction of Rcc pipe at Jinnaha Colony, near Baloch Goth in U.C # 27, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,20,586.00* /= + O/R

*BID SECURITY.* Rs. 16,412/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/10**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,20,586.00/=* + O/R

Earnest Money Rs. 16,412/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Construction of Rcc pipe at Jinnaha Colony, near Baloch Goth in U.C # 27, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 1706 Cft | 3327.50 %  Cft | 56,767/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3938 Cft | 4650.00 CFT | 18,312/- |
| 03 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” Dia, 15 “ Dia. | 750 Rft | 367.00 Rft | 2,75,250/- |
| 04 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52.5 Rft | 1540.00 Rft | - 80,850/- |
| 06 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 3018 cft | 2760.00 P.cft | 8,330/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 2627 Cft | 1065.00 % CFT | 27,978/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 63 Nos. | 913.63  Each | 57,559/= |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,20,586/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Construction of Rcc pipe at Jinnaha Colony, near Baloch Goth in U.C # 27, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 09 | P/F RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 47 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/11**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE NIT #/ 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Maintenance and Construction of CC Street in 14/G, Ward # 04 in U.C # 28, Orangi Zone,

DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *5,39,947.00*/= + O/R

*BID SECURITY.* Rs. 10,799/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/11**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,39,947.00*/= + O/R

Earnest Money Rs. 10,799/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Maintenance and Construction of CC Street in 14/G, Ward # 04 in U.C # 28, Orangi Zone,

DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2520 Cft | 3327.50 % Cft | 83,853/= |
| 02 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 2138 Cft | 1306.80 % Cft | 27,933/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 4658 Cft | 1065.00 % CFT | 49,602/= |
| 05 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 4165 Cft | 1437.00 % Cft | 5,985/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 9800 Sft | 526.28%  Sft | 51,575/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9800 Sft | 3275.50 % Sft | 3,20,999/= |
| **SUB TOTAL PART-A** | | | | **5,39,947/= + O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***Subject: Maintenance and Construction of CC Street in 14/G, Ward # 04 in U.C # 28, Orangi Zone,

DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 04 | Supplying and Fixing Imported Earth with in the radious of 5 miles including digging, loading, unloading, all lead and lift leveling, water compaction etc complete (A/Rate). | 3283 P.cft | Offer Rate | Offer Rate |
| 07 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2848 Cft | Offer Rate | Offer Rate |
| 08 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3675 P. Cft | Offer Rate | Offer Rate |
| 10 | Extra for using (S.R Cement ) Sulphate resistant cement in place of ordinary Portland cement (A/Rate). | 283 P.Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/12**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Improvement repairing of Broken C.C & pipe and Main Hole Paradise School at Ammazai

Mohallah, in U.C-21, Orangi Zone, D.M.C (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,58,987.00* /= + O/R

*BID SECURITY.* Rs. 17,179/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/12**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,58,987.00/=* + O/R

Earnest Money Rs. 17,179/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Improvement repairing of Broken C.C & pipe and Main Hole Paradise School at Ammazai

Mohallah, in U.C-21, Orangi Zone, D.M.C (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2327 Cft | 3327.50 %  Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 30 Nos. | 913.63  Each | 28,100/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6891 Cft | 1065.00 % CFT | 73,389/= |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,58,987/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Improvement repairing of Broken C.C & pipe and Main Hole Paradise School at Ammazai

Mohallah, in U.C-21, Orangi Zone, D.M.C (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2000 Cft | Offer Rate | Offer Rate |
| 11 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours). | 30 Nos | Offer Rate | Offer Rate |
| 12 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 11/13**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT / 11 /2017. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2017.

Subject: Rehabilitation of sewerage System i/c Main Holes near House # 1720 , Haryana Colony

and other Area, in U.C # 21, Orangi Zone, DMC (West).

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* *8,54,900.00* /= + O/R

*BID SECURITY.* Rs. 17,098/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 11/13**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,54,900.00/=* + O/R

Earnest Money Rs. 17,098/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: Rehabilitation of sewerage System i/c Main Holes near House # 1720 , Haryana Colony

and other Area, in U.C # 21, Orangi Zone, DMC (West).

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete plain flooring. (10/19-b). CC 1.2.4. | 2327 Cft | 3327.50 %  Cft | 77,431/= |
| 02 | Excavation for pipe line in trenches & pits in all kinds of soils of murum i/c trimming & dressing sides to true alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3/P-62/6). | 3000 Cft | 4650.00 CFT | 13,950/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (PHE, Ch-3 /P-62/6). | 3281 Cft | 10770.00 CFT | 35,336/- |
| 04 | P/L RCC pipe with Rubber ring i/c cartage loading un loading site of work fixing in tranches and Jointing with rubber ring etc complete. (Ch-2/P-18/B-2) 12” | 750 Rft | 367.00 Rft | 2,75,250/- |
| 05 | Construction of manholes 4” dia inside i/c with RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff upto one chain etc complete. (app/rates). | 35 Nos. | 13064.00  Each | 4,57,240/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70 Rft | 1540.00 Rft | -1,07,800/- |
| 07 | Refilling the excavated stuff in tranches 6” thick layer including watering ramming to full compaction etc complete. (Ch-2/P-77/24). | 2207 cft | 2760.00 P.cft | 6,091/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 23 Nos. | 913.63  Each | 24,013/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide & lift ( Lead upto 15 Miles etc ) (Ch 1/P-1/1). | 6891 Cft | 1065.00 % CFT | 73,389/= |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **8,54,900/=O/R** |

***Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

Subject: Rehabilitation of sewerage System i/c Main Holes near House # 1720 , Haryana Colony

and other Area, in U.C # 21, Orangi Zone, DMC (West).

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 10 | S/F Imported earth with in a reduce of 5 miles i/c digging, loading, unloading, all lead and lift leveling and water compaction etc complete. | 2000 Cft | Offer Rate | Offer Rate |
| 11 | Hiring of Private labour for cleaning of Nallah ( by Afghani or Bajorri for 8 hours). | 30 Nos | Offer Rate | Offer Rate |
| 12 | P/F Per coasted RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. \_\_\_\_ Rupees \_\_\_\_\_\_\_\_\_\_\_\_

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***