***SCHEDULE OF QUANTITIES***

***WORK No: 03***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,98,210/- Earnest Money Rs: 19,964/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Providing & Laying 2” thickness C.C Flooring at Street No.36, 56, 22 Ward No.3,***

***Sector 5-G Saeedabad in UC-30 DMC (West) Baldia Zone.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

|  |  |
| --- | --- |
|  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Dismantling Cement concrete plain 1:4:8.* | *725* | *1663.75* | *%Cft* | *12062/-* |
| *2.* | *Earth work Excavator undressed lead up to a single throws of Kassi Phawrah or Shovel.* | *6525* | *1361.25* | *%Cft* | *8882/-* |
| *3.* | *P/L cement concrete brick or stone 6 ballast 1 ½” to 2” gauge 1:4:8.* | *4785* | *9416.28* | *% Sft* | *450569/-* |
| *4.* | *P/L 2” thick topping cement concrete 1:2:4 i/c surface finishing and diving into panels etc complete.* | *14500* | *3275.50* | *% Sft* | *474947/-* |
| *5.* | *Carriage of 100 cft tons of all kinds’ material like Cole bricks i/c loading unloading 10 miles.* | *7250* | *595.80* | *% Cft* | *43195/-* |
| *6.* | *P/F C-I M/H Cover frame i/c cast of 1 kg material etc.* | *35* | *140* | *P-Kg* | *4900/-* |
| *7.* | *M/S R.C.C M/H cover cast silo 1:2:4 C.C. 3 Inch deep in center reinforced with 3/8” dia M.S Bar welded on M.S Sheet i/c curing transportation. 21”Dia.* | *04* | *913.63* | *Each* | *3655/-* |
| ***Total Estimated Cost*** | | | | | ***9,98,210.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*