***SCHEDULE OF QUANTITIES***

***WORK No: 05***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,85,213/- Earnest Money Rs: 19,705/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Improvement of C.C Nallah and R.C.C Culvert in Abidabad Town Near Graveyard***

***Abidabad in UC-31 Baldia Zone, DMC (West).***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | | ***AMOUNT*** |
| *1.* | *Dismantling cement rain for Separating reinforced cement form concrete cleaning and straightening 1ft same.* | *112* | *5445* | *%Cft* | | *6098/-* |
| *2.* | *Dismantling cement concrete plain 1:2:4.* | *1120* | *3327.50* | *%Cft* | | *37268/-* |
| *3.* | *Excavation for pipe line in trenches, and pits in all kind of soil of Murum Shape Leveling of beds of trenches to correct lever & grade, surplus earth within a one chain as directed by Eng incharge.* | *3920* | *4650* | *%0Cft* | | *18228/-* |
| *4.* | *Stone Piloting for top Layer only (1.3 to 1.5) thick.* | *980* | *1996* | *%Cft* | | *19561/-* |
| *5.* | *P/L Cement concrete brick or stone ballast 1 ½ “to 2” gauge ratio 1:4:8.* | *490* | *9416.28* | *%Cft* | | *46140/-* |
| *6.* | *Erection and removal of centering for R.C.C. or plain cement concrete works of Deodar Wood (2nd class).* | *2300* | *3127.41* | *%Cft* | | *71930/-* |
| *7.* | *P/L 1:2:4 CC Situ i/c placing compacting finishing and coring complete including screening and wishing at stone aggregate wild out shuttering etc.* | *1150* | *14429.25* | *%Cft* | | *165936/-* |
| *8.* | *P/L RCC Work i/c all Labour material the cast of range its labour bending which will be a paid Separately i/c all kind from moulds lifting shuttering washing finishing single R.C.C work roof slab blame lintel columns other structure member laid a situ or pre-cast in position in all respect.* | *547* | *337* | *P-Cft* | | *184339/-* |
| *9.* | *Fabrication at mold steel reinforcement cement concrete i/c cutting binding laying in position making joints and fastening i/c cast of bending wire also i/c removal rust from bars,* | *2441* | *5001.73* | *P-Cwt* | | *122092/-* |
| *10.* | *Carriage of 100-Cft tons of all kind material like Cole brick i/c loading unloading 10 mile.* | *5152* | *1065.04* | *%Cft* | | *54871/-* |
| *11.* | *Hiring of Skilled Labour for cleaning of Nallah (Afghani Bajorri) for 8-Hour* | 225 | *1150* | *P-Labour* | | *258750/-* |
| ***Total Estimated Cost*** | | | | | ***9,85,213.00*** | |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*