**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 01**

**SUBJECT: - CONST / IMP OF CC FLOORING AT AGHA KHAN FLAT KAREEM**

**NAGAR IN SECTOR IV METROVILL IN UC-04 SITE ZONE DMC (WEST)**

**E/Cost: 9,98,920/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 6525/Cft 3327.50%Cft

2. Cartage of 100 Cft 5 tons all materials like stone

aggregate spwals lime surkhi BG rail fasting points

crossing bridge guders pipe sheet M/S Brass sheets

1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft

timber 100 mould fuel wood by trenches owned by the

contractor withing 10 miles etc comp: 5220/Cft 902.20%Cft

3. CC plain i/c placing compacting finishing and curing

complete i/c screening and washing of stone aggregate

without shuttering ratio 1:4:8 3263/Cft 9416.28%Cft

4. P/L 2" thick toping cement concrete 1:2:4 i/c surface

finishing and dividing into panels eto completed. 13050/Sft3275.50%Sft

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 02**

**SUBJECT: - CONST / IMP OF SEWERAGE LINE I/C CC FLOORING FROM RUSTOM**

**KHAN AT SECTOR 5 METROVILL IN UC-04 SITE ZONE DMC (WEST)**

**E/Cost: 9,49,810/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 2805/Cft 3327.50%Cft

2. Excavation of pipe line trenches pipe all kind of soil

murum i/c trimming dressing leveling beds trenches

correct level and graded cutting joints holes disposal

of surplus earth with in 1 chains as directed by the

Engg: Inch: P. fence guard lights flags temporary

crossing non vehicler traffic where ever req: a lift up

to 5 ft & lead up to 1 chain. 4500/Cft 4650 %0 Cft

3. P. Rcc pipe ASTM class class ‘C’ 76-62 T/C 76-70

class II wall ‘B’ and fixing in trenches i/c cutting

fitting jointing with rubber ring i/c testing with water

to specified pressure 9″ & 12″dia pipe. 400/Rft 412/P.Rft

4. Const of Main Holes 4 inside with Rcc covers 21″dia

3×¾ with flat iron frame 5ft depth 1:2:4 in laying CC

cost in situ 9″ thick wall and disposal of surplus stuff

etc comp: 16/Nos. 13028 / Each

5. Add or deduct for depth of man holes above or beyond

5 ft (RA). 16/Rft 2245.55/P.Rft

6. Refilling the excavated stuff in trenches 6″ thick layer i/c

watering ramming to full compaction etc comp: 4050/Cft 2760.0/%0Cft

7. Cartage of 100 Cft 5 tons all materials like stone aggregate

spwals lime surkhi BG rail fasting points crossing bridge

guders pipe sheet M/S Brass sheets 1000 trenches 10×5×3"  
1000 tiles 12×6×2" 150 cft timber 100 mould fuel wood

by trenches owned by the contractor withing 10 miles

etc comp: 2244/Cft 902.20%Cft

8. CC plain i/c placing compacting finishing and curing

complete i/c screening and washing of stone aggregate

without shuttering ratio 1:4:8 2125/Cft 9416.28%Cft

9. P/L 2" thick toping cement concrete 1:2:4 i/c surface

finishing and dividing into panels eto completed. 8140/Sft3275.50%Sft

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**1I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 03**

**SUBJECT: - CONST / IMP OF CC FLOORING FROM H. NO E-107 TO E-78 AND**

**PROFFESAR KHURRAM AT SECTOR 2 IN UC-04 SITE ZONE DMC**

**(WEST)**

**E/Cost: 9,97,000/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 4998/Cft 3327.50%Cft

2. Cartage of 100 Cft 5 tons all materials like stone

aggregate spwals lime surkhi BG rail fasting points

crossing bridge guders pipe sheet M/S Brass sheets

1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft

timber 100 mould fuel wood by trenches owned by the

contractor withing 10 miles etc comp: 3998/Cft 902.20%Cft

3. CC plain i/c placing compacting finishing and curing

complete i/c screening and washing of stone aggregate

without shuttering ratio 1:4:8 3900/Cft 9416.28%Cft

4. P/L 2" thick toping cement concrete 1:2:4 i/c surface

finishing and dividing into panels eto completed. 13600/Sft3275.50%Sft

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 04**

**SUBJECT: - CONST OF CC FLOORING FROM HAJI JANDAD HOUSE TO**

**METROVILL HOSPITAL AT SECTOR IV METROVILL IN UC-04**

**SITE ZONE DMC (WEST)**

**E/Cost: 9,98,000/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 2079/Cft 3327.50%Cft

2. Excavation of pipe line trenches pipe all kind of soil

murum i/c trimming dressing leveling beds trenches

correct level and graded cutting joints holes disposal

of surplus earth with in 1 chains as directed by the

Engg: Inch: P. fence guard lights flags temporary

crossing non vehicler traffic where ever req: a lift up

to 5 ft & lead up to 1 chain. 7875/Cft 4650 %0 Cft

3. P. Rcc pipe ASTM class class ‘C’ 76-62 T/C 76-70

class II wall ‘B’ and fixing in trenches i/c cutting

fitting jointing with rubber ring i/c testing with water

to specified pressure 9″ & 12″dia pipe. 700/Rft 412/P.Rft

4. Const of Main Holes 4 inside with Rcc covers 21″dia

3×¾ with flat iron frame 5ft depth 1:2:4 in laying CC

cost in situ 9″ thick wall and disposal of surplus stuff

etc comp: 28/Nos. 13028 / Each

5. Add or deduct for depth of man holes above or beyond

5 ft (RA). 28/Rft 2245.55/P.Rft

6. Refilling the excavated stuff in trenches 6″ thick layer i/c

watering ramming to full compaction etc comp: 7085/Cft 2760.0/%0Cft

7. Cartage of 100 Cft 5 tons all materials like stone aggregate

spwals lime surkhi BG rail fasting points crossing bridge

guders pipe sheet M/S Brass sheets 1000 trenches 10×5×3"  
1000 tiles 12×6×2" 150 cft timber 100 mould fuel wood

by trenches owned by the contractor withing 10 miles

etc comp: 1663/Cft 902.20%Cft

8. CC plain i/c placing compacting finishing and curing

complete i/c screening and washing of stone aggregate

without shuttering ratio 1:4:8 1238/Cft 9416.28%Cft

9. P/L 2" thick toping cement concrete 1:2:4 i/c surface

finishing and dividing into panels eto completed. 4950/Sft3275.50%Sft

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**1I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (B&R) SITE ZONE DMC WEST KARACHI**

**Work 05**

**SUBJECT: - CONST / IMP OF SEWERAGE LINE I/C CC FLOORING FROM TILAWAT**

**HOUSE AND ZAHEER HOUSE AT SECTOR III IN UC-04 METROVILL**

**SITE ZONE DMC (WEST)**

**E/Cost: 9,61,940/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Dismantling of CC Work 1:2:4 4998/Cft 3327.50%Cft

2. Cartage of 100 Cft 5 tons all materials like stone

aggregate spwals lime surkhi BG rail fasting points

crossing bridge guders pipe sheet M/S Brass sheets

1000 trenches 10×5×3" 1000 tiles 12×6×2" 150 cft

timber 100 mould fuel wood by trenches owned by the

contractor withing 10 miles etc comp: 3998/Cft 902.20%Cft

3. CC plain i/c placing compacting finishing and curing

complete i/c screening and washing of stone aggregate

without shuttering ratio 1:4:8 3927/Cft 9416.28%Cft

4. P/L 2" thick toping cement concrete 1:2:4 i/c surface

finishing and dividing into panels eto completed. 11900/Sft3275.50%Sft

**EXECUTIVE ENGINEER (B&R)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (M&E) SITE ZONE DMC WEST KARACHI**

**Work 06**

**SUBJECT: - REPAIR / MAINTENANCE & ENGINE OVERHAULING OF SANITATION**

**VEHICLE NO. CH-11402 & CH-21288 IN SITE ZONE DMC (WEST)**

**E/Cost: 9,72,000/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. **MACHINING / GRINDING WORK.**
2. Crank Shaft Grinding Polish.
3. Cam Bush Fitting.
4. Connecting Rod Bush Fitting Boring.
5. Cylinder Boring / Sleeve Removing.
6. Sleeve Fitting.
7. Head Tikli Fitting.
8. Main & Big end Bearing.
9. Valve Seat Cutting & Facing.
10. Head Facing.
11. Main Tikli Fitting.
12. Crank Shaft Alignment.
13. Engine Block and Head Checking with Lines

Chemical Treatment of Cleaning all Engine

Complete. 01 Job 35,500/-

1. **ENGINE.**
2. Liner kit.
3. Main & Big end Bearing. 01 Set.
4. Engine Overhauling Kit. 01 Set.
5. Valve Intel / Exhaust set. 01 Set.
6. Valve Guide Set. 01 Set.
7. Came Bush Set. 01 Set.
8. Connecting Rod Bush Set. 01 Set.
9. Tappid Bush. 01 Set.
10. Valve Catcher. 01 Set.
11. Oil Pump Assembly. 01 Set.
12. Hose Pipe / Fan belt. 01 Set.
13. Water Jacket. 01 Set.
14. Complete Gas Kit. 01 Set.

Complete in all Respect 01 Job 1,45,000/-

1. **FUEL INJECTION PUMP.**
2. Providing / fixing Rear / Head Disk. 01 No
3. Providing / fixing Diesel Plate. 01 No
4. Providing / fixing Packing Kit. 01 No
5. Providing / fixing Spring with washers. 01 No
6. Providing / fixing Plunger Nozzles. 01 No
7. Providing / fixing Injection Nozzles. 01 No 01 Job 31,700/-
8. Providing /Fixing the air compressor by means complete

replacement of piston, sleeve & connecting rod & gray

in all respect. 01 Job 80,900/-

1. Clutch system over hauling work I/C the cost of

replacement of following parts:

1. Clutch Plate.
2. Pressure Plate.
3. Clutch Cylinder(upper & Lower) kit. 02 Kit
4. Fly wheel twining & polishing. 01 Job 01 Job 35,500/-
5. Brake System: over hauling work I/C the cost of

replacement of following parts:

1. Brake Washers. 12 Nos
2. Brake Shoes. 16 Nos
3. Wheel Oil Seal. 04 Nos
4. Brake Booster control valves. 03 Nos
5. Brake Booster diaphragms. 04 Nos
6. Liner kit of compressor. 01 Set
7. Wheel Cylinder complete in all respect. 04 Job 01 Job 30,500/-
8. Electric System Providing / Fixing complete

wiring kit work i/c the cost of the replacement of

following Genuine / imported accessories.

1. P/Fixing head light complete with housing. 04 Nos
2. Back light assembly. 02 Nos
3. P/Fixing Parking light. 02 Nos
4. P/Fixing indicator assembly. 04 Nos
5. P/Fixing Choke Cable. 02 Nos
6. Complete wiring.
7. P/Fixing oil gauge. 02 Nos
8. P/Fixing batteries 100AMP. 02 Nos
9. Wiring of Batteries. 01 Set 01 Job 40,700/-
10. P/Fixing the water body complete in all respect
11. Repair of rear spring leaf by means of opening leaf

repairing & refitting the same the work i/c P/F

broken spring leaf, change of U-Clamp, centre bolt

bush & tensioning the all leafs etc as required as per

instruction of E/I. 01 Job 13,500/-

1. Repair of front spring leaf by means of opening leaf

repairing & refitting the same the work i/c P/F

broken spring leaf, change of U-Clamp, centre bolt

bush & tensioning the all leafs etc as required as per

instruction of E/I. 01 Job 14,500/-

1. P/Fixing the radiator opening the radiator from top

& bottom side & soldering top & bottom cover

damage fixing the nut bolt & bracket fitting &

complete as required. 01 Job 15,900/-

1. P/Fixing the self complete in all respect as required. 01 Job 12,900/-
2. Providing / Fixing Alternator Complete 01 Job 11,500/-
3. P/Fixing the tie rod & steering knuckle repairing of

spindle, P/Fixing the ball joint, & all rubber

accessories bearings complete in all respect. 01 Job 10000/-

**CH-21288**

1. **MACHINING / GRINDING WORK.**
2. Crank Shaft Grinding Polish.
3. Cam Bush Fitting.
4. Connecting Rod Bush Fitting Boring.
5. Cylinder Boring / Sleeve Removing.
6. Sleeve Fitting.
7. Head Tikli Fitting.
8. Main & Big end Bearing.
9. Valve Seat Cutting & Facing.
10. Head Facing.
11. Main Tikli Fitting.
12. Crank Shaft Alignment.
13. Engine Block and Head Checking with Lines

Chemical Treatment of Cleaning all Engine

Complete. 01 Job 35,500/-

1. **ENGINE.**
2. Liner kit.
3. Main & Big end Bearing. 01 Set.
4. Engine Overhauling Kit. 01 Set.
5. Valve Intel / Exhaust set. 01 Set.
6. Valve Guide Set. 01 Set.
7. Came Bush Set. 01 Set.
8. Connecting Rod Bush Set. 01 Set.
9. Tappid Bush. 01 Set.
10. Valve Catcher. 01 Set.
11. Oil Pump Assembly. 01 Set.
12. Hose Pipe / Fan belt. 01 Set.
13. Water Jacket. 01 Set.
14. Complete Gas Kit. 01 Set.

Complete in all Respect 01 Job 1,45,000/-

1. **FUEL INJECTION PUMP.**
2. Providing / fixing Rear / Head Disk. 01 No
3. Providing / fixing Diesel Plate. 01 No
4. Providing / fixing Packing Kit. 01 No
5. Providing / fixing Spring with washers. 01 No
6. Providing / fixing Plunger Nozzles. 01 No
7. Providing / fixing Injection Nozzles. 01 No 01 Job 31,700/-
8. Providing /Fixing the air compressor by means complete

replacement of piston, sleeve & connecting rod & gray

in all respect. 01 Job 80,900/-

1. Clutch system over hauling work I/C the cost of

replacement of following parts:

1. Clutch Plate.
2. Pressure Plate.
3. Clutch Cylinder(upper & Lower) kit. 02 Kit
4. Fly wheel twining & polishing. 01 Job 01 Job 35,500/-
5. Brake System: over hauling work I/C the cost of

replacement of following parts:

1. Brake Washers. 12 Nos
2. Brake Shoes. 16 Nos
3. Wheel Oil Seal. 04 Nos
4. Brake Booster control valves. 03 Nos
5. Brake Booster diaphragms. 04 Nos
6. Liner kit of compressor. 01 Set
7. Wheel Cylinder complete in all respect. 04 Job 01 Job 30,500/-
8. Electric System Providing / Fixing complete

wiring kit work i/c the cost of the replacement of

following Genuine / imported accessories.

1. P/Fixing head light complete with housing. 04 Nos
2. Back light assembly. 02 Nos
3. P/Fixing Parking light. 02 Nos
4. P/Fixing indicator assembly. 04 Nos
5. P/Fixing Choke Cable. 02 Nos
6. Complete wiring.
7. P/Fixing oil gauge. 02 Nos
8. P/Fixing batteries 100AMP. 02 Nos
9. Wiring of Batteries. 01 Set 01 Job 40,700/-
10. P/Fixing the water body complete in all respect
11. Repair of rear spring leaf by means of opening leaf

repairing & refitting the same the work i/c P/F

broken spring leaf, change of U-Clamp, centre bolt

bush & tensioning the all leafs etc as required as per

instruction of E/I. 01 Job 13,500/-

1. Repair of front spring leaf by means of opening leaf

repairing & refitting the same the work i/c P/F

broken spring leaf, change of U-Clamp, centre bolt

bush & tensioning the all leafs etc as required as per

instruction of E/I. 01 Job 14,500/-

1. P/Fixing the radiator opening the radiator from top

& bottom side & soldering top & bottom cover

damage fixing the nut bolt & bracket fitting &

complete as required. 01 Job 15,900/-

1. P/Fixing the self complete in all respect as required. 01 Job 12,900/-
2. Providing / Fixing Alternator Complete 01 Job 11,500/-
3. P/Fixing the tie rod & steering knuckle repairing of

spindle, P/Fixing the ball joint, & all rubber

accessories bearings complete in all respect. 01 Job 10000/-

**EXECUTIVE ENGINEER (M&E)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**OFFICE OF THE EXECUTIVE ENGINEER (M&E) SITE ZONE DMC WEST KARACHI**

**Work 07**

**SUBJECT: - REPAIR / MAINTENANCE OF VEHICLE NO. CH-16643 HINO**

**LIFTER SITE ZONE DMC (WEST)**

**E/Cost: 9,75,800/- E/Money 20,000/- T/Limit 45 Days Penalty 500/- PD.**

**S.No Description of Work Quantity Rate Per%**

1. Re-fabrication of driver cabin Hino-KR-by means of

Manufacturing and fixing of roof complete as per

Genuine shape and design, P/F of inner roof regizin

And form repairing of seats by means of full

cautioning with seat cover best quality

manufacturing and fixing of mudguard left and right

side rear and front denting of front show denting

L/R side door denting of rear side denting and

repairing front bumper repairing of cooly seat, P/F

of valve 3”dia with electric welding complete cabin

painted with under coat and protein etc. P/F of

following accessories door lock. P/F of glass

channel and side glass with handle cabin back glass

with rubber. P/F of front indicator set. 01 Job 2,50,000/-

2. P/F Tyres, Tubes & Flap Size 7-50-16 General

Make as required. 06 Nos 1,50,000/-

3. Clutch system over hauling work I/C the cost of

replacement of following parts:

1. Clutch Plate.
2. Pressure Plate.
3. Clutch Cylinder(upper & Lower) kit. 02 Kit
4. Fly wheel twining & polishing. 01 Job 01 Job 35,500/-

4. Brake System: over hauling work I/C the cost of

replacement of following parts:

1. Brake Washers. 12 Nos
2. Brake Shoes. 16 Nos
3. Wheel Oil Seal. 04 Nos
4. Brake Booster control valves. 03 Nos
5. Brake Booster diaphragms. 04 Nos
6. Liner kit of compressor. 01 Set
7. Wheel Cylinder complete in all respect. 04 Job 01 Job 30,500/-

5. Fuel Injection Pump.

1. Providing / fixing Rear / Head Disk. 01 No
2. Providing / fixing Diesel Plate. 01 No
3. Providing / fixing Packing Kit. 01 No
4. Providing / fixing Spring with washers. 01 No
5. Providing / fixing Plunger Nozzles. 01 No
6. Providing / fixing Injection Nozzles. 01 No 01 Job 50,500/-

6. P/F of Hydraulic Jack shaft with piston, Oil Seal Kit

& both sides pin with lock. 01 Job 65,700/-

7. Manufacturing and fixing of all pin with lock rear &

front side Booms. 01 Job 45,900/-

8. P/F of Control Valve Assembly. 01 Set 25,000/-

9. P/F of Hydraulic Pipe with tee both side as per req. 10 Nos 35,700/-

10. Manufacturing, Cutting, Bending of M.S Sheet for

floor with electric welding as par required. 01 Job 45,500/-

11. Repair of rear hydraulic jacks both side with

hydraulic pipe both side. 01 Job 75,900/-

12. P/Fixing self & generator complete as required. 01 Job 60,900/-

13. Repair of Fiber Basket as per required. 01 Job 45,000/-

14. Complete Vehicle of Hydrulic Boom Painted as per

required. 01 Job 35,000/-

15. P/Fixing batteries 100AMP Exide with Terminals. 02 Nos 24,700/-

**EXECUTIVE ENGINEER (M&E)**

**SITE ZONE DMC (WEST)**

**I / we hereby quoted \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Above / Below the SR.**

**Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**