|  |  |
| --- | --- |
| **NAME OF WORK :** | **RENOVATION / ALTERATION OF LEFT & RIGHT SIDE OF SEVEN FLOOR OF A.K. LODHI BLOCK SINDH SECRETARIAT NO-6, FINANCE DEPARTMENT (DIFFERENT WORKS)** |

**“ SCHEDULE ‘’B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A-i” ( CIVIL WORKS )** | |  |  |  |
| 1 | Applying chemical polishing on existing mosaic /Marble flooring / dado including cleaning, grinding with carborandum stone / sand paper and applying chemical polish as per requirement. ( SI.70/P-49 ). | 4707.00 Sft. | 36/60 | P/Sft. | 172276/- |
|  | Rupees. thirty six. And. Sixty. Paisa | | | | |
| 2 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2” thick Teak wood ply shutters of 2nd class deodar wood skeleton ( solid ) styles and rails core of partal wood and commercial ply wood ( 3-Ply ) on both side in/c hold fasts, hinges, Iron tower bolts, handles and cleats with cord etc complete. ( SI.58 / P-65 ) – ( SI.25-b / P-61 )  Rs.1077/06 ( - ) Rs.370/83 = **706/23** | 276.25-Sft | 706/23 | P.Sft | 195096/- |
|  | Rupees. seven hundred & six. And. Twenty three. Paisa | | | | |
| 3 | P/F 3/8” thick marble tiles of approved quality and colure and shade size 8”x4/6”x4” in dado skirting and facing removal / tucking of existing plaster surface etc over ½” thick base of cement mortar 1:3 setting of tiles in slurry of white cement over mortar base in/c filling the joints and washing the tiles with white cement slurry curing finishing cleaning and polishing etc complete. (ii) for old work. (SI.58-i/P-49) | 266.00 Sft. | 201/07 | P/Sft. | 5348/- |
|  | Rupees. two hundred & one. And. Seven. Paisa | | | | |
|  | **Total Rs.** | | | | **372720/-** |
|  | Above / Below Rs. | | | |  |
|  | **(A) Total Rs.** | | | |  |
|  | **Part (A-ii) NON-SCHEDULE ITEMS.** |  |  |  |  |
| 1 | French polishing of doors windows ventilators stair floor work etc includes preparing surface and polishing by using Indian lakh Dana, spirit, thinner, pigment, ICI Lacquer, ICI hardener, Regmal (Germany) material ICI sealer tar pine oil, polishing as per satisfaction of competent authority etc complete | 756.00-Sft |  | PSft |  |
| 2 | Supplying and fixing in position Aluminum channels framing for sliding windows & ventilators of Lucky or equivalent made with 5mm thick tinted glass glazing (Belgium) and aluminum fly screen, handles, stoppers and locking arrangement etc complete. (b) Deluxe Model (Bronze of Champion color) | 92.00 Sft. |  | P/Sft. |  |
| 3 | P/F Aluminum partition with fixed glass (frosted) 5mm thick using 4” lucky section in champion color as frame on floor or block masonry fixed with necessary fixtures rubber packings etc. The cost in/c tools & plants used in making and carriage from shop to site as directed by the Engineer Incharge. | 120.00 Sft. |  | P/Sft. |  |
| 4 | P/F Gypsum board pelmet to be hanged from ceiling in specified shape and design as approved by the consultant. This in/c cutting the existing Gypsum board false ceiling in proper shape, hanging the structure by aluminum angle 1’x1” @ 3’-0 apart drilled and screwed in RCC slab, making hanging frame by using Aluminum U-channel section 1-1/2” wide in 18”x18” rafters and fixing Gypsum board sheet with chips and screws. Then filling the joints & screws holes with plastic mesh and plaster of Paris and making surface smooth as directed by the Engineer Incharge. | 5864.00-Sft |  | P/Sft. |  |
|  |  | **(B). Total Rs.** | | |  |
|  |  | **(A). Total Rs.** | | |  |
|  |  | **(A + B ). Total Rs.** | | |  |
|  |  | **Say Rs** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |