|  |  |
| --- | --- |
| **NAME OF WORK** | **M/R TO SINDH SECTT; NO. V I (OLD STATE BANK) KARACHI**  **(COLOR CRETE, FLOOR TILES, WOOD WORK WINDOW REPLACEMENT, COLORING, PAINTING & MISCELLANIES WORK FOR BUILDING(OLD STATE BANK ).** |

**“ SCHEDULE ‘B’ ”**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.#.** | | **DESCRIPTION OF ITEMS.** | **QTY:** | **RATE.** | **UNIT.** | **AMOUNT.** |
| **PART “A ) SCHEDULE ITEMS.** | | | | | | |
| 1 | Scraping (b) Ordinary distemper, oil bound distemper or paint on walls. ( SI.54(b)/P-13 ). | | 49985.00  Sft | 226/88 | %Sft | 113406/- |
|  | Rupees. Two hundred twenty six. And. Eighty eight. Paisa | | | | | |
| 2 | Distempering (b) Two coats. (SI.24(b).P-53) | | 3861.84  Sft | 1043/90 | %Sft | 40314/- |
|  | Rupees. One thousand forty three. And. Ninety . Paisa | | | | | |
| 3 | Preparing the surface & painting with weather coat of approved make to old weather coat surface (Old surface) (B) 2nd & subsequent coat. (SI.39(A+B+B)/P-56) | | 83688.26  Sft | 2118/33 | %Sft | 1772788/- |
|  | Rupees. Two thousand one hundred eighteen. And. Thirty three. Paisa | | | | | |
| 4 | Extra labour for external surface for distemper / paint / white wash / color wash / weather coat above 20’-0 height using long ladder of jhoola for each every 10’-0 additional height (20’-0 to 30’-0) (SI.42/P56)  (228.09 x 2 = 456/18) | | 10724.94  Sft | 456/18 | %Sft | 48925/- |
|  | Rupees. Four hundred fifty six. And. Eighteen. Paisa | | | | | |
| 5 | Extra labour external surface (30’-0 to 40’-0)  (SI.42/P-56) (228.09 x 2 = 456.0 x 2 = 912/36) | | 10125.61 Sft | 912/36 | %Sft | 92382/- |
|  | Rupees. Nine hundred twelve. And. Thirty six . Paisa . | | | | | |
| 6 | Extra labour external surface (40’-0 to 50’-0)  (SI.42/P-56) (228.09 x 3 = 684.27 x 2 = 1368/54) | | 10676.99  Sft | 1368/54 | %Sft | 146119/- |
|  | Rupees. One thousand three hundred sixty eight. And. Fifty four. Paisa | | | | | |
| 7 | Extra labour external surface (50’-0 to 60’-0)  (SI.42/P-56) (228.09 x 4 = 912/36 x 2 = 1824/72) | | 12946.90  Sft | 1824/72 | %Sft | 236245/- |
|  | Rupees. One thousand eight hundred twenty four. And. Seventy two. Paisa | | | | | |
| 8 | Extra labour external surface (60’-0 to 70’-0)  (SI.42/P-56) (228.09 x 5 = 1140/45 x 2 = 2280/90) | | 8859.50  Sft | 2280/90 | %Sft | 202076/- |
|  | Rupees. Two thousand two hundred eighty. And. Ninety. Paisa | | | | | |
| 9 | Painting old surface (d) painting Guard bars gates iron brass gratings railing in/c standard braces (etc) similar open work (i) 1st coat (ii) each subsequent coat. (SI.4.d.i+ii)/P-69) (3- coats) | | 913.00  Sft | 977/40 | %Sft | 8924/- |
|  | Rupees. Nine hundred seventy seven. And. Forty. Paisa | | | | | |
| 10 | Providing and fixing with jute felt paper of 60 Lbs over roof in/c cleaning of roof with wire brush and removing dust, applying bitumen coat at the rate of 34 Lbs per% Sft as premix inter coats and then laying felt paper with 10% over laps, then applying and spreading hill sand at the rate of 1 Cft for 100 Sft. The cost also in/c necessary fire material ,kerosene oil, wood etc. (SI.42 / P-39 ). | | 11452.97-Sft | 106/73 | P.Sft | 1222375/- |
|  | Rupees. One hundred & six. And. Seventy three. Paisa . | | | | | |
|  | **Total Rs.** | | | | | **3883554/-** |
|  | Above / Below Rs. | | | | |  |
|  | **(A). Total Rs.** | | | | |  |
|  | **PART (B) NON-SCHEDULE ITEMS.** | |  |  |  |  |
| 1 | P/F granite top 1” thick galaxy black in/c cutting marble top for vanity fixing cutting walls with cement sand in/call cost of labour material polishing cartage etc complete. | | 742.34Sft |  | PSft |  |
|  | **(B). Total Rs.** | | | | |  |
|  | **(A). Total Rs.** | | | | |  |
|  | **Say:** | | | | |  |
|  | **Say Rs.** | | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |