|  |  |
| --- | --- |
| **NAME OF WORK** | **M/R TO SINDH SECRETARIAT BUILDING NO.III (OLD KDA BUILDING) KARACHI**  **(SPECIAL REPAIR IN OFFICE OF THE ADVISOR TO C.M. 3RD FLOOR (REMAINING WORK)).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **NON-SCHEDULE ITEM** |  |  |  |  |
| 1 | Preparing the surface & fixing wall paper of required color and design in/c fixing border as required pasted to glue or solution as directed by the Engineer Incharge. | 1000.35-Sft |  | PSft |  |
| 2 | P/F Gypsum board pelmet to be hanged from ceiling in specified shape and design as approved by the consultant. This in/c cutting the existing Gypsum board false ceiling in proper shape, hanging the structure by aluminum angle 1’x1” @ 3’-0 apart drilled and screwed in RCC slab, making hanging frame by using Aluminum U-channel section 1-1/2” wide in 18”x18” rafters and fixing Gypsum board sheet with chips and screws. Then filling the joints & screws holes with plastic mesh and plaster of Paris and making surface smooth as directed by the Engineer Incharge. | 1699.66-Sft |  | PSft |  |
| 3 | S/F LED spot light China make with 7 Nos lamps each 6 watts fitted on walls, ceiling of approved quality as directed by the Engineer Incharge. | 67-Nos |  | Each |  |
| 4 | P/F fine quality roller type blind with approved design false & in/c steel angle fixing with steel screws as per window as required @ site as directed by the Engineer Incharge. | 371.52-Sft |  | PSft |  |
| 5 | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 24”x24”x1/4”** | 891.14- Sft |  | P.Sft |  |
|  |  |  | **Total Rs.** | |  |
|  |  |  | **Say Rs.** | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |