**Draft Bidding for works upto . Work No. 15**

**NIT-**

**NAME OF WORK: - CONSTRUCTION OF CC STREEL MEMON MUHALLA, SHORA MUHALLA WARD NO. 3**

**BILL OF QUANTITIES**

1. **Description and rate of Items based on Composite Schedule of Rates.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.** | **DESCRIPTION** | **QUANITITY** | **RATE** | **UNIT** | **AMOUNT** |
|  | **Preparing sub grade to including earth excavation or filling to an average depth of 9” dressing to camber and consolidation with power roller.**  **2.14 x 100 x 10 = 2140.0 Sft** | **2140.Sft** | **Rs.526.28** | **%Sft** | **Rs:11,262.00** |
|  | **P/L cement concrete brick or stone ballast 1-1/2’to2’ gauge 1:4:8 ratio etc complete (G. Sch: P-No: It/No: )**  **2.14 x 100 x 10 x 0.375 = 802.0 Cft** | **802.0Cft** | **Rs:9416.28** | **% Cft** | **Rs:75,518.00** |
|  | **Providing and laying 2”thick topping cement concrete (1:2:) inlcuidng surface finishing and dividing in to panels : (G.Sch:P/41 It/16d)**  **2.14 x 100 x 10 =2140.0Sft** | **2140.0Sft** | **Rs:3275.50** | **%Sft** | **Rs:70,095.00** |
|  |  | **Total** | | | **Rs.1,56,875.00** |

**\_\_\_\_\_\_\_\_%Above/Below On The Schedule Rates of CSR. Amount to be Added/Deducted on the basis of premium quoted Total (b)**

**Total (A) = a + b in words**

**Contractor**

**Assistant Executive Engineer / Procuring Agency**

**(Cont…..Page No.02)**

**Summary of Bill of Quantities**

**Cost of Bid Amount\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

1. **(A) Cost based on composite Schedule of Rate** ­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
2. **(B) Cost of based on Non / Offered Schedule of Rates.** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TOTAL COST OF BID (C) = TOTAL (A) + Total (B)** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Contractor**

**Assistant Executive Engineer / Procuring Agency**