**Draft Bidding for works upto . Work No. 12**

**NIT-**

**NAME OF WORK: - CONSTRUCTION OF METALED ROAD MIR BEHAR MOHALLAH WARD NO. 4**

**BILL OF QUANTITIES**

1. **Description and rate of Items based on Composite Schedule of Rates.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.** | **DESCRIPTION** | **QUANITITY** | **RATE** | **UNIT** | **AMOUNT** |
|  | **Preparing sub grade to including earth excavation or filling to an average depth of 9” dressing to camber and consolidation with power roller.**  8.1**0 x 100 x 10.0 = 8100.0 Sft** | **= 8100.0Sft** | **Rs.526.28** | **%Sft** | **Rs: 42628.00** |
|  | **Preparing sub-base supplying and spreading stone metal 1-1/2” -2” guage of approved quality from approve quarry in required thickness to proper camber and grade including hand packing mixed with shingle pit run grabel fines having P.I of not more than 6% in the ratio 2:3 including watering & compacting to achieve 98-100% density as per modified AASHO specifications. (Rate includes all cost of materials T&P and carriage upto 3 chains)**  **8.10x100x 10x0.48 = 3888.0 Cft** | **3888.0Cft** | **Rs:7518.52** | **%Cft** | **Rs: 292320.00** |
|  | **Providing surface dressing 1st coat on new or existing surface with 40 lbs bitumen and 5.5 Cft. Of Bajri of required size including cleaning the road surface rolling etc, complete. (Rate includes all cost of materials T&P and carriage upto 3 chains)**  **8.10 x 100 x 10.0 = 8100.0Sft** | **8100.0 Sft** | **Rs:1954.42** | **%Sft.** | **Rs: 158308.00** |
|  | **Providing 1-1/2” thick (consolidated) premixed carpet in proper camber and grade including supplying 15 Cft. Bajri, 5Cft. Hill sand (of approved quality and grade) bitumen of 80/100 Penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the road surface (Hill sand 3 Cft. For mixing and 2.0 Cft. For dusting) (Rate includes all cost of materials T&P and carriage upto 3 Chains)**  **8.10 x 100 x 10.0 = 8100.0Sft** | **8100.0 Sft** | **Rs:6165.84** | **%Sft.** | **Rs: 499433.00** |
|  |  | **Total** | | | **Rs. 992433.00** |

**\_\_\_\_\_\_\_\_%Above/Below On The Schedule Rates of CSR. Amount to be Added/Deducted on the basis of premium quoted Total (b)**

**Total (A) = a + b in words**

**Contractor**

**Assistant Executive Engineer / Procuring Agency**

**(Cont…..Page No.02)**

**Summary of Bill of Quantities**

**Cost of Bid Amount\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

1. **(A) Cost based on composite Schedule of Rate** ­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
2. **(B) Cost of based on Non / Offered Schedule of Rates.** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TOTAL COST OF BID (C) = TOTAL (A) + Total (B)** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Contractor**

**Assistant Executive Engineer / Procuring Agency**