**SCHEDULE B**

**CONSTRUCTION OF DIAGNOSTIC CENTRE WITH OPD /REFERRAL AT VILLAGE ADUR NEREJO U.C. JADO WAHAN TALUKA GAMBAT DISTRICT KHAIRPUR**

**EXTERNAL DEVELOPMENT I/C PATH ETC.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **ITEM OF WORKS** | **No: L: B: D:** | **Qty:** | **Rate** | **Unit** | **Amount** |
| **01.** | **S/Filling sand under floor plugging into wall 1:3** | |  |  |  |  |
|  |  |  | **88791.0** | **1141/25** | **% Cft** | **Rs.1527791/-** |
| **02.** | **Dressing leveling of the earth.** | |  |  |  |  |
|  |  |  | **88791.0** | **187/55** | **%Cft** | **Rs.16653/-** |
| **03.** | **Cement concrete brick or stone ballast 1-1/2 to 2 gauge. (A) ratio 1:5:10. (S.I.No.4 P.No.14).** | |  |  |  |  |
|  |  |  | **1149Cft** | **8694/95** | **%Cft** | **Rs.99905/-** |
| **04.** | **Cement concrete plain including placing compacting finishing and curing, complete (including screening and washing of stone aggregate without shuttering Ratio 1:2:4. (S.I.No.05 (f) P.No.18).** | |  |  |  |  |
|  |  |  | **575.0** | **14429/25** | **% CFT** | **Rs. 82968/-** |
| **05.** | **Providing & Fixing cement paving blocks o/s Building. Etc.** | |  |  |  |  |
|  |  |  | **3480.0** | **199/77** | **P.Sft** | **Rs:695200/-** |
| **06.** | Excavation in foundation of buildings bridges and other structures including dag belling dressing refilling around structure with excavated earth watering and ramming lead upto 5ft. (b) in ordinary soil. (S.I.No.18 P.No.5). | |  |  |  |  |
|  |  |  | **1314.0** | **3176/25** | **%0Cft** | **Rs:4174/-** |
| **07.** | **Cement concrete brick or stone ballast 1-1/2 to 2 gauge. (A) ratio 1:5:10. (S.I.No.4 P.No.14).** | |  |  |  |  |
|  |  |  | **438.0** | **8694/95** | **%Cft** | **Rs:38084/-** |
| 08. | Pacca Brick work in foundation & plinth in cement & Sand mortar Ratio 1:6 (S.I.No.4 (c) P.No.25). | |  |  |  |  |
|  |  |  | **988.0** | **11948/36** | **% CFT** | **Rs. 118050/-** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **ITEM OF WORKS** | **No: L: B: D:** | **Qty:** | **Rate** | **Unit** | **Amount** |
| **09.** | Cement plaster 1:6 upto 20 height ½ thick. (S.I.No.13 P.No.58). | |  |  |  |  |
| **10.** | Cement plaster 1:4 upto 20 height3/8 thick. (S.I.No.13 P.No.58). | | **1022.0** | **2206/60** | **%Sft** | **Rs:22551/-** |
|  |  |  | **1022.0** | **2197/52** | **%Sft** | **Rs:22459/-** |
|  |  | |  |  |  |  |
|  |  | |  |  | **Total** | **Rs;2627835/-** |

% Above/Below (Amount to be added/deducted).Rs.

**Grand Total** Rs.

Total Amount in word:

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |

**SCHEDULE B**

**CONSTRUCTION OF DIAGNOSTIC CENTRE WITH OPD /REFERRAL AT VILLAGE ADUR NEREJO U.C. JADO WAHAN TALUKA GAMBAT DISTRICT KHAIRPUR.**

**External Development**

**Part (B) Water Supply And Saintary Fitting.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **ITEM OF WORK** |  | **QTY:** | **RATE** | **UNIT** | **AMOUNT (RS.)** |
| **14.** | Providing RCC pipe with collars class “Band digging the troches to required depth and fixing in position including cutting fitting and jointing with asphalt composition and cement mortar 1:1 and testing with water pressure head of 4ft above the top of the height pipes and refilling with excavated staff. | |  |  |  |  |
|  | 9” Dia |  | **430 Rft** | **250/60** | **P.RFT** | **Rs. 107758/-** |
|  |  |  |  |  |  |  |
|  |  | | **Total** | | | **Rs107758/** |

% Above/Below (Amount to be added/deducted).Rs.

**Grand Total** Rs.

Total Amount in word:

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |