k

***SCHEDULE OF QUANTITIES***

***WORK No: 10***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 8,40,000/- Earnest Money Rs: 16,800/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Construction / Improvement at Gulshan-e-Ghazi UC-33, Baldia Zone, DMC (West).***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** | |
| *1.* | *Earth work excavator in undressed lead upto 5,9 Single throw of Kassi Phawrah or Shovel.* | *5800* | *1361.25* | *%0Cft* | *7895/-* | |
| *2.* | *P/L cement concrete brick or stone ballast 1 ½” to 2” gauge 1:4:8.* | *3828* | *9416.28* | *%0Cft* | *360455/-* | |
| *3.* | *P/L 2” Thick topping cement concrete 1:2:4 i/c surface finishing and sividing into panel etc complete.* | *11600* | *3275.50* | *%Sft* | *379958/-* | |
| *4.* | *Cartage of 100 Cft 5 tons of all kind material like cole bricks i/c loading unloading 10 miles.* | *5800* | *1065.04* | *%Cft* | *61772/-* | |
| *5.* | *P/F C.I M/H Cover Frame i/c cost of 1-Kg material etc.* | *35* | *140* | *P-Kg* | *4900/-* | |
| *6.* | *Manufacturing and supplying R.C.C main hole covers cast in situ 1:2:4 C.C 3” inch deep in center reinforced with 3/8” dia M.S Bars welded on M.S Sheet i/c curing transportation 21” dia.* | *27* | *913.63* | *Each* | *24668/-* | |
| ***Total Estimated Cost*** | | | | | | ***8,40,000.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*