SCHEDULE-B

PROVISION OF MISSING FACILITIES FOR TEACHING HOSPITAL N EXISTING D H Q AT DISTRICT KHAIRPUR PROVIDING INTERNAL ELECTRIFICATION. K M C TEACHING MEDICINE STORE

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | ITEM OF WORK | QTY | RATE | UNIT | AMOUNT |

(PART A SCHEDULE ITEMS)

1. Wiring for light or fan point with 1.1.13/.029)PVC insulated wire in 20 mm PVC

Insulated wire in ¾ PVC conduit recessed in the wall or columns as required (SINO: 124/p: 15)

Light point 156--Nos: 1130/- Each 176280/-

Fan point 78-Nos: 1130/- Each. 88140/--

2. Wiring for call bell point with 1.1.13(3/.029) PVC insulated wire in 20 mm ¾ PVC conduit recessed in the wall or columns as required(S.i.No:128-P15)

4-NoS: 1764/- Each 7056/--

3) Wiring for plug point with 1.1.13(3/.029) PVC insulated wire in 20 mm ¾ PVC conduit recessed in the wall or columns as required (S.i.no:126P-15

60-Nos: 985/- Each 59100/-

4) P/F 3 pin 10/15 amps plug socket flush type (S.I.NO;226/33)

32-No: 151/- Each 4832/-

5) P/F flush type 2 pin 5amps plug and socket flush type (S.I.No:225 p-33)

60-Nos: 83/- Each 4980/-

6) Wiring for( Main or sub Main )with 2-7/.029)PVC insulated wire in 20 mm PVC conduit recessed in the wall or columns as required (SINO:10p-2)

500-Mtr: 222/- P-Mtr: 111000/-

7 Wiring for(Main or sub Main with 2-7.036 PVC insulated wire in 25 mm 1 PVC conduit recessed in the wall or columns as required(SINO:

400-Mtr: 252/- P-Mtr: 100800/--

8) Wiring for (Main or sub Main) with 2-7/..044) PVC insulated wire in 25 mm PVC conduit recessed in the wall or columns as required (SINO12.P-2)

300- Mtr: 341/- P.Mtr: 102300/-

9) P/L Main or sub-Main PVC insulated with 2-7/.064 (6mm2) copper conductor ¾ dia PVC

Conduit in the wall or columns as required (S.I.No:14p-02)

150-Mtr: 641/- P-Mtr: 96150/-

10) P/F circuit bracket 15 amp to 100 amps TP ((XS-100NS) on prepared board as required (S.I.No.207p-31 02-Nos: 9261/- Each 18522/-

11) P/F circuit bracket 6 amp to 63 amps SP ((TB-5S) on prepared board as required (S.I.No.203p-31 35-Nos: 916/- - Each 32060/-

12) Providing circuit breaker 125, 150, 200, & 225, TP XS 225 NS on prepared board as required (SINO: 208/p31)

01-Nos: 25541/- Each 25541/-

13) P/F brass pendent lamp holder (SINO: 229-p33)

60-Nos: 74/- Each 4440/-

14) P/F backlit ceiling rose with two terminals (S.I.NO; 228 P—33)

142-Nos: 72/- Each 10224/-

15) P/L main or sub main PVC insulated and PVC sheated with 4 core armored copper conductor 600/1000 volt size 35 mm 2 (SINO. 115-P-13)

60-Mtr: 3008/- p-Mtr; 180480/-

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Total= 1,066,073/-

(PART B NON SCHEDULE ITEMS)

1) P/F main Panel board double shutter to accommodate heavy duty circuit breaker

I/c painting with enameled paint for other similar job on surface

4- SFT Each

2) P/F energy sever superior quality

92-No: Each

3) P/F Earthing set with 2x2x1/4 copper plate buried in the ground at a depth of 12 ft or less if the water comes out from the ground level with salt and cholorocal etc i/c providing G.I. pipe and copper wire size size 8 SWG in all respect

1-No: Each

4) P/F mild steel bar fan clamps 15.8mm (5/8”) suitable for RCC roof.

78-Nos: Each

5) Errection of AC ceiling fan i/c wiring of down rod with 1.1.3/.029) PVC wire in fixing on regulators blade canopy etc complete

78-Nos: Each,

6) P/F fancy dimmer for AC ceiling fan etc complete

78-Nos: Each

7) P/F of double tube light china made electronic chowke grill framed and 2 Nos:

Tube rod 4 ft long etc complete.

40-Nos: Each.

8) P/F of tube light Patti fitting i/c 40 watts choke starter 4 ft long tube rod along with

Holder fitting complete in all respects

24-Nos: Each

9) Providing and fixing of fancy switch plate sheet china made 10 gang frame i/c approved quality i/c internal connection etc complete

15-Nos: Each

10) Providing and fixing of fancy switch plate sheet china made 04 gang frame i/c approved quality i/c internal connection etc complete

36-No: Each

11) P/F of Fancy light fitting superior quality etc complete

32-Nos: Each

12) S/F AC ceiling fan56 sweep size pak fan GFC SK company i/c fixing and wiring connection etc complete

78-Nos: Each

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Total=

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR EXECUTIVE ENGINEER

PROVINCIAL BUILDINGSDIVISION

. SHAHEED BENAZIR ABAD