**SCHEDULE-B**

**CONSTRUCTION OF SECURITY BARRIERS/C.C BLOCK NEAR IMAM BARGAH QASAR-E-HUSSAINI MOHALLA ALI MURAD SHAH TALUKA & DISTRICT KHAIRPUR.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR#** | **ITEM OF WORKS** | **NO. L: B: D:** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| **01.** | Dismantling Cement concrete plain (1:2:4) etc completed. | |  |  |  |  |
|  |  |  | **570.00** | **3327/50** | **%Cft** | **Rs.18967/-** |
|  |  |  |  |  |  |  |
| **02.** | Cement concrete brick or stone ballast 1-1/2 to 2 gauge. (A) ratio 1:5:10. (S.I.No.4 P.No.17). | |  |  |  |  |
|  |  |  | **753.00** | **8694/95** | **%Cft** | **Rs.65473/-** |
|  |  |  |  |  |  |  |
| **03.** | Cement concrete plain including placing compacting finishing and curing, complete (including screening and washing of stone aggregate without shuttering Ratio 1:2:4. (S.I.No.05 P.No.18). | |  |  |  |  |
|  |  |  | **388.00** | **14429/25** | **%Cft** | **Rs.55985/-** |
|  |  |  |  |  |  |  |
| **04.** | Providing and laying floor of Verona marble tiles 24x12x¾ fine dressed on the surface with out winding set in white cement over a base of 1:2 grey cement mortar ¾”thick filling of joint with salary of white cement and pigment in desired shape with finishing cleaning cursing cutting tiles to proper profile rubbing & chemical polishing etc complete (R.A sanctioned ). | |  |  |  |  |
|  |  |  | **26.00** | **301/-** | **%Cft** | **Rs.782600/-** |
|  |  |  |  |  |  |  |
|  |  |  | **TOTAL** | | | **Rs.923025** |

% Above/Below (Amount to be added/deducted).

Rs. **Grand Total** Rs. **Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |