***SCHEDULE OF QUANTITIES***

***WORK No: 10***

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 5,90,801/-O/R Earnest Money Rs: 11,816/-+O/R***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: *Construction and Maintenance of Park at Sector 8-B New Saeedabad UC-37 DMC***

***(West) Baldia Zone.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Excavation for foundation of building bridges & other structures i/c day boiling dressing refilling governed structure with excavated earth watering & ramming lead up to 5 Ft in ordinary soil.* | *1473* | *3176.25* | *%0Cft* | *4678/-* |
| *2.* | *Cement concrete plain i/c placing compacting finishing and curing complete (including screening and washing at stone aggregate without shuttering ratio (1:2:4).* | *1037* | *14429.25* | *%Cft* | *149631/-* |
| *3.* | *Cement concrete brick or stone ballast 1½” to 2” gauge (1:4:8).* | *346* | *9416.28* | *%Cft* | *32580/-* |
| *4.* | *Erection or removal Centering for R.C.C or plain C.C work decoder wood 2nd Glass vertical.* | *2073* | *3127.41* | *%Sft* | *64831/-* |
| *5.* | *Providing and Laying 1:3:6 cement concrete solid block masonry wall above 6” in thickness set in 1:6 cement mortar in G.F Ground floor super instruction including raking out joint & curing etc.* | *952* | *14621.44* | *%Cft* | *139196/-* |
| *6.* | *Cement plaster 1:2 upto 12” height ½” thick.* | *4913* | *2496.72* | *%Sft* | *122664/-* |
| *7.* | *Distempering three coats.* | *11360* | *1079.65* | *%Sft* | *122648/-* |
| *8.* | *Leveling dressing and making lawns.* | *18018* | *181.50* | *%Sft* | *32703/-* |
| *9.* | *Painting with enamel paint on masonry walls 2nd subsequent coats.* | *2073* | *837.10* | *%Sft* | *17353/-* |
| *10* | *Supply and Spreading red moron.* | *864* | *O/R* | *%Cft* | *O/R* |
| *11.* | *Supply Dhaka Grass.* | *18018* | *O/R* | *P/Sft* | *O/R* |
| *12.* | *Carriage of 100cft 5 tons of all kinds of material like stone aggregate sprawl, coal, line sukhi etc. BG Rail fasting and point and grass bridge 1000- Nos Brick “10”x5”x3” or 1000-Nos Tiles “12”X6”X2”* | *1473* | *595.80* | *%Cft* | *8776/-* |
| ***Total Estimated Cost*** | | | | | ***5,90,801/-+O/R*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***SUB-ENGINEER (PARK & RECREATION) D.T.O (PARK & RECREATION)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*