**SCHEDULE-B**

**ESTIMATE FOR M/R TO SESSION COURT COMPLELX AT NAWABSHAH PROVIDING INTERNAL E.I**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.No: | Item of work | Qty | Rate | Unit | Amount |

**(Part A Schedule Items)**

1. Wiring for light or fan point with 1.1.13/.029)PVC insulated wire in 20 mm PVC Insulated wire in ¾ PVC conduit recessed in the wall or columns as required(SINO:124/p:15)

Light point 51-Nos: 1130/- Each 57630/-

2) P/F circuit bracker 15 amps to 60 amps TP XE-100 on a prepared as required (S.I.NO;206 p-31

4-No: 5521/- Each 22084/-

3) 8) P/F circuit breacket 6 amp to 63 amps SP ((TB-5S) on prepared board As required (S.I.No.203p-31

21-Nos: 916/- - Each 19236/-

4) P/F brass bracket lamp holder suitable for 15 mm 5/8 “ holder (SINO:231p-33)

13-Nos: 72/- Each 936/-

5) providing and laying main or sub main PVC insulated wire with size 2-7/.036 4mm2 copper conductor in ¾ dia PVC conduit on surface (SINO:4p-1)

397-Mtr: 200/- P.Mtr 79400/-

(6)Providing and fixing DP i/c change over switch 500 volts 1000 amps on a

Prepared board (S.I.NO; 198P-30)

1-No: 7612/- Each 7612/-

\_\_\_\_\_\_\_\_\_\_\_\_

Total= 186,898/-

\_\_\_\_\_\_\_\_\_\_\_\_

**(PART B NON SCHEDULE ITEMS)**

1) P/F Energy sever 85 watt superior quality etc complelte

3-Nos: Each

2) Providing and fixing energy server25 watt superior quality.

13-Nos: Each

3) Rewinding of motor 2 HP single phase 220 voltes etc complete.

04-Nos: Each

4) P\F Dimmer for electric fan and regulator etc complete.

2-Nos: Each

*5) P/F main Panel board double shutter to accommodate heavy* duty circuit breaker i/c painting with enameled paint for other similar job on surface

06 SFT Each

6) Providing and fixing fan capacitor 3.5 good quality.

2-Nos: Each

7) P/F Chowke for tube light 40 watt complete

2-Nos: Each

8)P/F Tube rod 4 ft ling 40 watt good quality etc complete

21-Nos: Each

9) Rewinding ofAC ceiling fan 56 sweep size with copper i/c replacement

Of ball bearing etc complete.

19-Nos: Each

8) S/Fixing L.ED light 24 watt complete wth fixing internal connection in the shape of square or round type

44-Nos: Each

9) P/F I T systm Connector patti 10 connector fixing in the I T panel box approved

quality

03-Nos: Each

(10) Providing and universal fixing on a prepared board approved quality.

05-Nos: Each

\_\_\_\_\_\_\_\_\_\_\_\_

Total=

\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR EXECUTIVE ENGINEER

PROVINCIAL BUILDINGS DIVISION

SHAHEED BENAZIR ABAD