**TENDER FORM (Tender Form Fees Rs.500/-(Non Refundable)**

**PURCHASE OF I.T EQUIPMENT FOR THE YEAR 2017-18**

**TENDER INQUIRY NO. 10/2017-18 DUE ON 14-02-2018**

**Time of issuance of Tender form upto 13-02-2018 at 02:00 P.M**

**Time of Submission of Tender on 14-02-2018 at 11.30 A.M**

**Time of Opening of Tender on 14-02-2018 at 12.00 Noon**

|  |  |  |  |
| --- | --- | --- | --- |
| **S.No** |  | **Qty** | **Price in Figure and Word** |
| **01** | **Desktop PC with UPS 650 VA**  Brand: HP,DELL, IBM. Intel® Core™ i7-7700 (3.5 GHz) with Intel® Turbo Boost Technology, 6 MB cache, 4 cores) Processing - Ram : Minimum 8GB DDR4  - Storage : Minimum 1 TB SATA, supports upto 4 TB  - Display: Wide Screen 17 “- Ports: HDMI, VGA, RJ45, minimum 6 x USB 2.0, Audio Head Phone, Power input  - Network interface: 10/100/1000 GbE –  Graphics  NVIDIA® GeForce® GTX 1060 3G  Optical drive  Ultra Slim-tray SuperMulti DVD burner  Wireless technology  WLAN RT 8821CE ac 1x1 +BT 4.2 WW  Keyboard and mouse  HP USB Wired Keyboard with volume control  Optical mouse with 1 Year Warranty  Pre-Installed OS Windows 10 License - Warranty: 1 year | **10** |  |
| **02** | **Heavy Duty Scanner (With UPS 650 VA)**  **[Technical specifications](javascript:%20void(0);)**  Scanner type: Flatbed, ADF  Digital sending standard features  Local or network folder; e-mail; SharePoint 2007 & 2010; Cloud destinations; Google Drive; Box; FTP; printer; fax; user-defined command-line application; web folder  Scan resolution, optical Up to 600 dpi  Recommended daily duty cycle: 5000 pages  Bit depth: 48-bit  Levels of grayscale: 256  Multifeed detection: Yes, ultrasonic  Scan size, maximum: 297.2 x 431.8 mm  Media types: Paper (plain, inkjet, photo), envelopes, cards (index, greeting), 3-D objects  Media weights, supported ADF: 49 to 120 g/m²  Scan file format:  PDF (image-only, searchable, MRC, PDF/A, encrypted), TIFF (single page, multi-page, compressed: G3, G4, LZW, JPEG), DOC, RTF, WPD, XLS, TXT, XML, XPS, HTML, OPF, JPG, BMP, PNG  VirtualRescan (VRS) Professional drivers  Scanner advanced features:48-bit internal/24-bit external bit depth  Control panel: 2 quick start buttons (Scan, Copy), Cancel, Tools, Powersave  **[ADF specifications](javascript:%20void(0);)**  Automatic document feeder capacity  Standard, 200 sheets  Automatic document feeder speed  Up to 50 ppm/100 ipm (b&w, gray, color, 200 dpi)[1]  Scanning options (ADF)  Single-pass duplex  Scan size (ADF), maximum  300 x 864 mm  Scan size (ADF), maximum  11.7 x 34 in  Scan size (ADF), minimum  70 x 148 mm  Scan size (ADF), minimum  2.75 x 5.8 in | **01** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **03** | **Photo Copier with UPS 650VA**  Brand: Xerox,HP,Canon or Equivalent. Standard functions  Copy, Email, Print, Scan Optional functions Walkup Fax, Xerox Integrated RFID Card Reader Recommended monthly print volume Up to 13,000 pages Duty cycle Up to 107,000 images/month First-page-out time, copying  As fast as 6.8 seconds First-page-out time, printing  As fast as 10.4 seconds Two-sided output Standard  Accounting Network 1200 x 1200 dpi Page Description Languages (PDL) HP-GL, JPEG, PCL® 5e, 6, PDF, TIFF, XPS (optional: Adobe PostScript® 3™) Print memory (standard) 2 GB standard Hard drive 320 GB (optional on Desktop Model) Connectivity Ethernet 10/100/1000 Base-T, High-speed USB 3.0, NFC Tap-to-Pair, Wi-Fi 802.11n and Wi-Fi Direct with optional Wi-Fi Kit (concurrent wired and wireless connections supported)  Or similar | **01** |  |
| **04** | **Card Printer with UPS 650VA**  Brand: HP, FARGO, Canon or Equivalent  **Sided Printing:** Single or Dual  **Print Method:** HDP Dye-Sublimation / Resin Thermal Transfer  **Resolution:** 300 dpi  **Print Speed:** up to 24 seconds per card / 150 cards per hour (YMC with transfer)\*  **Accepted Card Sizes:** CR-80  **Warranty:** 3 years (printer); Lifetime (printhead)  Printer Options:  **New:** Dual Card Input Hopper - Upgradable  Card Lamination Module - single-sided or dual-sided (simultaneous) - Upgradable  Smart card encoding (contact/contactless) - Upgradable  Door and cartridge locks  Printer cleaning kit  Magnetic stripe encoding - Upgradable  200-card input hopper - Upgradable  Dual-sided printing - Upgradable  Single Wire Ethernet and USB 2.0 interface for in-line printing and encoding (note: single wire Ethernet encoding is only available for iCLASS and contact smart card encoding)  Or similar | **01** |  |
| **05** | **Flash Disk 32GB (USB)**  **Samsung / Segate/ Kingston or equivalent** | **10** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **06** | **Hard Drive 1 TB (Portable)**  **Samsung / Segate/ Western Digital** | | **06** | |  |
| **07** | **Laser Pointer**  **Logitech / A4 Tech/Audio link or equivalent** | | **03** | |  |
| **08** | **Multimedia Projector with LED with UPS 650VA**  Optical Specifications Detail: Projection System3 LCD Color Light Output3800lm Light Output3800lm Contrast Ratio3300:1 Lamp225W Lamp Life9 Projection Lens Approx. x1.6 Throw Ratio1.40:1 to 2.27:1 Screen Coverage30 to 300" **Input/ Output Specifications Detail:** S-Video In4 pin(x1) Composite Video InRCA (1) Analog RGB/Component In15 pin HD(2) Digital In HDMI (2) NetworkRJ45 Monitor Out15 pin HD Variable Audio Out1280 **Electrical Specifications Detail:** Native Resolution1024 by 768 Color SystemNTSC3.58, PAL, SECAM, NTSC4.43, PAL-M, PAL-N Acceptable Computer Signals Maximum display resolution : 1600x1200 dots Acceptable Video Signals Video(Composite), 15k(480/60i, 575/50i), DTV (480/60p, 575/50p, 720/60p, 720/50p, 1080/60i, 1080/50i, 1080/60p, 1080/50p) | **01** | |  | |
| **09** | **Fax Machine Color Tonner Complete Original**  Tonner Model No. 201A | **01** | |  | |
| **10** | **Printer Model No. M1132 MFP** | **01** | |  | |
| **11** | **HP Color LaserJet Pro M254 DW** | **01** | |  | |

**NATIONAL TAX No:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ SIGNATURE …………………………………..**

**GST No: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ NAME OF CONTRACTOR ……….…………**

**C.N.I.C No: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ADDRESS …...…………………….…….……**

**(Photostat copies must be enclosed) Contact NO ………..…………….……………**

**I N S T R U C T I O N S**

1. **The tender should be accompanied with pay order / demand draft of 2.5% as security Deposit in the name of Sindh Institute of Ophthalmology & Visual Sciences (SIOVS) Hyderabad.**
2. **The Income Tax / GST/SST will be deducted according to rules of Govt: of Sindh / Pakistan.**
3. **The tenderer will be responsible to deliver the tendered items on his own cost at SIOVS HYDERABAD.**
4. **In case of short/late supply, it will be purchased from open Market and difference if any will be recovered from the Contractor.**
5. **The vendor must possess authorization letter for the concerned item.**
6. **Conditional/ Incomplete Tenders will not be accepted.**
7. **Sample of all dry items should be provided at the time of opening of tender otherwise tender will be rejected.**
8. **For alternate offer separate tender purchase receipt must be enclosed**
9. **The tenderer should be fulfilling all requirements as per Government rules**
10. **Minimum Two Hundred Thousands turn over with Bank Certificate**
11. **Minimum Three Years Experience in relevant field with documentary proof**
12. **Three Years Income Tax Return (Photo Copy Must Enclosed)**
13. **The Performance Security is 10% for One Year w.e.f the date of contract agreement.**
14. **The Performance Security is 10% for One Year w.e.f the date of contract agreement in the name of Sindh Institute of Ophthalmology & Visual Sciences (SIOVS) Hyderabad.**

**Purchase & Store Officer,**

Sindh Institute of Ophthalmology

& Visual Sciences, Hyderabad