**TENDER FORM (Tender Form Fees Rs.500/-(Non Refundable)**

**PURCHASE, INSTALLATION , TESTING & COMMISSIONING OF WALK THROUGH GATES ON TURNKEY BASIS**

**FOR THE YEAR 2017-18**

**TENDER INQUIRY NO. 17/2017-18 DUE ON 14-02-2018**

**Time of issuance of Tender form upto 13-02-2018 at 02:00 P.M**

**Time of Submission of Tender on 14-02-2018 at 11.30 A.M**

**Time of Opening of Tender on 14-02-2018 at 12.00 Noon**

|  |  |  |  |
| --- | --- | --- | --- |
| **S.No** |  | **Qty** | **Price in Figure and Word** |
| **01** | **SPECIFICATIONS OF WALKTHROUGH GATE (COLUMN TYPE)**   * **SENSITIVITY**   Digitally adjustable sensitivity with a wide range of values**.**   * **DETECTION:-**   Detection of magnetic, non-magnetic and mixed alloy metal weapons**.**   * **DETECTION SPEED: -**   High detection speed up to 15meters per seconds.   * **IMMUNITY :-**   Very High Immunity to both electrical and mechanical interference**.**   * **PROGARMMABLE:-**   Programmable operation controlled by microprocessor**.**   * **HIGH-INTEGRATION: -**   High-integration Professional electronics and maximum reliability.   * **CONTROL UNIT:-**   Control unit incorporated into detector**.**   * **CALIBRATION : -**   No need for initial or periodic calibration.  **Visible signals:**   * **DISPLAY: -**   High intensity display**.**   * **GREEN AND RED SIGNAL: -**   Green and red metering signal, proportional to the mass if the object detected.  **Audible Signals:**   * **ALARM :-**   High acoustic intensity alarm signal.   * **CONFORM:-**   Conforms to the FAA “3-GUN-Test” standard and to the NILECJ-0601-00 standards for all International Security Standards.   * **POWER SUPPLY:-**   Power Supply 115/230VAC, ±15%,45-65Hz,30VA MAX   * **OPERATIVE TEMPERATURE AND RELATIVE HUMIDITY:-**   Temperature and Relative Humidity form -15°c to +70°c; from 0 to 95% (without condensations)  ***Note: Manufacturer Authorization Certificate for this project is must*** | **03** |  |

**NATIONAL TAX No:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ SIGNATURE …………………………………..**

**GST No: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ NAME OF CONTRACTOR ……….…………**

**C.N.I.C No: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ADDRESS …...…………………….…….……**

**(Photostat copies must be enclosed) Contact NO ………..…………….……………**

**I N S T R U C T I O N S**

1. **The tender should be accompanied with pay order / demand draft of 2.5% as security Deposit in the name of Sindh Institute of Ophthalmology & Visual Sciences (SIOVS) Hyderabad.**
2. **Registered with P.E.C Islamabad**
3. **The Income Tax / GST/SST will be deducted according to rules of Govt: of Sindh / Pakistan.**
4. **The tenderer will be responsible to deliver the tendered items on his own cost at SIOVS HYDERABAD.**
5. **In case of short/late supply it will be purchased from open Market and difference if any will be recovered from the Contractor.**
6. **Conditional/ Incomplete Tenders will not be accepted.**
7. **Sample of all dry items should be provided at the time of opening of tender otherwise tender will be rejected.**
8. **For alternate offer separate tender purchase receipt must be enclosed**
9. **The tenderer should be fulfilling all requirements as per Government rules**
10. **Minimum Two Hundred Thousands turn over with Bank Certificate**
11. **Minimum Three Years Experience in relevant field with documentary proof**
12. **Three Years Income Tax Return (Photo Copy Must Enclosed)**
13. **The Performance Security is 10% for One Year w.e.f the date of contract agreement.**
14. **In case of Import , the copy of LC should be provided.**

**Purchase & Store Officer,**

Sindh Institute of Ophthalmology

& Visual Sciences, Hyderabad